{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["定稿"],"read":"whole","date_system":"1900"}

{"sheet":"定稿","index":0,"n_rows":12,"n_cols":8,"rows_kept":12,"merged":[[0,0,0,7],[1,0,1,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[13,2,13,7]]}
["工程量清单"]
["工程名称：霍邱县主城区中央景观带（EPC）市政道路橡胶沥青及沥青路铣刨、铺设专业分包工程"]
["序号","项目名称","施工内容及计算规则","单位","数量","综合单价(元)","合价（元）","备注"]
[1,"车行道\n1cm厚橡胶沥青应力吸收层\n1、集料：预裹附（0.3%-0.5%的沥青）玄武岩石子（粒径0.9-1.5cm，石质坚硬、清洁、不含风化颗粒、近立方体、反击式破碎机轧制的玄武岩碎石）\n2、橡胶沥青：70号普通沥青（橡胶粉含量18%-20%）\n4、施工机械：同步碎石封层车","1、基层清扫、吹尘、清洗、去除浮浆，橡胶沥青路面喷撒，轮胎式压路机碾压。\n2、工程计量按依据施工图纸施工的实际沥青面层完成面的净面积计算。","m2",30000]
[2,"自粘式抗裂贴","1、基层裂缝处粘贴自粘式抗裂贴。\n2、工程计量按实际粘贴面积计算。","m2",18000]
[3,"上面层-3.5cm厚细粒式改性沥青混凝土AC-13C（SBS改性剂4.5％～6.5％） ",null,"m2",9600]
[4,"粘层-：快裂型乳化沥青粘层PCR（喷洒型改性乳化沥青） ",null,"m2",9600]
[5,"路面铣刨机铣刨沥青路面",null,"m2",9600]
[null,null,"合计：",{"$nulls":3},{"$f":"SUM(G4)","v":{"v":0,"d":"0.00"}}]
[]
[null,"1、全费用单价其组成包括人工费、材料费（包括主材、辅材，甲供材除外）、机械使用费、管理费、利润、风险、规费、税金。以及施工降排水、夜间照明、防尘、施工便道等措施费用。施工人员的食宿费、办公费、生活生产水电费、保险费也包含在全费用单价里，由投标人自行考虑计入全费用单价；"]
[null,"2、结算量以招标人现场负责人、成本专员、施工员联签的现场计量工程量计算，最终结算以公司审计监察部审计后金额为准。"]