{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":70,"n_cols":8,"rows_kept":70,"merged":[[0,0,0,7],[1,0,1,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[65,2,65,4],[67,2,67,4],[69,2,69,4]]}
["工程量报价清单"]
["工程名称：贵州省都匀市第四届中国绿化博览会博览园建设项目南广场园建劳务分包工程"]
["序号","项目名称","工程内容","单位","数量","全费用单价","合价","备注"]
[null,"石材铺装"]
[1,"600*200*150芝麻黑光面道牙","剔槽、放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、扫缝、清理净面.","m",366,null,null,"花岗岩、水泥、黄沙、碎石甲供"]
[2,"水沟盖板600*600*80芝麻黑烧面","放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、扫缝、清理净面.","m",935,null,null,"花岗岩、水泥、黄沙、碎石甲供"]
[3,"600*300*50芝麻黑烧面道牙","剔槽、放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、扫缝、清理净面.","m",1500,null,null,"花岗岩、水泥、黄沙、碎石甲供"]
[4,"600*200*150芝麻灰光面道牙","剔槽、放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、扫缝、清理净面.","m",400,null,null,"花岗岩、水泥、黄沙、碎石甲供"]
[5,"600*250*150芝麻灰光面道牙","剔槽、放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、扫缝、清理净面.","m",1650,null,null,"花岗岩、水泥、黄沙、碎石甲供"]
[6,"花岗岩(厚5cm)铺装","放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、扫缝、清理净面.","m2",400,null,null,"花岗岩、水泥、黄沙、碎石甲供"]
[7,"花岗岩(厚6cm)铺装","放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、扫缝、清理净面.","m2",200,null,null,"花岗岩、水泥、黄沙、碎石甲供"]
[8,"花岗岩(厚3cm)铺装","放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、扫缝、清理净面.","m2",958,null,null,"花岗岩、水泥、黄沙、碎石甲供"]
[9,"种植池压顶600*600*50芝麻白","放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、扫缝、清理净面.","m2",200,null,null,"花岗岩、水泥、黄沙、碎石甲供"]
[10,"种植池压顶600*200*100芝麻白","放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、扫缝、清理净面.","m2",120,null,null,"花岗岩、水泥、黄沙、碎石甲供"]
[11,"种植池压顶600*400*30芝麻白","放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、扫缝、清理净面.","m2",150,null,null,"花岗岩、水泥、黄沙、碎石甲供"]
[12,"立面铺贴400*300*30芝麻白","放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、扫缝、清理净面.","m2",140,null,null,"花岗岩、水泥、黄沙、碎石甲供"]
[13,"卵石散铺","清理基层,材料倒运,卵石散铺面层","m3",300,null,null,"材料甲供"]
[14,"花岗岩台阶(厚4-5cm)铺贴","清理基层,砂浆拌合运输,面层材料倒运铺贴","m2",100,null,null,"花岗岩、水泥、黄沙、碎石甲供"]
[15,"花岗岩台阶(厚6-8cm)铺贴","清理基层,砂浆拌合运输,面层材料倒运铺贴","m2",100,null,null,"花岗岩、水泥、黄沙、碎石甲供"]
[16,"花岗岩台阶(厚9-10cm)铺贴","清理基层,砂浆拌合运输,面层材料倒运铺贴","m2",100,null,null,"花岗岩、水泥、黄沙、碎石甲供"]
[null,"土石方"]
[1,"人工挖沟槽（石渣）","1.挖石渣,将石渣堆放在沟、槽周边,清理沟槽及周边.\n2.清理边坡,工作面内人工排水等辅助性工作。","m3",200]
[2,"机械挖沟槽（石渣）","1.挖石渣,将石渣堆放在沟、槽周边,清理沟槽及周边.\n2.清理边坡,工作面内人工排水等辅助性工作。","m3",200]
[3,"人工挖沟槽土方","人工挖沟槽土方、修整沟槽底、边坡等。","m3",120]
[4,"回填土石方","1、包含沟槽、基坑装土、推土、卸土压实，密实度达到设计要求，通过检测，按压实方计量。\n 2.运距：500m内","m3",350]
[5,"机械挖沟槽土方","挖沟槽土方、修整沟槽底、边坡等。","m3",200]
[6,"余土、石方弃置","机械石渣500米内弃置：包含挖土、石渣装车、运输、卸土,清理道路。","m3",450]
[7,"基础商品混凝土垫层","1、厚度15cm以内商品混凝土；      \n2、混凝土场内运输、振捣、浇筑等；        \n3、包含混凝土震动器、混凝土振捣收光找平养护。                       ","m3",100,null,null,"混凝土甲供"]
[8,"基础自拌砼混凝土垫层","厚度15cm以内混凝土自行搅拌、浇筑、振捣、找平等。                       ","m3",120,null,null,"水泥、沙、石子甲供"]
[9,"碎石垫层","1、厚度20cm以内碎石垫层摊铺；          2、含原场地清理、平整、找平、洒水、夯实等；                    \n3、碎石场内运输、找平压实等；              \n4、完成面标高误差2cm以内。","m3",220,null,null,"碎石甲供"]
[10,"C20细石混凝土基础","1、清底、浇筑、捣固(夯实)抹平、材料场内运输。\n2、包含原土夯实\n","m3",180,null,null,"混凝土甲供"]
[null,"砖砌墙体、小型砖砌体、小型结构体"]
[1,"拆除砖砌体","构筑物:拆除、旧料清理成堆清运.","m3",120]
[2,"结构、砌体碎石垫层","1、厚度20cm以内碎石垫层摊铺；          2、含原场地清理、平整、找平、洒水、夯实等；                    \n3、碎石场内运输、分层铺设、找平压实等；              \n4、完成面标高误差2cm以内。","m3",200,null,null,"碎石甲供"]
[3,"结构、砌体自拌砼混凝土垫层","厚度15cm以内混凝土自行搅拌、浇筑、振捣、找平等。                       ","m3",130,null,null,"碎石、水泥、黄砂甲供"]
[4,"标准砖砌小型砌体、排水沟、弧形墙","砂浆调制、运输，运砖、砌小型砌体、排水沟、弧形墙等。","m3",250,null,null,"砖、水泥、黄砂甲供"]
[5,"标准砖砌规则砖墙、矮墙、规花池墙","砂浆调制，运砖，砌筑砖墙。","m3",200,null,null,"砖、水泥、黄砂甲供"]
[6,"小型砖砌体、排水沟、弧形墙墙面刮糙","池、坐凳、台阶、基础、明沟等刮糙。","m2",220,null,null,"砖、水泥、黄砂甲供"]
[7,"规则墙墙面刮糙","砖墙、规则矮墙、规则花池等刮糙。","m2",400]
[8,"脚手架","含安装、拆卸、周转。                       ","m2",800]
[9,"抹灰","润湿墙面、调制砂浆、抹灰、材料运输、清理场地.","m2",1200,null,null,"材料甲供"]
[10,"混凝土垫层模板","1、模板、支撑材料费及安装、拆卸、周转；\n2、按接触面积计算。                         ","m2",500]
[11,"伸缩缝","1、按设计图纸要求切割施工伸缩缝","m",200]
[12,"商品混凝土小型结构（基础、梁、柱、板等）","1、混凝土场内运输、振捣、浇筑等；          \n2、包含混凝土震动器、混凝土振捣收光找平养护。","m3",88,null,null,"砖、水泥、黄砂甲供"]
[13,"自拌混凝土小型结构（基础、梁、柱、板等）","混凝土自行搅拌、运输、振捣、浇筑等，包含混凝土震动器、混凝土振捣收光找平养护。","m3",88,null,null,"砖、水泥、黄砂甲供"]
[14,"成品钢筋网片安装（φ10以内）","1、单层钢筋网片","m2",150,null,null,"材料甲供"]
[null,"装饰装修"]
[1,"墙面文化石","基层清理、调运砂浆,水泥砂浆打底糙,粘贴面层等","m2",400,null,null,"材料甲供"]
[2,"外墙真石漆","清理基层,批腻子二遍，外墙真石漆二遍","m2",560,null,null,"材料甲供"]
[3,"内墙面乳胶漆","清理基层,901胶白水泥满批腻子三遍，刷乳胶漆三遍","m2",1500,null,null,"材料甲供"]
[4,"砼面刷界面剂","清理基层,涂刷界面剂","m2",1500,null,null,"材料甲供"]
[5,"花岗岩墙面粘贴","基层清理、调运砂浆,水泥砂浆打底糙,粘贴面层,砂浆闭缝,表面清理等","m2",350,null,null,"材料甲供"]
[6,"防水砂浆防潮层","基层清理,抹防水砂浆,包含人工费、材料费及机械费用","m2",600,null,null,"材料甲供"]
[7,"陶粒层","陶粒铺设、场内材料运输","m3",140,null,null,"材料甲供"]
[8,"地面铺设—实木地板","清理基层,安装木地板等","m2",160,null,null,"材料甲供"]
[9,"石材楼地面","20mm找平，石材铺装、防护","m2",200,null,null,"材料甲供"]
[10,"不锈钢管栏杆","栏杆材料下料、加工、运输、安装等","m",130,null,null,"材料甲供"]
[11,"屋面瓦","调制砂浆、铺瓦,修界瓦边,安脊瓦、檐口梢头坐灰,固定,清扫瓦面.","m2",800,null,null,"材料甲供"]
[12,"墙面木格栅","定位、放线、下料、制作、安装等.","m2",680,null,null,"材料甲供"]
[null,"合计："]
[null,"1、基础标高、控制点参照标高由招标人提供，乙方在垫层施工中负责按甲方交底要求施工并控制各垫层标高，垫层标高控制在2cm以内，经验收标高未达到要求的，由投标人自行组织整改，并承担整改费用。"]
[null,"2、所有甲供材料均未明确场内运输距离的，均按100m以内考虑，除备注甲供材料，其他所有材料由乙方提供"]
[null,"3、全费用单价是指完成一个规定清单项目所需的人工费、材料费、施工机具使用费、企业管理费、利润和完成该规定清单项目所需的措施费、规费和税金以及一定范围内的风险费用。分部分项分包工程项目的全部费用价格，应包括招标文件所确定的招标范围内的全部内容。全费用单价包含但不限于人工费（含人员加班费用）、甲供材下料、验收、保管、材料二次倒运费用、小型机具费用、耗材(切割片)费用、赶工措施费用、技术服务费（测量等）、通讯费、交通费、食宿费、劳保用品费、相关保险费用、企业管理费、利润、措施费、规费、税金及政策性文件规定费用等所有费用。"]
[null,"4、以上报价税金按3%报价，提供3%点税率的增值税专用发票。"]
[]
[null,null,"报 价 人：                                                       "]
[]
[null,null,"法定代表人或委托代理人：                                           "]
[]
[null,null,"日期：        年     月     日"]