{"text_format":"3","workbook":"xlsx","n_sheets":4,"sheets":["参数","SZ-4C","SZ-3D","智能屏参数"],"not_rendered":{"images":4,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"参数","index":0,"n_rows":9,"n_cols":5,"rows_kept":9,"merged":[[0,0,0,4],[5,2,5,3],[6,0,6,4],[7,0,7,4],[8,0,8,4],[9,0,9,4]]}
["灯具图样确认表"]
["序号","规格","图片","单价","数量"]
[1,"单臂9m高SZ-4C（入口大桥）（智能屏：P4屏512mm*1024mm，双面）（含太阳能板、光源） ",null,"灯杆为方管，壁厚4mm",10]
[2,"单臂6m高SZ-4C（含太阳能板、光源） ",null,"灯杆为圆管",285]
[3,"双臂6m高SZ-3D（含太阳能板、光源） ",null,"灯杆为圆管",56]
[]
["报价说明："]
["1.产品价格为到最终用户指定现场价格(含运保费)，应包含从安装验收合格后起24个月的保修期费用、包含13%增值税。"]
["1、单臂：高度6米，上下口径60*140mm,壁厚3mm，出臂1米，直径60，厚2.5，法兰260*260*12mm，灯杆材质为热镀锌钢管 2、 双臂： 高度6米，上下口径60*140mm,壁厚 3mm，出臂1米，直径60，厚2.5,法兰260*260*12mm，灯杆材质为热镀锌钢管。                                                                                                                    3、9m高（含LED显示屏p4）灯杆臂厚4mm，上150*150mm，下200*200mm，法兰400*400mm，出臂1.2m，灯杆材质为热镀锌钢管。每天照明时间 12-15h， 抗阴雨天数 365天 ，使用环境 -40°C-70°C ，灯头材质 全铝合金 ，锂电池寿命5年。"]

{"sheet":"SZ-4C","index":1,"n_rows":64,"n_cols":5,"rows_kept":64,"merged":[[0,0,1,0],[0,1,0,4],[2,0,37,0],[2,1,2,2],[2,3,2,4],[3,1,3,2],[3,3,3,4],[4,1,4,2],[4,3,4,4],[5,1,5,2],[5,3,5,4],[6,1,6,2],[6,3,6,4],[7,1,7,2],[7,3,7,4],[8,1,8,2],[8,3,8,4],[9,1,9,2],[9,3,9,4],[10,1,10,2],[10,3,10,4],[11,1,11,2],[11,3,11,4],[12,1,12,2],[12,3,12,4],[13,1,13,2],[13,3,13,4],[14,1,14,2],[14,3,14,4],[15,1,15,2],[15,3,15,4],[16,1,16,2],[16,3,16,4],[17,1,17,2],[17,3,17,4],[18,1,18,2],[18,3,18,4],[19,1,19,2],[19,3,19,4],[20,1,20,2],[20,3,20,4],[21,1,21,2],[21,3,21,4],[22,1,22,2],[22,3,22,4],[23,1,23,2],[23,3,23,4],[24,1,24,2],[24,3,24,4],[25,1,25,2],[25,3,25,4],[26,1,26,2],[26,3,26,4],[27,1,27,2],[27,3,27,4],[28,1,28,2],[28,3,28,4],[29,1,29,2],[29,3,29,4],[30,1,30,2],[30,3,30,4],[31,1,31,2],[31,3,31,4],[32,1,32,2],[32,3,32,4],[33,1,33,2],[33,3,33,4],[37,2,37,4],[40,0,40,4]]}
["外观尺寸及图例","规格说明"]
[null,"灯具型号","SZ-4C","灯具名称"]
["外观：\n\n\n\n\n\n\n\n\n\n\n\n\n\n效果图：\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n尺寸图\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n","光学性能",null,"根据安装场景调整"]
[null,"光伏板功率",null,"80W"]
[null,"CTC微光发电板(弱光测试）",null,{"v":0.1645,"d":"16.45%"}]
[null,"CTC微光发电板(强光测试）",null,"24-25%"]
[null,"光源参数"]
[null,"品    牌",null,"神州微光（同档次）"]
[null,"LED芯片",null,"台湾晶元（同档次）"]
[null,"灯头类型"]
[null,"色    温",null,"3000K-9000K"]
[null,"光 通 量",null,">10 lm "]
[null,"显色指数",null,"75-85"]
[null,"平均寿命",null,"＞80000小时"]
[null,"防护等级"]
[null,"控制器防护等级",null,"IP65"]
[null,"整灯防护等级",null,"1（绝缘及接地装置）"]
[null,"物理性能"]
[null,"灯体颜色",null,"根据实际情况定制"]
[null,"灯体材质",null,"全铝合金"]
[null,"反射罩材质"]
[null,"整灯寿命",null,"＞15年"]
[null,"防腐蚀处理",null,"防腐蚀静电喷涂"]
[null,"适用环境温度",null,"﹣40℃-70℃"]
[null,"抗阴雨天数",null,"365天"]
[null,"灯杆参数"]
[null,"杆高",null,"6m"]
[null,"支臂数量",null,"单臂"]
[null,"安装位置",null,"道路两侧"]
[null,"供电性能及保质期"]
[null,"供电电压",null,"AC220V"]
[null,"供电频率",null,"50Hz"]
[null,"保质期",null,"两年"]
[null,"产品尺寸",null,"550*990*150mm"]
[null,"控光附件",null,"安装形式","落地安装"]
[null,"灯具品牌",null,"产地","中国"]
[null,"数量（单位：根）",{"$f":"参数!$E$4","v":285},"单价（人民币元）"]
[null,"合计（人民币元）"]
[]
[]
["太阳能板参数"]
["序号","型号","SZ-4C"]
[1,"光伏板功率","130W"]
[2,"光通量(单颗）",">10 lm "]
[3,"LED芯片","台湾晶元（同档次）"]
[4,"CTC微光发电板(弱光测试）",{"v":0.1988,"d":"19.88%"}]
[5,"CTC微光发电板(强光测试）","24-25%"]
[6,"电压","24V"]
[7,"锂电池","40Ah"]
[8,"色温","3000K-9000K"]
[9,"显色指数","75-85"]
[10,"每天照明时间","12-15h"]
[11,"抗阴雨天数","365天"]
[12,"使用环境","﹣40℃-70℃"]
[13,"灯具材质","全铝合金"]
[14,"锂电池寿命","3-5年"]
[15,"光源寿命","＞80000小时"]
[16,"整灯寿命","＞15年"]
[17,"控制器防护等级","IP67"]
[18,"整灯防护等级","IP65"]
[19,"建议安装间距","20-30m"]
[20,"建议安装高度\n及照度","10-12m,30LXS"]
[21,"产品尺寸","600*1300mm\n"]
[23,"重量","23公斤"]

{"sheet":"SZ-3D","index":2,"n_rows":64,"n_cols":5,"rows_kept":64,"merged":[[0,0,1,0],[0,1,0,4],[2,0,37,0],[2,1,2,2],[2,3,2,4],[3,1,3,2],[3,3,3,4],[4,1,4,2],[4,3,4,4],[5,1,5,2],[5,3,5,4],[6,1,6,2],[6,3,6,4],[7,1,7,2],[7,3,7,4],[8,1,8,2],[8,3,8,4],[9,1,9,2],[9,3,9,4],[10,1,10,2],[10,3,10,4],[11,1,11,2],[11,3,11,4],[12,1,12,2],[12,3,12,4],[13,1,13,2],[13,3,13,4],[14,1,14,2],[14,3,14,4],[15,1,15,2],[15,3,15,4],[16,1,16,2],[16,3,16,4],[17,1,17,2],[17,3,17,4],[18,1,18,2],[18,3,18,4],[19,1,19,2],[19,3,19,4],[20,1,20,2],[20,3,20,4],[21,1,21,2],[21,3,21,4],[22,1,22,2],[22,3,22,4],[23,1,23,2],[23,3,23,4],[24,1,24,2],[24,3,24,4],[25,1,25,2],[25,3,25,4],[26,1,26,2],[26,3,26,4],[27,1,27,2],[27,3,27,4],[28,1,28,2],[28,3,28,4],[29,1,29,2],[29,3,29,4],[30,1,30,2],[30,3,30,4],[31,1,31,2],[31,3,31,4],[32,1,32,2],[32,3,32,4],[33,1,33,2],[33,3,33,4],[37,2,37,4],[40,0,40,4]]}
["外观尺寸及图例","规格说明"]
[null,"灯具型号","SZ-3D","灯具名称"]
["外观：\n\n\n\n\n\n\n\n\n\n\n\n\n\n效果图：\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n尺寸图\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n","光学性能",null,"根据安装场景调整"]
[null,"光伏板功率",null,"60W"]
[null,"CTC微光发电板(弱光测试）",null,{"v":0.1645,"d":"16.45%"}]
[null,"CTC微光发电板(强光测试）",null,"24-25%"]
[null,"光源参数"]
[null,"品    牌",null,"神州微光（同档次）"]
[null,"LED芯片",null,"台湾晶元（同档次）"]
[null,"灯头类型"]
[null,"色    温",null,"3000K-9000K"]
[null,"光 通 量",null,">10 lm "]
[null,"显色指数",null,"75-85"]
[null,"平均寿命",null,"＞80000小时"]
[null,"防护等级"]
[null,"控制器防护等级",null,"IP65"]
[null,"整灯防护等级",null,"1（绝缘及接地装置）"]
[null,"物理性能"]
[null,"灯体颜色",null,"根据实际情况定制"]
[null,"灯体材质",null,"全铝合金"]
[null,"反射罩材质"]
[null,"整灯寿命",null,"＞15年"]
[null,"防腐蚀处理",null,"防腐蚀静电喷涂"]
[null,"适用环境温度",null,"﹣40℃-70℃"]
[null,"抗阴雨天数",null,"365天"]
[null,"灯杆参数"]
[null,"杆高",null,"6m"]
[null,"支臂数量",null,"双臂"]
[null,"安装位置",null,"隔离带"]
[null,"供电性能及保质期"]
[null,"供电电压",null,"AC220V"]
[null,"供电频率",null,"50Hz"]
[null,"保质期",null,"两年"]
[null,"产品尺寸",null,"550*990*150mm"]
[null,"控光附件",null,"安装方式","落地安装"]
[null,"灯具品牌",null,"产地","中国"]
[null,"数量（单位：根）",{"$f":"参数!E5","v":56},"单价（人民币元）"]
[null,"合计（人民币元）"]
[]
[]
["太阳能板参数"]
["序号","型号","SZ-3D"]
[1,"光伏板功率","60W"]
[2,"光通量(单颗）",">10 lm "]
[3,"LED芯片","台湾晶元（同档次）"]
[4,"CTC微光发电板(弱光测试）",{"v":0.1988,"d":"19.88%"}]
[5,"CTC微光发电板(强光测试）","24-25%"]
[6,"电压","12V"]
[7,"锂电池","30Ah"]
[8,"色温","3000K-9000K"]
[9,"显色指数","75-85"]
[10,"每天照明时间","12-15h"]
[11,"抗阴雨天数","365天"]
[12,"使用环境","﹣40℃-70℃"]
[13,"灯具材质","全铝合金"]
[14,"锂电池寿命","3-5年"]
[15,"光源寿命","＞80000小时"]
[16,"整灯寿命","＞15年"]
[17,"控制器防护等级","IP67"]
[18,"整灯防护等级","IP65"]
[19,"建议安装间距","20-25m"]
[20,"建议安装高度\n及照度","6m,30LXS"]
[21,"产品尺寸","465*815\n*150mm"]
[23,"重量","15公斤"]

{"sheet":"智能屏参数","index":3,"n_rows":0,"n_cols":0,"rows_kept":0}