{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["一标段","二标段"],"read":"whole","date_system":"1900"}

{"sheet":"一标段","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"merged":[[0,0,0,7],[45,0,45,7],[46,0,46,5],[47,0,47,5],[48,0,48,5],[49,0,49,5]]}
["东平县东平湖（水浒古镇至泰安港老湖码头段）生态防护林建设项目\n园建劳务工程量清单一标段(K0+000至K4+700)"]
["项目名称：","东平县东平湖（水浒古镇至泰安港老湖码头段）生态防护林建设项目-园建劳务工程"]
["序号","项目名称","项目特征","单位","工程数量","全费用综合单价（元）","合计（元）","备注"]
["一","土方工程"]
[1,"挖土方","1.土壤类别：土\n2.机械挖土，路床整形、人工配合（含机械费）\n3.不装车，堆置于工作面以外整平","m3",10164,null,null,"广场园路停车场垫层土方开挖"]
[2,"挖沟槽（坑）土方","1.土壤类别：土\n2.机械挖沟槽，人工配合人工配合（含机械费）\n3.不装车，堆置于工作面以外整平","m3",2000,null,null,"花池、挡墙等小品工程土方开挖"]
[3,"人工配合机械挖生态排水沟","1.土壤类别：土\n2.配合机械挖土，修整沟槽（坑）底、边坡等。（不含机械费用）\n3.不装车，堆置于工作面以外整平","m3",16362,null,null,"生态排水沟土方开挖"]
[4,"人工夯填土方","1.填方来源：场内运输平衡、取土\n2.人工回填沟槽土方\n2.夯实系数：不小于0.93","m3",555,null,null,"花池、挡墙等小品工程土方回填"]
[5,"人工配合机械填土","1.土壤类别：土\n2.配合机械回填，修整边坡等（不含机械费用）\n","m3",2875,null,null,"生态排水沟土方回填"]
["二","基层类"]
[1,"素土夯实","1.土壤类别：土\n2.工作内容：洒水、平整、打夯\n3.夯实系数：不小于0.93","m2",232000,null,null,"含机械费"]
[2,"碎石垫层","1.厚度：100~300；\n2.完成面标高误差2cm以内；\n3.碎石场内运输、摊铺、找平、压实等                   ","m3",8625,null,null,"含机械费，材料甲供"]
[3,"碎石黏土垫层","1.厚度：350mm；\n2.完成面标高误差2cm以内；   \n3.20-30石子：土=8:2                \n4.材料场内运输、摊铺、拌和、找平、压实等；","m3",1365,null,null,"含机械费，材料甲供"]
[4,"砂垫层","1.30厚中粗砂\n2.底层平整、铺设、找平压实、材料场内运运输等","m3",70,null,null,"含机械费，材料甲供"]
[5,"混凝土垫层","1.厚度：100~250mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；非泵送              ","m3",2580,null,null,"材料甲供"]
[6,"混凝土垫层","1.厚度：100~250mm\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；泵送              ","m3",1550,null,null,"材料甲供"]
[7,"混凝土带形基础、独立基础","1.厚度：300mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；非泵送              ","m3",800,null,null,"材料甲供"]
[8,"混凝土带形基础、独立基础","1.厚度：300mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；泵送              ","m3",500,null,null,"材料甲供"]
[9,"垫层、基础模板","1.按接触面积计算。\n2.模板、支撑材料费及安装、拆卸、周转全部费用；","m2",1635,null,null,"包工包料"]
[10,"不锈钢路牙","1.160*5厚不锈钢304挡板，100长Φ8钢筋固定 @ 600\n2.材料场内运输、制作、预埋铁件、安装、基层清理等","m",295,null,null,"材料甲供"]
[11,"青石平道牙","1.600*120*80自然面青石道牙\n2.20厚1:2.5水泥砂浆\n3.清理基层,材料倒运,砂浆拌合运\n输,路牙铺装","m",5600,null,null,"材料甲供"]
["三","结构小品"]
[1,"混凝土垫层（水上木栈道）","1.厚度：100mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；非泵送              ","m3",200,null,null,"材料甲供"]
[2,"混凝土垫层（水上木栈道）","1.厚度：100mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；泵送              ","m3",85,null,null,"材料甲供"]
[3,"垫层模板(木栈道）","1.按接触面积计算。\n2.模板、支撑材料费及安装、拆卸、周转全部费用；","m2",225,null,null,"包工包料"]
[4,"混凝土池底","1.厚度：250mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；非泵送              ","m3",135,null,null,"材料甲供"]
[5,"混凝土池底","1.厚度：250mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；泵送              ","m3",60,null,null,"材料甲供"]
[6,"池底模板","1.按接触面积计算。\n2.模板、支撑材料费及安装、拆卸、周转全部费用；","m2",150,null,null,"包工包料"]
[7,"混凝土墙（池壁）","1.厚度：250mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；非泵送              ","m3",85,null,null,"材料甲供"]
[8,"混凝土墙（池壁）","1.厚度：250mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；泵送              ","m3",37,null,null,"材料甲供"]
[9,"池壁、墙模板","1.按接触面积计算。\n2.模板、支撑材料费及安装、拆卸、周转全部费用；","m2",970,null,null,"包工包料"]
[10,"混凝土台阶","1.厚度：120mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；非泵送              ","m3",25,null,null,"材料甲供"]
[11,"台阶模板","1.按接触面积计算。\n2.模板、支撑材料费及安装、拆卸、周转全部费用；","m2",45,null,null,"包工包料"]
[12,"混凝土压顶","1.厚度：100mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；非泵送              ","m3",3,null,null,"材料甲供"]
[13,"压顶模板","1.按接触面积计算。\n2.模板、支撑材料费及安装、拆卸、周转全部费用；","m2",1,null,null,"包工包料"]
[14,"钢筋制安","1.种类规格：依据图纸要求，钢筋Φ8~Φ12\n2.场内运输、调直、折弯、制作、安装等，包含钢筋调直机、切断机等机械费用。","t",55,null,null,"材料甲供"]
[15,"钢板安装","1.5厚钢板与钢梁焊接上设抗剪器与砼板固定\n2.场内运输、制作、安装、焊接等，包含钢筋调直机、切断机等机械费用。","m2",3450,null,null,"材料甲供"]
[16,"墙面抹水泥砂浆保护层","1.20厚1:2.5水泥砂浆保护层\n2.清理基层、材料运输、抹保护层、养护等","m2",3945,null,null,"材料甲供"]
[17,"花池、挡墙砖砌体","1.墙\n2.基层清理、砂浆调制、运输，运砖、砌砖砌体。\n3.Mu7.5标准砖砌筑\n4.M5水泥砂浆","m3",30,null,null,"材料甲供"]
[18,"花池、挡墙砖基础","1.基础\n2.基层清理、砂浆调制、运输，运砖、砌砖砌体。\n3.Mu7.5标准砖砌筑\n4.M5水泥砂浆\n5.地面完成面以下为基础","m3",30,null,null,"材料甲供"]
[19,"毛石墙砌筑","1.墙\n2.基层清理、砂浆调制、运输，砌筑、勾缝。\n3.浆砌毛石\n4.M5水泥砂浆","m3",350,null,null,"材料甲供"]
["四","其他"]
[1,"技工",null,"工日",150]
[2,"小工",null,"工日",200]
["五","合计"]
["1.全费用综合单价：包含但不限于人工费（含人员加班费用）、甲供材下料、清点、卸车、验收、保管、施工、养护、清理施工后现场、垃圾清运、材料二次倒运费用（平均按500m以内考虑）、机械费及小型机具费用、赶工措施费用、技术服务费（测量放线等）、通讯费、交通费、食宿费、劳保用品费、相关保险费用、企业管理费、利润、措施费、规费、税金及政策性文件规定费用等所有费用。"]
["2、以上工程量均为暂定量，结算以现场实际发生工程量为准。"]
["3、材料损耗按山东省园林定额2016损耗考核，超过定额损耗的，由乙方承当损失。"]
["4、以上报价按9%的增值税税金报价，签订合同时按实际税点调整合同单价。"]

{"sheet":"二标段","index":1,"n_rows":49,"n_cols":8,"rows_kept":49,"merged":[[0,0,0,7],[45,0,45,7],[46,0,46,5],[47,0,47,5],[48,0,48,5],[49,0,49,5]]}
["东平县东平湖（水浒古镇至泰安港老湖码头段）生态防护林建设项目\n园建劳务工程量清单二标段(K4+700至K9+000)"]
["项目名称：","东平县东平湖（水浒古镇至泰安港老湖码头段）生态防护林建设项目-园建劳务工程"]
["序号","项目名称","项目特征","单位","工程数量","全费用综合单价（元）","合计（元）","备注"]
["一","土方工程"]
[1,"挖土方","1.土壤类别：土\n2.机械挖土，路床整形、人工配合（含机械费）\n3.不装车，堆置于工作面以外整平","m3",6800,null,null,"广场园路停车场垫层土方开挖"]
[2,"挖沟槽（坑）土方","1.土壤类别：土\n2.机械挖沟槽，人工配合人工配合（含机械费）\n3.不装车，堆置于工作面以外整平","m3",1880,null,null,"花池、挡墙等小品工程土方开挖"]
[3,"人工配合机械挖生态排水沟","1.土壤类别：土\n2.配合机械挖土，修整沟槽（坑）底、边坡等。（不含机械费用）\n3.不装车，堆置于工作面以外整平","m3",10900,null,null,"生态排水沟土方开挖"]
[4,"人工夯填土方","1.填方来源：场内运输平衡、取土\n2.人工回填沟槽土方\n2.夯实系数：不小于0.93","m3",370,null,null,"花池、挡墙等小品工程土方回填"]
[5,"人工配合机械填土","1.土壤类别：土\n2.配合机械回填，修整边坡等（不含机械费用）\n","m3",1910,null,null,"生态排水沟土方回填"]
["二","基层类"]
[1,"素土夯实","1.土壤类别：土\n2.工作内容：洒水、平整、打夯\n3.夯实系数：不小于0.93","m2",154600,null,null,"含机械费"]
[2,"碎石垫层","1.厚度：100~300；\n2.完成面标高误差2cm以内；\n3.碎石场内运输、摊铺、找平、压实等                   ","m3",5800,null,null,"含机械费，材料甲供"]
[3,"碎石黏土垫层","1.厚度：350mm；\n2.完成面标高误差2cm以内；   \n3.20-30石子：土=8:2                \n4.材料场内运输、摊铺、拌和、找平、压实等；","m3",900,null,null,"含机械费，材料甲供"]
[4,"砂垫层","1.30厚中粗砂\n2.底层平整、铺设、找平压实、材料场内运运输等","m3",50,null,null,"含机械费，材料甲供"]
[5,"混凝土垫层","1.厚度：100~250mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；非泵送              ","m3",1900,null,null,"材料甲供"]
[6,"混凝土垫层","1.厚度：100~250mm\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；泵送              ","m3",650,null,null,"材料甲供"]
[7,"混凝土带形基础、独立基础","1.厚度：300mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；非泵送              ","m3",850,null,null,"材料甲供"]
[8,"混凝土带形基础、独立基础","1.厚度：300mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；泵送              ","m3",360,null,null,"材料甲供"]
[9,"垫层、基础模板","1.按接触面积计算。\n2.模板、支撑材料费及安装、拆卸、周转全部费用；","m2",1090,null,null,"包工包料"]
[10,"不锈钢路牙","1.160*5厚不锈钢304挡板，100长Φ8钢筋固定 @ 600\n2.材料场内运输、制作、预埋铁件、安装、基层清理等","m",195,null,null,"材料甲供"]
[11,"青石平道牙","1.600*120*80自然面青石道牙\n2.20厚1:2.5水泥砂浆\n3.清理基层,材料倒运,砂浆拌合运\n输,路牙铺装","m",3750,null,null,"材料甲供"]
["三","结构小品"]
[1,"混凝土垫层（水上木栈道）","1.厚度：100mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；非泵送              ","m3",150,null,null,"材料甲供"]
[2,"混凝土垫层（水上木栈道）","1.厚度：100mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；泵送              ","m3",65,null,null,"材料甲供"]
[3,"垫层模板(木栈道）","1.按接触面积计算。\n2.模板、支撑材料费及安装、拆卸、周转全部费用；","m2",150,null,null,"包工包料"]
[4,"混凝土池底","1.厚度：250mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；非泵送              ","m3",150,null,null,"材料甲供"]
[5,"混凝土池底","1.厚度：250mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；泵送              ","m3",80,null,null,"材料甲供"]
[6,"池底模板","1.按接触面积计算。\n2.模板、支撑材料费及安装、拆卸、周转全部费用；","m2",100,null,null,"包工包料"]
[7,"混凝土墙（池壁）","1.厚度：250mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；非泵送              ","m3",120,null,null,"材料甲供"]
[8,"混凝土墙（池壁）","1.厚度：250mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；泵送              ","m3",80,null,null,"材料甲供"]
[9,"池壁、墙模板","1.按接触面积计算。\n2.模板、支撑材料费及安装、拆卸、周转全部费用；","m2",650,null,null,"包工包料"]
[10,"混凝土台阶","1.厚度：120mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；非泵送              ","m3",16,null,null,"材料甲供"]
[11,"台阶模板","1.按接触面积计算。\n2.模板、支撑材料费及安装、拆卸、周转全部费用；","m2",30,null,null,"包工包料"]
[12,"混凝土压顶","1.厚度：100mm；\n2.完成面标高误差1cm以内；     \n3.混凝土场内运输、底层平整、浇筑、振捣、找平、养护等；非泵送              ","m3",2,null,null,"材料甲供"]
[13,"压顶模板","1.按接触面积计算。\n2.模板、支撑材料费及安装、拆卸、周转全部费用；","m2",1,null,null,"包工包料"]
[14,"钢筋制安","1.种类规格：依据图纸要求，钢筋Φ8~Φ12\n2.场内运输、调直、折弯、制作、安装等，包含钢筋调直机、切断机等机械费用。","t",36,null,null,"材料甲供"]
[15,"钢板安装","1.5厚钢板与钢梁焊接上设抗剪器与砼板固定\n2.场内运输、制作、安装、焊接等，包含钢筋调直机、切断机等机械费用。","m2",2250,null,null,"材料甲供"]
[16,"墙面抹水泥砂浆保护层","1.20厚1:2.5水泥砂浆保护层\n2.清理基层、材料运输、抹保护层、养护等","m2",2625,null,null,"材料甲供"]
[17,"砖墙","1.墙\n2.基层清理、砂浆调制、运输，运砖、砌砖砌体。\n3.Mu7.5标准砖砌筑\n4.M5水泥砂浆","m3",10,null,null,"材料甲供"]
[18,"砖基础","1.基础\n2.基层清理、砂浆调制、运输，运砖、砌砖砌体。\n3.Mu7.5标准砖砌筑\n4.M5水泥砂浆\n5.地面完成面以下为基础","m3",15,null,null,"材料甲供"]
[19,"毛石墙砌筑","1.墙\n2.基层清理、砂浆调制、运输，砌筑、勾缝。\n3.浆砌毛石\n4.M5水泥砂浆","m3",280,null,null,"材料甲供"]
["四","其他"]
[1,"技工",null,"工日",120]
[2,"小工",null,"工日",150]
["五","合计"]
["1.全费用综合单价：包含但不限于人工费（含人员加班费用）、甲供材下料、清点、卸车、验收、保管、施工、养护、清理施工后现场、垃圾清运、材料二次倒运费用（平均按500m以内考虑）、机械费及小型机具费用、赶工措施费用、技术服务费（测量放线等）、通讯费、交通费、食宿费、劳保用品费、相关保险费用、企业管理费、利润、措施费、规费、税金及政策性文件规定费用等所有费用。"]
["2、以上工程量均为暂定量，结算以现场实际发生工程量为准。"]
["3、材料损耗按山东省园林定额2016损耗考核，超过定额损耗的，由乙方承当损失。"]
["4、以上报价按9%的增值税税金报价，签订合同时按实际税点调整合同单价。"]