{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":12,"rows_kept":6,"merged":[[0,0,0,8],[1,9,4,9],[5,0,5,8]]}
["工程量清单"]
["序号","项目名称","项目特征","工作内容","单位","工程数量","全费用综合单价（元）","合计（元）","备注",null,"对上单价（元）","合计（元）"]
[1,"低剂量水泥稳定碎石","1.水泥含量：3.5%\n2.石料规格：最大粒径31.5mm\n3.厚度：16cm                 4.压实度不低于97%\n5.按符合图纸要求的合格施工内容，以现场实际完成面积计量","按施工图纸控制道路定位及标高、上料、运料、拌和、整形、摊铺、找平、碾压、养护、清理等","m2",{"v":17743,"d":"17743.00"},null,null,"包工包料",null,105.66,{"$f":"F3*K3","v":1874725.38}]
[2,"水泥稳定碎石","1.水泥含量：4.5%\n2.石料规格：最大粒径31.5mm\n3.厚度：16cm                 4.压实度不低于98%\n5.按符合图纸要求的合格施工内容，以现场实际完成面积计量","按施工图纸控制道路定位及标高、上料、运料、拌和、整形、摊铺、找平、碾压、养护、清理等","m2",{"v":41873,"d":"41873.00"},null,null,"包工包料",null,110.23,{"$f":"F4*K4","v":4615660.79}]
[null,"合计",{"$nulls":5},{"$f":"SUM(H3:H4)","v":{"v":0,"d":"0.00"}},{"$nulls":3},{"$f":"SUM(L3:L4)","v":6490386.17}]
["1、全费用综合单价包含完成分部分项工程项目的全部费用价格（税金按9%考虑），其组成包括但不限于人工费（包括人员加班工资、差旅及窝工费等）、材料费、材料运输、卸车及二次搬运费、二次或者多次进出场费、养护费、已完工项目成品保护措施费、机械使用费及进出场安拆费、耗材费、试验及工程检测费用、管理费、利润、风险、规费、税金以及夜间照明、防尘、施工便道、安全文明（现场安全人员管理）、施工排水、赶工等措施费用。交叉施工影响及配合费用，施工人员的食宿费、劳保费用、办公费、生活生产水电费、保险费也包含在报价里。\n2、结算量以招标人现场负责人、成本专员、施工员联签的现场计量工程量计算，最终结算以公司内审部审计后金额为准。\n3、清单计量规格实行《2013年工程量清单计量规范》\n4.验收规范：满足设计及相关现行规范要求，清单未尽事宜详见图纸以及规范要求。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}