{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["工程量清单"],"read":"whole","date_system":"1900"}

{"sheet":"工程量清单","index":0,"n_rows":65,"n_cols":9,"rows_kept":65,"merged":[[0,0,0,8],[1,0,1,8],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[56,1,56,8],[57,1,57,8],[58,1,58,8],[59,1,59,7],[60,2,60,4],[62,2,62,4],[64,2,64,4]]}
["工程量清单"]
["工程名称：贵州省都匀市第四届中国绿化博览会博览园建设项目园区零星园建劳务分包工程"]
["序号","项目名称","项目特征","工程内容","单位","数量","全费用综合单价（元）","合计（元）","备注"]
[]
["（一）","土石方工程"]
[1,"人工平整场地","30CM内人工挖填、平整、夯实等。","30CM内人工挖填、平整、夯实等。","m2",{"v":500,"d":"500.00"}]
[2,"人工挖基槽、基坑","1.土壤类别：三类土\n2.挖土深度：100cm以内\n3.弃土运距:就近堆置于工作面以外                         4.须按照施工图设计要求标高进行","人工开挖填、修整沟槽底、边坡夯实等。","m3",{"v":620,"d":"620.00"}]
[3,"人工回填土方","1.密实度要求:不小于93%\n2.填方材料品种、填方来源:满足图纸要求，场内取土；\n3.运距:100m内                      4.须按照施工图设计要求标高进行","回填、找平、夯实等","m3",{"v":400,"d":"400.00"}]
[4,"机械回填土方","1.密实度要求:满足设计要求\n2.填方材料品种、填方来源:满足图纸要求，场内取土；\n3.运距:100m内                      \n4.须按照施工图设计要求标高进行","回填、找平、夯实等","m3",{"v":520,"d":"520.00"}]
[5,"机械挖基坑、沟槽土方（不装车）","1、土壤类别：三类土\n2、挖土深度：1m以内\n3、弃土运距:就近堆置于工作面以外                          4、须按照施工图设计要求标高进行","挖沟槽土方，修整沟槽底、边坡等","m3",{"v":500,"d":"500.00"}]
["（二）","园路、广场"]
[1,"碎石垫层（20cm内）","1、20cm厚以内碎石垫层\n2、包含素土压实\n3、完成面标高误差2cm以内","底层平整、压实,分层铺设,找平压实,运 输等","m2",{"v":2900,"d":"2900.00"},null,null,"碎石甲供"]
[2,"水泥稳定碎石层","1.水泥含量:5%\n2.厚度:360厚              3、完成面标高误差1cm以内","放线、上料、运料、拌和、整形、摊铺、找平、碾压、二层铺筑时下层扎毛、养护.","m2",{"v":1600,"d":"1600.00"},null,null,"水稳碎石甲供"]
[3,"非泵送商品混凝土垫层（10cm内）","1、10cm厚商品混凝土垫层                         \n2、完成面标高误差2cm以内。     \n3、标高误差经验收未达到要求的，自行整改，不补偿费用。             \n4、其他厚度按15cm厚度折算本项单价。","混凝土场内运输、浇筑、振捣、找平、切缝、养护等。","m2",{"v":3100,"d":"3100.00"},null,null,"砼甲供"]
[4,"垫层模板","1、包含模板、支撑材料费及安装、拆卸、周转","制作人工费、模板、支撑等主辅 材及机械费用","m2",{"v":600,"d":"600.00"},null,null,"包工包料"]
[5,"石材碎拼（山坡）","1、3-5cm青石板碎拼\n2、30mm厚水泥砂浆\n3、包含山坡二次转运","清理基层，砂浆拌合运输，面层材料倒运铺装","m2",{"v":1150,"d":"1150.00"},null,null,"石材、水泥、砂甲供"]
[6,"石材碎拼（平地）","1、3-5cm青石板碎拼\n2、30mm厚水泥砂浆","清理基层，砂浆拌合运输，面层材料倒运铺装","m2",{"v":1500,"d":"1500.00"},null,null,"石材、水泥、砂甲供"]
[7,"道路平缘石","600*300*50厚预制C30混泥土平缘石\n30厚1:3干硬性水泥砂浆","放样、整修路槽、运料、调浆、安砌、勾缝、回填、养护、清理.","m",{"v":370,"d":"370.00"},null,null,"石材、水泥、砂甲供"]
[8,"路牙石铺设","600*200*150花岗岩路牙石\n30厚1:3干硬性水泥砂浆","剔槽、放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、扫缝、清理净面.","m",600,null,null,"石材、水泥、砂甲供"]
[9,"花岗岩(厚5cm)铺装","1、花岗岩(厚5cm)铺装\n2、30mm厚水泥砂浆","放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、扫缝、清理净面.","m2",2000,null,null,"石材、水泥、砂甲供"]
[10,"花岗岩(厚3cm)铺装","1、花岗岩(厚3cm)铺装\n2、30mm厚水泥砂浆","放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、扫缝、清理净面.","m2",1500,null,null,"石材、水泥、砂甲供"]
[11,"5cm石材走边（波打线）","1、花岗岩(厚5cm)铺装\n2、30mm厚水泥砂浆","放线、清理基层、调运砂浆、刷素水泥浆、锯板磨边、铺贴块料、作缝、清理净面.","m2",{"v":116,"d":"116.00"},null,null,"石材、水泥、砂甲供"]
[12,"石材汀步","1.石料种类、规格:300*600*50青石板\n","挖基层土方,面层材料倒运铺贴，就近土方回填周边压实、水泥砂浆嵌缝","m2",400,null,null,"石材甲供"]
["（三）","基础结构"]
[1,"结构、砌体碎石垫层","1、厚度20cm以内碎石垫层摊铺          2、含原场地清理、平整、找平、洒水、夯实等。                                  3、碎石80m以内场内运输、分层铺设、找平压实等。                             4、完成面标高误差2cm以内。","底层平整、压实,分层铺设,找平压实,运 输等","m3",{"v":200,"d":"200.00"},null,null,"碎石甲供"]
[2,"结构、砌体商品混凝土垫层","1、厚度15cm以内非泵送商品混凝土                      2、非泵混凝土50m以内场内运输、振捣、浇筑等，                          3、包含混凝土震动器、混凝土振捣收光找平养护，                ","混凝土场内运输、浇筑、振捣、找平、养护等。","m3",{"v":150,"d":"150.00"},null,null,"砼甲供，甲方机械配合"]
[3,"混凝土垫层模板","1、模板、支撑材料费及安装、拆卸、周转；\n2、按接触面积计算。","制作人工费、模板、支撑等主辅 材及机械费用","m2",{"v":600,"d":"600.00"},null,null,"包工包料"]
[4,"自拌混凝土小型结构（基础、梁、柱、板等）","1、自拌混凝土强度符合图纸要求\n2、完成面标高误差2cm以内。\n3、标高误差经验收未达到要求的，自行整改，不补偿费用。","混凝土自行搅拌、运输、振捣、浇筑等，包含混凝土震动器、混凝土振捣收光找平养护\n","m3",100,null,null,"水泥、黄砂甲供"]
[5,"结构木模板（基础、梁、柱、墙、板等）","1、包含模板、支撑材料费及安装、拆卸、周转","制作人工费、模板、支撑等主辅 材及机械费用","m2",{"v":800,"d":"800.00"},null,null,"包工包料"]
[6,"弧形模板（屋面板、弧形墙）","1、包含模板、支撑材料费及安装、拆卸、周转","制作人工费、模板、支撑等主辅 材及机械费用","m2",{"v":600,"d":"600.00"},null,null,"包工包料"]
[7,"商品混凝土小型结构（基础、梁、柱、板等）","1、非泵混凝土50m以内场内运输、振捣、浇筑等\n2、标高误差经验收未达到要求的，自行整改，不补偿费用。                                 ","混凝土场内运输、浇筑、振捣、找平、切缝、养护等。","m3",{"v":115,"d":"115.00"},null,null,"砼甲供"]
[8,"砖砌填充墙","1.砖品种、规格、强度等级:烧结页岩多孔砖、水泥标砖\n2.墙体类型:砖砌墙\n3.砂浆强度等级、配合比:M7.5水泥砂浆灌孔砌筑","调、运、铺砂浆,运、砌砖,安放木砖、垫块、铁件、填料、原浆勾缝.","m3",{"v":80,"d":"80.00"},null,null,"砖、水泥、黄沙甲供"]
[9,"青砖镂空砌筑填充墙","1.砖品种、规格、强度等级:Mu10青砖镂空砌筑\n2.墙体类型:填充墙\n3.砂浆强度等级、配合比:M7.5水泥砂浆灌孔砌筑","调、运、铺砂浆,运、砌砖,安放木砖、垫块、铁件、填料、原浆勾缝.","m3",{"v":50,"d":"50.00"},null,null,"青砖、水泥、黄沙甲供"]
[10,"加气砖砌填充墙","1、加气混凝块600*200*200\n2、满足设计图纸要求","砂浆调制、运输，运砌块、砌加气混凝土砌块砌体。","m3",{"v":100,"d":"100.00"},null,null,"加气混凝土砖、水泥、黄沙甲供"]
[11,"预埋件","200*200*6钢板，440*440*20预埋钢板，M20螺栓固定","铁件埋设、焊接固定.","t",{"v":3.5,"d":"3.50"},null,null,"预埋件、螺栓甲供"]
[12,"脚手架","含外脚手架和满堂脚手架，钢管、扣件的租赁、搭设、拆除、转场等","含外脚手架和满堂脚手架，钢管、扣件的租赁、搭设、拆除、转场等","m2",{"v":1200,"d":"1200.00"},null,null,"包工包料"]
[13,"内墙面乳胶漆","清理基层,刮大白、901胶白水泥满批腻子两遍，刷乳胶漆两遍","清理基层,刮大白、901胶白水泥满批腻子两遍，刷乳胶漆两遍","m2",{"v":1100,"d":"1100.00"},null,null,"材料甲供"]
[14,"墙面水泥砂浆刮糙","按设计图纸要求墙面基层抹灰找平、刮糟","基层清理，调运砂浆，墙面水泥砂浆找平刮糙","m2",{"v":1100,"d":"1100.00"},null,null,"材料甲供"]
[15,"墙体粉刷","1.按设计图纸要求墙面粉刷抹灰","1.清理、修补、湿润基层表面、堵墙眼、调运砂浆、清扫落地灰.\u20292.分层抹灰找平、刷浆、洒水湿润、罩面压光(包括门窗洞口侧壁及护角抹灰).","m2",1100,null,null,"材料甲供"]
[16,"钢筋制安","1、钢筋制作\n2、按图纸及规范要求施工","钢筋的1km以内场内运输、调直、折弯、制作、安装等，包含钢筋调直机、切断机等机械费用","t",{"v":90,"d":"90.00"},null,null,"钢筋甲供"]
["（四）","砌体结构"]
[1,"标准砖砌小型砌体、排水沟、弧形墙\n","1、水泥标砖、烧结砖砌筑\n2、满足设计图纸要求","砂浆调制、运输，运砖、砌小型砌体、排水沟、弧形墙等","m3",160,null,null,"材料甲供"]
[2,"砌筑毛石挡墙，皮面做缝","1.石料种类、规格:毛石\n2.石表面加工要求:按图纸设计要求\n3.勾缝要求:按图纸设计要求，单面清水勾缝\n4.砂浆强度等级、配合比:M5水泥砂浆               ","砂浆调制、运输，毛石50m以内场内二次倒运，砌毛石墙身，、排水管安装，面墙做皮带缝等","m3",{"v":165,"d":"165.00"},null,null,"毛石、水泥、黄砂、混凝土甲供"]
[3,"砌筑毛石基础","1.石料种类、规格:毛石\n2.石表面加工要求:按图纸设计要求\n3.砂浆强度等级、配合比:M5水泥砂浆               ","砂浆调制、运输，场内二次倒运，砌毛石基础等","m3",{"v":50,"d":"50.00"},null,null,"毛石、水泥、黄砂甲供"]
["（五）","其他"]
[1,"小型木格栅","1.材质：防腐杉木                 2.规格：按施工设计图要求","定位、放线、下料、制作、安装等.","m2",70,null,null,"材料甲供"]
[2,"小型瓦片","1.规格、品种：黏土平瓦、脊瓦387×218          2.结合层砂浆配合比：自拌水泥砂浆","调制砂浆、安脊瓦、平瓦","m2",1200,null,null,"材料甲供"]
[3,"市政路牙拆除","拆除花岗岩路牙石","拆除、堆放、清理，平整场地","m",80]
[4,"钢套管埋设","\n1.材质及规格:钢管\n2.连接形式:焊接\n3.规格尺寸：De100mm以内     4.铺设深度:根据设计图纸要求\n","调直、切管、坡口、煨弯、挖眼接管、异径管制作, 组对, 焊接","m",600,null,null,"材料甲供"]
[5,"1000*300*50青石板汀步","1.石料种类、规格:1000*300*50青石板\n2.砂浆强度等级、配合比:30mm厚水泥砂浆","清理基层,砂浆拌合运输,面层材料倒运铺贴，黑色瓜子片嵌缝","m2",{"v":80,"d":"80.00"},null,null,"青石板、砂、瓜子片甲供"]
[6,"排水沟盖板","500*500*50预制C20钢筋混泥土盖板","放线、清理基层、运料、调浆、盖板运输和安装","m2",{"v":225,"d":"225.00"},null,null,"盖板、水泥、黄沙甲供"]
[7,"菠萝格木地板","1.截面120*40菠萝格防腐木，留缝5mm制作安装2.50*50木龙骨制作安装3.根据设计图纸要求","\n放样、选料、运料、截料、划线、起线、凿眼、锯榫、汇榫、弹安装线、标写安装号、试装、修整榫卯、入位、栽销、校正,钉牢、齐头、安装.","m2",650,null,null,"菠萝格甲供"]
[8,"卵石镶嵌排水沟","1.石料种类、规格:鹅卵石\n2.砂浆强度等级、配合比:1：2自拌水泥砂浆","放线、清理基层、运料、调浆、铺面层、清扫","m2",400,null,null,"卵石、砂浆甲供"]
[9,"8厚陶瓷马赛克、颗粒规格100*100，整贴300*300（弧形游泳池墙面和地面）","\n1.结合层厚度、砂浆配合比:15厚M15砂浆结合层\n3.面层材料品种、规格、颜色:8厚陶瓷马赛克、颗粒规格100*100，整贴300*300","1.基层清理、修补;砂浆制作、运输、砂浆打底、抹粘结层砂浆,刷粘接剂.\n2.选料、贴瓷块、擦缝、清洁表面.\n","m2",500,null,null,"材料甲供"]
[10,"8厚陶瓷马赛克、颗粒规格25*25，整贴300*300（弧形游泳池墙面和地面）                  ","\n1.结合层厚度、砂浆配合比:15厚M15砂浆结合层\n3.面层材料品种、规格、颜色:8厚陶瓷马赛克、颗粒规格25*25，整贴300*300                     ","1.基层清理、修补;砂浆制作、运输、砂浆打底、抹粘结层砂浆,刷粘接剂.\n2.选料、贴瓷块、擦缝、清洁表面.\n","m2",400,null,null,"材料甲供"]
[null,"合计"]
[null,"1、基础标高、控制点参照标高由招标人提供，乙方在垫层施工中负责按甲方交底要求施工并控制各垫层标高，垫层标高控制在2cm以内，经验收标高未达到要求的，由投标人自行组织整改，并承担整改费用。"]
[null,"2、所有甲供材料均已考虑转运费用，除备注甲供材料，其他所有材料由乙方提供"]
[null,"3、全费用单价是指完成一个规定清单项目所需的人工费、材料费、施工机具使用费、企业管理费、利润和完成该规定清单项目所需的措施费、规费和税金以及一定范围内的风险费用。分部分项分包工程项目的全部费用价格，应包括招标文件所确定的招标范围内的全部内容。全费用单价包含但不限于人工费（含人员加班费用）、甲供材下料、验收、保管、材料二次倒运费用、小型机具费用、耗材(切割片)费用、赶工措施费用、技术服务费（测量等）、通讯费、交通费、食宿费、劳保用品费、相关保险费用、企业管理费、利润、措施费、规费、税金及政策性文件规定费用等所有费用。"]
[null,"4、以上报价税金按9%报价，提供9%点税率的增值税专用发票。"]
[null,null,"报 价 人：                                                       "]
[]
[null,null,"法定代表人或委托代理人：                                           "]
[]
[null,null,"日期：        年     月     日"]