{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":21,"n_cols":9,"rows_kept":21,"merged":[[0,0,0,7],[1,0,1,7],[20,0,20,7]]}
["工程量清单"]
["项目名称：东平县东平湖（水浒古镇至泰安港老湖码头段）生态防护林建设扩建项目木栈道专业分包工程"]
["序号","项目名称","项目特征","工作内容","单位","工程数量","全费用综合单价（元）","合计（元）"]
["一","三米贴水段(园路、平台）"]
[1,"栏杆","1.栏杆高度:1.1m\n2.140*50mm红柳桉防腐木扶手，底部刻槽，面刷清漆两道\n3.5mm厚90*20mmU型不锈钢槽，结构胶固定\n4.70*50mm矩形钢管壁厚5mm上刷蓝灰色氟碳漆与扶手底部钢件焊接\n5.包50mm厚红柳桉防腐木板外刷清漆两道底部留槽70*20mm\n6.直径12mm*2不锈钢管连接件，内接直径6mm镀锌钢索\n7.详见图纸\n8.按栏杆立柱外边线测量、以延长米计量","含材料下料、加工、运输、安装、喷涂、清理、成品维护等","m",{"v":400,"d":"400.000"},null,null," "]
[2,"木栈道","1.50mm厚红柳桉防腐木板\n2.50*50mm樟子松防腐木龙骨@500mm\n3.按木栈道图示尺寸净量计量","含材料下料、加工、运输、安装等","m2",{"v":572,"d":"572.000"},null,null," "]
[3,"木质装饰线","1.100*30mm厚红柳桉防腐木侧封板不锈钢螺钉固定\n2.按图示尺寸净量计量","含材料下料、加工、运输、安装等","m",{"v":155.434782608696,"d":"155.435"}]
[4,"钢板垫层","1.5mm厚钢板与钢梁焊接、上设抗剪器与砼板固定","含安装、固定、材料场内倒运等","m2",{"v":600,"d":"600.000"}]
[5,"钢板上混凝土板","1.100mm厚C30素混凝土板\n2.商品混凝土\n3.按符合图纸要求的合格施工内容，以图示尺寸以净量计量","含模板、浇筑、振捣、收光、找平、养护","m3",{"v":57.2,"d":"57.200"}]
[6,"现浇构件钢筋","1.钢筋种类:圆钢\n2.钢筋规格:φ8\n3.按图示尺寸净量计量","含制作、绑扎、安装、焊接、固定、材料场内倒运等","t",{"v":2.80805105547374,"d":"2.808"}]
[7,"钢梁","1.梁类型:工字钢梁\n2.钢材品种、规格:18#工字钢梁\n3.按图示尺寸净量计量","含制作、除锈、安装、焊接、固定、材料场内倒运等","t",{"v":13.2961413296141,"d":"13.296"}]
[8,"钢管内填芯","1.材质:混凝土\n2.混凝土强度等级:C30\n3.按图示尺寸净量计量","安装、拆除导管、漏斗、砼浇筑、养护等","m3",{"v":35.5,"d":"35.500"}]
[9,"钢管桩","1.材质:无缝钢管\n2.管径、壁厚:φ219mm壁厚4mm\n3.桩长9m\n4.按图示尺寸净量计量","含制作、安装、接桩、对接、焊接、桩头钢筋整理等","t",{"v":26.2746899402848,"d":"26.275"}]
[10,"现浇构件钢筋","1.钢筋种类:圆钢\n2.钢筋规格:φ8\n3.按图示尺寸净量计量","含制作、绑扎、安装、焊接、固定、材料场内倒运等","t",{"v":2.47596606974552,"d":"2.476"}]
[11,"现浇构件钢筋","1.钢筋种类:圆钢\n2.钢筋规格:φ12\n3.按图示尺寸净量计量","含制作、绑扎、安装、焊接、固定、材料场内倒运等","t",{"v":3.01954022988506,"d":"3.020"}]
[12,"预埋件安装","1.预埋件材质:250*250*5mm厚钢板\n2.按图加工","含制作、安装、固定、材料场内倒运等","t",{"v":0.313185503099666,"d":"0.313"}]
[13,"钢梁","1.梁类型:槽钢\n2.钢材品种、规格:20mm#B槽钢\n3.按图示尺寸净量计量","含制作、除锈、安装、焊接、固定、材料场内倒运等","t",{"v":9.74114441416894,"d":"9.741"}]
[14,"油漆","1.底漆：氟碳漆专用防锈底漆\n2.面漆：蓝灰色氟碳漆\n3.按图示尺寸净量计量","含基面处理、喷涂、成品维护","m2",{"v":841.176470588235,"d":"841.176"}]
[null,"合计"]
[]
["1、全费用综合单价包含完成分部分项工程项目的全部费用价格（税金按9%考虑），其组成包括但不限于人工费（包括人员加班工资、差旅及窝工费、承包人供应材料保管费等）、材料费、材料运输、卸车及二次搬运费、二次或者多次进出场费、已完工项目成品保护措施费、机械使用费及进出场安拆费、耗材费、试验及工程检测费用、管理费、利润、风险、规费、税金以及夜间照明、防尘、施工便道、脚手架、支架、安全文明（标识标牌的制作、购买及安装，绿网的覆盖，现场安全人员管理）、施工排水、赶工等措施费用。交叉施工影响及配合费用，施工人员的食宿费、劳保费用、办公费、生活生产水电费、保险费也包含在报价里。\n2、结算量以招标人现场负责人、成本专员、施工员联签的现场计量工程量计算，最终结算以公司内审部审计后金额为准。\n3、以上报价按9%的增值税税金报价，签订合同时按实际税点调整合同单价，最终结算按照实际开票税率进行调整税差。\n4、清单计量规格实行《2013年工程量清单计量规范》\n5、验收规范：满足设计及相关现行规范要求，清单未尽事宜详见图纸以及规范要求。"]