{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["工程量清单"],"read":"whole","date_system":"1900"}

{"sheet":"工程量清单","index":0,"n_rows":30,"n_cols":9,"rows_kept":30,"merged":[[0,0,0,8],[1,0,1,8],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[17,1,17,8],[18,1,18,8],[19,1,19,8],[20,1,20,8],[21,1,21,8],[22,1,22,8],[23,1,23,8],[25,5,25,7],[27,5,27,7],[29,5,29,7]]}
["工程量清单"]
["工程名称：麒麟塘公园及国贸大道两侧景观工程二期EPC工程总承包-大通路与涌金路等绿化种植劳务分包工程"]
["序号","项目名称","项目特征","施工内容","单位","数量","全费用综合\n单价（元）","全费用综合\n合价（元）","备注"]
[]
["一","乔、灌木"]
[1,"乔木","Φ≤6cm或D≤8cm","倒运装卸、散苗、 挖树坑、苗木种植,打支撑和裹草绳，移交前苗木养护等,含人工费及机械费用","株",{"$f":"78","v":78}]
[2,"乔木","6＜Φ≤8cm或8＜D≤10cm","倒运装卸、散苗、 挖树坑、苗木种植,打支撑和裹草绳，移交前苗木养护等,含人工费及机械费用","株",344]
[3,"乔木","8＜Φ≤10cm或10＜D≤12cm","倒运装卸、散苗、 挖树坑、苗木种植,打支撑和裹草绳，移交前苗木养护等,含人工费及机械费用","株",15]
[4,"乔木","14＜Φ≤16cm或16＜D≤18cm","倒运装卸、散苗、 挖树坑、苗木种植,打支撑和裹草绳，移交前苗木养护等,含人工费及机械费用","株",{"$f":"1274+2214+650+355+110","v":4603}]
[5,"乔木","18＜Φ≤20cm或20＜D≤24cm","倒运装卸、散苗、 挖树坑、苗木种植,打支撑和裹草绳，移交前苗木养护等,含人工费及机械费用","株",161]
["二","地被"]
[1,"地被植物","栽植地被植物 密度≤36株/m2","倒运装卸、散苗、 挖树坑、苗木种植,移交前苗木养护等,含人工费及机械费用","m2",{"$f":"5330+1788+9521+140","v":16779}]
[2,"地被植物","栽植地被植物 密度>36株/m2","倒运装卸、散苗、 挖树坑、苗木种植,移交前苗木养护等,含人工费及机械费用","m2",{"$f":"2085+411+27730+1187+2822","v":34235}]
[3,"满铺草坪","草坪满铺","清除杂物、搬运草坪、铺植草皮、浇水、清理、养护","m2",11973]
["三","绿化地细整"]
[1,"绿化地人工细整","放线、30cm以内挖、运、填土、找平等","土层找平、找坡、耙细,清除石子等杂物,刨出地面排水沟,清理现场,渣土集中堆放等","m2",{"$f":"SUM(F12:F14)","v":62987}]
[null,"合计："]
[null,"注：1、苗木、支撑杆、化肥、农药、营养土、草绳、遮阳网等由甲方提供；其余劳务及机械、小辅材由乙方供应；"]
[null,"2、全费用综合单价包括清理垃圾、清点苗木、撒营养土、卸车、二次倒运装卸、散苗、挖树坑、苗木修剪、种植、修边沟、机械（小型机械、二次倒运运输车、吊车等），乔木打支撑、裹草绳、浇水、必要的遮阴、打药费用，通讯费、交通费、食宿费、劳保用品费、相关保险费用、管理费、利润及税金；包含养护期内浇水、打药、施肥、修剪、清理等工作内容；"]
[null,"3、全费用综合单价包含种植费用和截止到2021年6月30日的养护费用。"]
[null,"4、以上报价包含苗木种植成活费用，名贵苗木考核成活率要求100%（苗木单价超2万元品种），乔木考核成活率要求95%（20cm以上乔木成活率97%）,灌木、地被考核成活率93%，水生考核成活率100%，养护结束后点交，超额死亡苗木不计种植及养护费并按种植、养护费用4倍扣罚，且需按要求进行补植（甲供苗木）。"]
[null,"5、以上报价税金按9%报价，提供9%点税率的增值税专用发票。最终合同签订时以中标人实际可提供的开票税率调整修正合同价格。"]
[null,"6、结算工程量以最终结算为准。"]
[null,"7、种植后应考虑植物造景以及植物基本形态重新修剪造型（修剪严禁截头），去掉阴枝、病残枝，并对剪口做处理，苗木修剪保持全枝全冠，做好井字撑，满足设计要求。造型树在之后需要人工再造型，核心区草坪铺植需设找平沙垫层。"]
[]
[{"$nulls":5},"投 标 人："]
[]
[{"$nulls":5},"法定代表人或委托代理人："]
[]
[{"$nulls":5},"日期：        年     月     日"]