{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["工程量清单"],"read":"whole","date_system":"1900"}

{"sheet":"工程量清单","index":0,"n_rows":9,"n_cols":9,"rows_kept":9,"merged":[[0,0,0,8],[1,0,1,8],[6,1,6,8],[7,1,7,8],[8,1,8,8],[10,2,10,8]]}
["工程量清单"]
["工程名称：霍邱县主城区中央景观带设计-采购-施工总承包（EPC）项目-EF区顶管专业分包工程"]
["序号","项目名称","项目特征","工作内容","单位","数量","综合单价(元)","合价（元）","备注"]
[1,"混凝土管道顶进（DN1500mm)","1、管径：D1500\n2、深度：详见设计\n3、管材规格：F型Ⅲ级钢筋砼管\n4、管道接口：参见06MS201-1 P25,管道接口处应设置内置橡胶圈\n5、顶管方式：机械顶管\n6、注浆：在每隔3节管道预留注浆孔，注浆采用42.5水泥，水灰比1：1，掺入1-2%的氯化钙\n7、根据现场情况，土方管道开挖、管道出土，土方外运、消纳，运距自行考虑\n8、按规定要求做闭水试验\n9、未说明处详见图纸及相关规范","根据现场情况，土方管道开挖、排水，机械顶管、管道出土，土方外运、消纳，运距自行考虑，接口处理，按规定要求做闭水试验等","m",{"v":140,"d":"140.00"},null,{"$f":"G4*F4","v":0}]
[2,"方形工作井","1、井内径尺寸：700cm*650*460cm，详见图纸\n2、底板为50cmC30砼，w4抗渗，抗冻F150，模板及附件施工，详见图纸\n3、井壁为50cmC30砼，w4抗渗，抗冻F150，模板及附件施工，详见图纸\n4、井身设置集水坑，详见图纸\n5、底板、井壁钢筋及附件的运输、制作、安装，详见图纸\n6、井深详见设计图纸\n7、顶部设置1.1m高钢管护栏，详见图纸及规范\n8、工作井四周灰土回填，详见图纸及规范\n9、根据现场情况，土方开挖、回填，土方外运、消纳，运距自行考虑\n10、未说明处详见图纸及相关规范","根据现场情况，土方开挖、回填，土方外运、消纳，运距自行考虑，底板、井壁钢筋及附件的运输、制作、安装、顶坑防护网制作、安装等","座",{"v":2,"d":"2.00"},null,{"$f":"G5*F5","v":0}]
[null,null,"合计：",{"$nulls":4},{"$f":"SUM(H4:H5)","v":0}]
[]
[null,"1、综合单价包括人工费（包括人员加班工资、差旅及窝工费）、材料费、材料运输、卸车及二次搬运费、二次或者多次进出场费、已完工项目成品保护措施费、机械使用费及进出场装卸费、耗材费、试验费、管理费、利润、风险、规费、税金以及夜间照明、防尘、施工便道、脚手架、支架、安全文明及防护、施工排水、围挡等措施费用。施工人员的食宿费、劳保费用、办公费、生活生产水电费、保险费也包含在报价里。"]
[null,"2、结算量以招标人现场负责人、成本专员、施工员联签的现场计量工程量计算，最终结算以公司内审部审计后金额为准。"]