{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["工程量清单"],"read":"whole","date_system":"1900"}

{"sheet":"工程量清单","index":0,"n_rows":34,"n_cols":9,"rows_kept":34,"merged":[[0,0,0,8],[1,0,1,6],[29,1,29,2],[30,0,30,8],[31,0,31,6],[32,0,32,6],[33,0,33,6]]}
["工程量清单"]
["项目名称：东平县东平湖（水浒古镇至泰安港老湖码头段）生态防护林建设项目花岗岩面层铺设劳务分包（二次）"]
[9,"项目名称","项目特征","工作内容","单位","数量","全费用单价（元）","合价（元）","备注"]
["一","石材墙面粘贴"]
[1,"石材贴面","1.20mm厚花岗岩贴面\n2.20mm厚1：2.5水泥砂浆结合层","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",84.51,null,null,"材料甲供"]
[2,"迎湖面原有驳岸改造自然片石贴面","1.20mm厚自然面片石贴面\n2.20mm厚1:3干硬性水泥砂浆","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",{"$f":"985.22+3040.8","v":4026.02},null,null,"材料甲供"]
["二","石材地面铺贴"]
[1,"石材铺装","1.50mm厚石材铺装\n2.30mm厚1:3干硬性水泥砂浆结合层","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",{"$f":"8083.29+2498.92","v":10582.21},null,null,"材料甲供"]
[2,"石材铺装","1.80mm厚石材铺装\n2.30mm厚1:3干硬性水泥砂浆结合层","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",240.18,null,null,"材料甲供"]
[3,"毛石铺装","1.块径300-400，60mm厚毛石铺装\n2.30mm厚1:3干硬性水泥砂浆","基层清理、砂浆调制、运输，石材修整、材料场内运输、铺贴、清扫现场、成品保护等","m2",390.49,null,null,"材料甲供"]
[4,"石材拼碎铺装","1.60mm厚石材拼碎\n2.30mm厚1:3干硬性水泥砂浆结合层","基层清理、砂浆调制、运输，石材修整、材料场内运输、铺贴、清扫现场、成品保护等","m2",{"v":137,"d":"137.00"},null,null,"材料甲供"]
[5,"天然片石拼碎","1.60mm厚天然片石碎拼铺装\n2.30mm厚1:3干硬性水泥砂浆","基层清理、砂浆调制、运输，石材修整、材料场内运输、铺贴、清扫现场、成品保护等","m2",{"$f":"3507.06+132","v":3639.06},null,null,"材料甲供"]
[6,"片石铺装","1.150mm厚片石铺装，块径200-600mm\n2.30mm厚1:3干硬性水泥砂浆结合层","基层清理、砂浆调制、运输，石材修整、材料场内运输、铺贴、清扫现场、成品保护等","m2",513.62,null,null,"材料甲供"]
[7,"石材台阶面","1.150mm厚条石台阶\n2.30mm厚1:3干硬性水泥砂浆","基层清理、砂浆调制、运输，材料场内运输、安装、清扫现场、成品保护等","m2",328.61,null,null,"材料甲供"]
[8,"石汀步","1.60mm厚天然料石块铺装\n2.30mm厚1:2.5干硬砂浆粘接层","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",{"v":149,"d":"149.00"},null,null,"材料甲供"]
[9,"井字植草砖铺装","1.250*190*70mm厚井字植草砖铺设\n2.30mm厚中粗砂","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",6652.29,null,null,"材料甲供"]
[10,"透水砖铺装","1.120*240*60mm厚透水砖席纹铺\n2.30mm厚1:3干硬性水泥砂浆","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",{"$f":"1847.35+3123.65","v":{"v":4971,"d":"4971.00"}},null,null,"材料甲供"]
["三","石材收边、压顶"]
[1,"石材收边","1.50mm厚石材收边\n2.20mm厚1:3水泥砂浆","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",{"$f":"34.17+623.92","v":658.09},null,null,"材料甲供"]
[2,"条石收边","1.80mm厚条石收边\n2.20mm厚1:3水泥砂浆","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",{"v":1082.014,"d":"1082.01"},null,null,"材料甲供"]
[3,"条石收边","1.150mm厚条石收边\n2.20mm厚1:3水泥砂浆","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",228.63,null,null,"材料甲供"]
[4,"木缘石压顶","1.50mm厚木缘石压顶，两边倒角，橡胶螺栓固定","基层清理、砂浆调制、运输，材料场内运输、铺贴、清扫现场、成品保护等","m2",14.46,null,null,"材料甲供"]
[5,"扶手、压顶","1.400*300*80mm厚石材压顶，两侧磨30圆角\n2.20mm厚1：2.5水泥砂浆结合层","基层清理、砂浆调制、运输，石材切割打磨、材料场内运输、铺贴、清扫现场、成品保护等","m",69.42,null,null,"材料甲供"]
[6,"扶手、压顶","1.600*450*100mm厚石材压顶，两侧机切20*10mm凹槽\n2.20mm厚1：2.5水泥砂浆结合层","基层清理、砂浆调制、运输，石材切割打磨、材料场内运输、铺贴、清扫现场、成品保护等","m",36.03,null,null,"材料甲供"]
["四","道牙部分"]
[1,"道牙铺设","1.600*150*350mm素混凝土立道牙\n2.30mm厚1:2.5厚水泥砂浆粘接层\n3.垫层、靠背混凝土浇筑","基层清理、砂浆调制、运输，材料场内运输、切割、安装、勾缝、护肩、清扫现场、成品保护等","m",2792.53,null,null,"材料甲供"]
[2,"道牙铺设","1.600*300*50mm素混凝土平道牙\n2.30mm厚1:2.5厚水泥砂浆粘接层\n3.垫层、靠背混凝土浇筑","基层清理、砂浆调制、运输，材料场内运输、切割、安装、勾缝、护肩、清扫现场、成品保护等","m",{"v":2531.2,"d":"2531.20"},null,null,"材料甲供"]
[3,"道牙铺设","1.300*300*80mm厚自然面青石道牙\n2.30mm厚1:2.5厚水泥砂浆粘接层\n3.垫层、靠背混凝土浇筑","基层清理、砂浆调制、运输，材料场内运输、切割、安装、勾缝、护肩、清扫现场、成品保护等","m",684.04,null,null,"材料甲供"]
[4,"道牙铺设","1.600*120*80mm厚自然面青石道牙\n2.30mm厚1:2.5厚水泥砂浆粘接层\n3.垫层、靠背混凝土浇筑","基层清理、砂浆调制、运输，材料场内运输、切割、安装、勾缝、护肩、清扫现场、成品保护等","m",{"$f":"487.72+20","v":507.72},null,null,"材料甲供"]
[null,"合计："]
["1.全费用综合单价：包含但不限于人工费（包括人员加班工资、差旅及窝工费、承包人供应材料保管费等）、甲供材下料、清点、卸车、验收、施工、养护、清理施工后现场、垃圾清运、材料二次倒运费用（平均按500m以内考虑）、机械费及小型机具费用、交叉施工影响及配合费用、赶工措施费用、技术服务费（测量放线等）、通讯费、交通费、食宿费、劳保用品费、生活生产水电费、相关保险费用、企业管理费、利润、措施费、规费、税金及政策性文件规定费用等所有费用。"]
["2、以上工程量均为暂定量，结算以现场实际发生工程量为准。"]
["3、材料损耗按山东省园林定额2016损耗考核，超过定额损耗的，由乙方承当损失，在工程结算中扣除。"]
["4、以上报价按9%的增值税税金报价，签订合同时按实际税点调整合同单价。"]