{"text_format":"3","workbook":"xlsx","n_sheets":7,"sheets":["总价汇总表","游客中心-装饰","游客中心-安装","游客中心措施费","花园餐厅装饰","花园餐厅安装","花园餐厅措施费"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"总价汇总表","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3],[18,0,18,3],[19,1,19,3],[21,1,21,3]]}
["投标报价汇总表"]
["工程名称：第四届中国绿化博览会游客服务中心、花园餐厅装饰装修专业分包工程"]
["序号","项目名称","投标总价","备注"]
["一","游客服务中心"]
[1,"装饰工程",{"$f":"'游客中心-装饰'!P259","v":{"v":37228.296,"d":"37228.30"}}]
[2,"安装工程",{"$f":"'游客中心-安装'!P113","v":{"v":0,"d":"0.00"}}]
[3,"措施费",{"$f":"游客中心措施费!E13","v":{"v":0,"d":"0.00"}}]
[null,"小计：",{"$f":"C7+C6+C5","v":{"v":37228.296,"d":"37228.30"}}]
["二","花园餐厅"]
[1,"装饰工程",{"$f":"花园餐厅装饰!P133","v":{"v":67100.4,"d":"67100.40"}}]
[2,"安装工程",{"$f":"花园餐厅安装!P91","v":{"v":6635.484,"d":"6635.48"}}]
[3,"措施费",{"$f":"花园餐厅措施费!E13","v":{"v":0,"d":"0.00"}}]
[null,"小计：",{"$f":"C12+C11+C10","v":{"v":73735.884,"d":"73735.88"}}]
[null,"合计：",{"$f":"C13+C8","v":110964.18}]
[]
["1、报价包含人工费（包括人员加班工资、差旅及窝工费）、材料费、机械费、管理费、利润、风险、规费、税金的包工包料价格，包含深化设计、监理资料及竣工图绘制费用，包括水电、卸货、材料保管、二次搬运、上楼、各种保险、加班、临时设施、赶工措施、已完工项目成品保护措施、夜间照明、安全文明施工等费用，施工人员的食宿费、劳保费用、办公费、生活生产水电费、保险费也包含在报价里,措施费按实际发生计取，不发生不计取。"]
["2、投标人应充分踏勘现场，对各区域各节点施工作业条件充分认识，投标报价已充分考虑现场构件运输、堆放等条件，在报价中综合体现，进场施工后招标人不做任何补偿。"]
["3、报价税率按9%考虑报价，提供9%税率的增值税专用发票。"]
[]
[null,"投标单位（公章）："]
[null,"授权委托人："]
[null,"日    期：   2020     年     月    日"]

{"sheet":"游客中心-装饰","index":1,"n_rows":265,"n_cols":20,"rows_kept":265,"merged":[[0,0,0,16],[1,0,1,16],[2,0,5,0],[2,1,5,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6],[2,7,2,14],[2,15,5,15],[2,16,5,16],[3,7,5,7],[3,8,3,13],[4,8,4,12],[4,14,5,14],[259,0,259,16],[260,0,260,16],[261,0,261,16]]}
["装饰工程量报价清单",{"$nulls":16},"甲控乙供，主材价暂定，按质定价"]
["工程名称：第四届中国绿博会游客服务中心装饰装修专业分包工程"]
["序号","分项工程名称","项目特征","单位","数量","主材名称","综合单价","其        中：",{"$nulls":7},"合价","备注"]
[{"$nulls":7},"人工费","材    料    费"]
[{"$nulls":8},"主材费",{"$nulls":5},"机械费"]
[{"$nulls":8},"名称及规格","单位","单位耗量","单价","单位主材费合价","辅材"]
[1,"1游客服务大厅"]
[2,"1.1游客服务大厅"]
[3,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",1.8,"石材门槛石",{"$f":"H9+M9+N9+O9","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"$f":"G9*E9","v":{"v":0,"d":"0.00"}},"石材甲供",null,null,1]
[4,"石材楼地面","1.ST-01灰色石材规格900*1200水泥砂浆铺贴。","m2",433.37,"石材",{"$f":"H10+N10+O10","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格900*1200","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,2]
[5,"金属踢脚线","1.基层另计。\n3.MT-05白色铝板饰面。\n4.详见图纸ID-07/B","m",41.78,"成品踢脚线",{"$f":"H11+M11+N11+O11","v":{"v":0,"d":"0.00"}},null,"MT-05白色铝板饰面","m2",null,null,{"$f":"L11*K11","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},3]
[6,"格栅吊顶","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.MT-03木纹铝方通，规格100*50。\n4.详见图纸ID-07/A","m2",429.33,"铝方通",{"$f":"H12+M12+N12+O12","v":{"v":0,"d":"0.00"}},null,"MT-03木纹铝方通\n规格100*50","m",null,15,{"$f":"L12*K12","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"MT-03木纹铝方通甲控乙供，主材价暂定，按质定价",null,null,4]
[7,"灯带（槽）","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.成品定制灯箱，规格150*80。\n4.详见图纸ID-07/A","m",277.84,"定制灯箱",{"$f":"H13+N13+O13+M13","v":{"v":0,"d":"0.00"}},null,"成品定制灯箱\n规格150*80","m",null,180,{"$f":"K13*L13","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"成品定制灯箱甲控乙供，主材价暂定，按质定价",null,null,5]
[8,"天棚喷刷涂料","1.原顶喷PT-03黑色乳胶漆。","m2",551.2,"乳胶漆",{"$f":"H14+M14+N14+O14","v":{"v":0,"d":"0.00"}},null,"黑色乳胶漆","m2",null,null,{"$f":"L14*K14","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},6]
[9,"墙面装饰板","1.基层龙骨另计。\n3.铝扣板专用卡式龙骨。\n4.MT-05铝板饰面。","m2",172.65,"铝板",{"$f":"H15+M15+N15+O15","v":{"v":0,"d":"0.00"}},null,"MT-05铝板","m2",null,150,{"$f":"L15*K15","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价",null,null,7]
[10,"服务台","1.木制服务台，尺寸：7200*1100*1200\n2.详见图纸ID-08","个",1,"木制服务台",{"$f":"H16+M16+N16+O16","v":{"v":0,"d":"0.00"}},null,"木制服务台\n尺寸：7200*1100*1200","个",null,null,{"$f":"L16*K16","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},10]
[11,"1.2游客服务大厅接待室",{"$nulls":13},{"v":0,"d":"0.00"}]
[12,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",1.08,"石材门槛石",{"$f":"H18+M18+N18+O18","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,11]
[13,"石材楼地面","1.ST-01灰色石材规格900*1200水泥砂浆铺贴。","m2",48.2,"石材",{"$f":"H19+N19+O19","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格900*1200","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,12]
[14,"金属踢脚线","1.金属踢脚线，高度50mm。","m",19.91,"成品踢脚线",{"$f":"H20+M20+N20+O20","v":{"v":0,"d":"0.00"}},null,"踢脚线\nH50mm","m",null,null,{"$f":"L20*K20","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},13]
[15,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.双层9.5mm纸面石膏板。","m2",48.2,"纸面石膏板",{"v":0,"d":"0.00"},null,"纸面石膏板9.5mm厚","m2",null,null,{"$f":"L21*K21","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},14]
[16,"灯带（槽）","1.Φ8吊筋，M8膨胀螺栓固定。\n2.阻燃夹板、9.5mm纸面石膏板。\n3.自粘胶带、腻子、乳胶漆另计。\n4.尺寸280+120+80，详见图纸ID-07/04。","m",17.39,"纸面石膏板",{"v":0,"d":"0.00"},null,"纸面石膏板9.5mm厚","m2",null,null,{"$f":"L22*K22","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},15]
[17,"开孔（打洞）","1.石膏板开灯孔。","个",16,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},16]
[18,"开孔（打洞）","1.石膏板开出风口孔。","个",2,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},17]
[19,"送风口、回风口","1.木基层风口基层。\n2.木基层防火涂料。\n3.成品风口其他单位施工","个",2,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},18]
[20,"弧形木窗帘盒","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.阻燃夹板、9.5mm纸面石膏板。\n4.自粘胶带、腻子、乳胶漆另计。\n5.尺寸:200*200,详见图纸ID-07/02.","m",11.36,"纸面石膏板",{"v":0,"d":"0.00"},null,"纸面石膏板9.5mm厚","m2",null,null,{"$f":"L26*K26","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},19]
[21,"木质门带套","1.成品套装双开门，尺寸：1750*2380\n2.门五金另计","樘",1,"成品套装门",{"v":0,"d":"0.00"},null,"成品套装双开门\n尺寸：1750*2380","樘",null,null,{"$f":"L27*K27","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},20]
[22,"1.3卫生间",{"$nulls":13},{"v":0,"d":"0.00"}]
[23,"1.3.1卫生间前室",{"$nulls":13},{"v":0,"d":"0.00"}]
[24,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",2.02,"石材门槛石",{"$f":"H30+M30+N30+O30","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,23]
[25,"石材楼地面","1.ST-01灰色石材规格300*600水泥砂浆铺贴。","m2",50.06,"石材",{"$f":"H31+N31+O31","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格300*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,24]
[26,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.双层防水9.5mm纸面石膏板。","m2",50.06,"纸面石膏板",{"$f":"H32+M32+N32+O32","v":{"v":0,"d":"0.00"}},null,"防水9.5mm纸面石膏板","m2",null,null,{"$f":"L32*K32","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},25]
[27,"开孔（打洞）","1.石膏板开灯孔。","个",22,null,{"$f":"H33+M33+N33+O33","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},26]
[28,"石材墙面","1.水泥砂浆粘贴。\n2.ST-01灰色石材规格300*600","m2",165.46,"石材",{"$f":"H34+N34+O34","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格300*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,27]
[29,"成品木门窗套","1.成品WD-01木饰面门套。","m",11.28,"成品门套",{"$f":"H35+M35+N35+O35","v":{"v":0,"d":"0.00"}},null,"成品WD-01木饰面门套","m",null,null,{"$f":"L35*K35","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},28]
[30,"洗漱台","1.高度250mm,挡水板高度50mm。\n2.型钢骨架，ST-02白色石材饰面。\n3.台盆开工、磨边，挡水条及阳角倒角、磨边。\n4.详见图纸","m2",9.8,"石材",{"$f":"H36+M36+N36+O36","v":{"v":0,"d":"0.00"}},null,"ST-02白色石材","m2",null,350,{"$f":"L36*K36","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"ST-02白色石材甲控乙供，主材价暂定，按质定价",null,null,29]
[31,"卫生纸盒","1.不锈钢纸盒","个",2,"不锈钢纸盒",{"$f":"H37+M37+N37+O37","v":{"v":0,"d":"0.00"}},null,"不锈钢纸盒","个",null,null,{"$f":"L37*K37","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},30]
[32,"镜面玻璃","1.MR-01银镜玻璃。\n2.带框","m2",9.14,"成品银镜",{"$f":"H38+M38+N38+O38","v":{"v":0,"d":"0.00"}},null,"MR-01银镜玻璃","m2",null,null,{"$f":"L38*K38","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},31]
[33,"1.3.2第三卫生间",{"$nulls":13},{"v":0,"d":"0.00"}]
[34,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",0.36,"石材门槛石",{"$f":"H40+M40+N40+O40","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,33]
[35,"石材楼地面","1.ST-01灰色石材规格300*600水泥砂浆铺贴。","m2",10.62,"石材",{"$f":"H41+N41+O41","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格300*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,34]
[36,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.双层防水9.5mm纸面石膏板。","m2",10.62,"纸面石膏板",{"$f":"H42+M42+N42+O42","v":{"v":0,"d":"0.00"}},null,"防水9.5mm纸面石膏板","m2",null,null,{"$f":"L42*K42","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},35]
[37,"开孔（打洞）","1.石膏板开灯孔。","个",6,null,{"$f":"H43+M43+N43+O43","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},36]
[38,"开孔（打洞）","1.石膏板开出风口孔。","个",2,null,{"$f":"H44+M44+N44+O44","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},37]
[39,"送风口、回风口","1.木基层风口基层。\n2.木基层防火涂料。\n3.成品风口其他单位施工","个",2,null,{"$f":"H45+M45+N45+O45","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},38]
[40,"石材墙面","1.水泥砂浆粘贴。\n2.ST-01灰色石材规格300*600","m2",49.84,"石材",{"$f":"H46+N46+O46","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格300*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,39]
[41,"木质门带套","1.成品套装双开门，尺寸：1150*2070\n2.门五金另计","樘",1,"成品套装门",{"$f":"H47+M47+N47+O47","v":{"v":0,"d":"0.00"}},null,"成品套装双开门\n尺寸：1150*2070","樘",null,null,{"$f":"L47*K47","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},40]
[42,"卫生间扶手","1.洗漱台残疾人扶手","副",1,"残疾人扶手",{"$f":"H48+M48+N48+O48","v":{"v":0,"d":"0.00"}},null,"残疾人扶手","副",null,null,{"$f":"L48*K48","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},41]
[43,"卫生间扶手","1.坐便器残疾人扶手","副",1,"残疾人扶手",{"$f":"H49+M49+N49+O49","v":{"v":0,"d":"0.00"}},null,"残疾人扶手","副",null,null,{"$f":"L49*K49","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},42]
[44,"卫生纸盒","1.不锈钢纸盒","个",2,"不锈钢纸盒",{"$f":"H50+M50+N50+O50","v":{"v":0,"d":"0.00"}},null,"不锈钢纸盒","个",null,null,{"$f":"L50*K50","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},43]
[45,"镜面玻璃","1.MR-01银镜玻璃。\n2.带框","m2",2.4,"成品银镜",{"$f":"H51+M51+N51+O51","v":{"v":0,"d":"0.00"}},null,"MR-01银镜玻璃","m2",null,null,{"$f":"L51*K51","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},44]
[46,"1.3.3男、女卫生间",{"$nulls":13},{"v":0,"d":"0.00"}]
[47,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",0.44,"石材门槛石",{"$f":"H53+M53+N53+O53","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,46]
[48,"石材楼地面","1.ST-01灰色石材规格300*600水泥砂浆铺贴。","m2",67.98,"石材",{"$f":"H54+N54+O54","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格300*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,47]
[49,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.双层防水9.5mm纸面石膏板。\n4.自粘胶带、腻子、乳胶漆另计。","m2",67.98,"纸面石膏板",{"$f":"H55+M55+N55+O55","v":{"v":0,"d":"0.00"}},null,"防水9.5mm纸面石膏板","m2",null,null,{"$f":"L55*K55","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},48]
[50,"灯带（槽）","1.Φ8吊筋，M8膨胀螺栓固定。\n2.阻燃夹板、双层防水9.5mm纸面石膏板。\n3.自粘胶带、腻子、乳胶漆另计。\n5.尺寸300+120+80。","m",34.25,"纸面石膏板",{"$f":"H56+M56+N56+O56","v":{"v":0,"d":"0.00"}},null,"防水9.5mm纸面石膏板","m2",null,null,{"$f":"L56*K56","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},49]
[51,"开孔（打洞）","1.石膏板开灯孔。","个",7,null,{"$f":"H57+M57+N57+O57","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},50]
[52,"开孔（打洞）","1.石膏板开出风口孔。","个",6,null,{"$f":"H58+M58+N58+O58","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},51]
[53,"送风口、回风口","1.木基层风口基层。\n2.木基层防火涂料。\n3.成品风口其他单位施工","个",6,null,{"$f":"H59+M59+N59+O59","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"$f":"G59*E59","v":{"v":0,"d":"0.00"}},{"$nulls":3},52]
[54,"石材墙面","1.水泥砂浆粘贴。\n2.ST-01灰色石材规格300*600","m2",207.65,"石材",{"$f":"H60+N60+O60","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格300*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,53]
[55,"木质门带套","1.成品套装单开门，尺寸：850*2070\n2.门五金另计","樘",2,"成品套装门",{"v":0,"d":"0.00"},null,"成品套装单开门\n尺寸：850*2070","樘",null,null,{"$f":"L61*K61","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},54]
[56,"成品隔断","1.卫生间蹲坑WD-01木饰面成品隔断间。\n2.含五金。","间",26,"成品隔断",{"v":0,"d":"0.00"},null,"WD-01木饰面成品隔断间","间",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},55]
[57,"成品隔断","1.卫生间WD-01木饰面成品小便斗隔断。","套",7,"小便斗隔断",{"v":0,"d":"0.00"},null,"小便斗隔断","套",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},56]
[58,"卫生纸盒","1.不锈钢纸盒","个",26,"不锈钢纸盒",{"v":0,"d":"0.00"},null,"不锈钢纸盒","个",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},57]
[59,"1.3.4清洁间",{"$nulls":13},{"v":0,"d":"0.00"}]
[60,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",0.25,"石材门槛石",{"$f":"H66+M66+N66+O66","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,59]
[61,"石材楼地面","1.ST-01灰色石材规格300*600水泥砂浆铺贴。","m2",4.6,"石材",{"$f":"H67+N67+O67","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格300*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,60]
[62,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.双层防水9.5mm纸面石膏板。\n4.自粘胶带、腻子、乳胶漆另计。","m2",4.6,"纸面石膏板",{"$f":"H68+M68+N68+O68","v":{"v":0,"d":"0.00"}},null,"防水9.5mm纸面石膏板","m2",null,null,{"$f":"L68*K68","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},61]
[63,"开孔（打洞）","1.石膏板开灯孔。","个",2,null,{"$f":"H69+M69+N69+O69","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},62]
[64,"石材墙面","1.水泥砂浆粘贴。\n2.ST-01灰色石材规格300*600","m2",29.6,"石材",{"$f":"H70+N70+O70","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格300*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,63]
[65,"木质门带套","1.成品套装单开门，尺寸：850*2070\n2.门五金另计","樘",1,"成品套装门",{"$f":"H71+M71+N71+O71","v":{"v":0,"d":"0.00"}},null,"成品套装单开门\n尺寸：850*2070","樘",null,null,{"$f":"L71*K71","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},64]
[66,"2纪念品商店",{"$nulls":13},{"v":0,"d":"0.00"}]
[67,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",1.38,"石材门槛石",{"$f":"H73+M73+N73+O73","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,65]
[68,"石材楼地面","1.ST-01灰色石材规格900*1200水泥砂浆铺贴。","m2",303.39,"石材",{"$f":"H74+N74+O74","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格900*1200","m2",null,"/","/",null,null,{"$f":"G74*E74","v":{"v":0,"d":"0.00"}},"石材甲供",null,null,66]
[69,"地面成品灯带","1.LED成品灯带，宽100mm。","m",58,"成品灯带",{"$f":"H75+M75+N75+O75","v":{"v":0,"d":"0.00"}},null,"地面成品灯带","m",null,null,{"$f":"L75*K75","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},67]
[70,"金属踢脚线","1.金属踢脚线，高度50mm。","m",8.17,"成品踢脚线",{"$f":"H76+M76+N76+O76","v":{"v":0,"d":"0.00"}},null,"踢脚线\nH50mm","m",null,null,{"$f":"L76*K76","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},68]
[71,"格栅吊顶","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.MT-03木纹铝方通，规格100*50。\n4.详见图纸ID-07/A","m2",353.6,"铝方通",{"$f":"H77+M77+N77+O77","v":{"v":0,"d":"0.00"}},null,"MT-03木纹铝方通\n规格100*50","m",null,15,{"$f":"L77*K77","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"MT-03木纹铝方通甲控乙供，主材价暂定，按质定价",null,null,69]
[72,"灯带（槽）","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.成品定制灯箱，规格150*80。\n4.详见图纸ID-07/A。","m",190.63,"定制灯箱",{"$f":"H78+N78+O78+M78","v":{"v":0,"d":"0.00"}},null,"成品定制灯箱\n规格150*80","m",null,180,{"$f":"K78*L78","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"成品定制灯箱甲控乙供，主材价暂定，按质定价",null,null,70]
[73,"天棚喷刷涂料","1.原顶喷PT-03黑色乳胶漆。","m2",408,"乳胶漆",{"$f":"H79+M79+N79+O79","v":{"v":0,"d":"0.00"}},null,"黑色乳胶漆","m2",null,null,{"$f":"L79*K79","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},71]
[74,"吧台背柜","1.木龙骨、阻燃板基层。\n2.木基层防火涂料。\n3.纸面石膏板9.5mm面层。\n4.尺寸：2800*1800\n5.详见图纸IE-10/05、ID-6/02。","个",2,"吧台背柜",{"$f":"H80+M80+N80+O80","v":{"v":0,"d":"0.00"}},null,"吧台背柜2800*1800","个",null,null,{"$f":"L80*K80","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},72]
[75,"吧台背柜","1.木龙骨、阻燃板基层。\n2.木基层防火涂料。\n3.纸面石膏板9.5mm面层。\n4.尺寸：2800*2100\n5.详见图纸IE-10/05、ID-6/02。","个",1,"吧台背柜",{"$f":"H81+M81+N81+O81","v":{"v":0,"d":"0.00"}},null,"吧台背柜2800*2100","个",null,null,{"$f":"L81*K81","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},73]
[76,"其他隔断","1.木龙骨、细木工板18mm基层。\n2.木基层防火涂料。\n3.纸面石膏板9.5mm面层。\n4.详见图纸IE-10/05、ID-6/02。","m2",14.68,"纸面石膏板",{"$f":"H82+M82+N82+O82","v":{"v":0,"d":"0.00"}},null,"纸面石膏板9.5mm厚","m2",null,null,{"$f":"L82*K82","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},74]
[77,"3生态饮食餐厅",{"$nulls":13},{"v":0,"d":"0.00"}]
[78,"3.1一楼餐厅",{"$nulls":13},{"v":0,"d":"0.00"}]
[79,"3.1.1生态饮食餐厅",{"$nulls":13},{"v":0,"d":"0.00"}]
[80,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",2.16,"石材门槛石",{"$f":"H86+M86+N86+O86","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,76]
[81,"石材楼地面","1.ST-01灰色石材规格900*1200水泥砂浆铺贴。","m2",369.6,"石材",{"$f":"H87+N87+O87","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格900*1200","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,77]
[82,"竹、木（复合）地板","1.WD-02木地板。\n2.防潮垫。","m2",33.08,"木地板",{"$f":"H88+M88+N88+O88","v":{"v":0,"d":"0.00"}},null,"WD-02木地板","m2",null,100,{"$f":"L88*K88","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"WD-02木地板甲控乙供，主材价暂定，按质定价",null,null,78]
[83,"格栅吊顶","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.MT-03木纹铝方通，规格100*50。\n4.详见图纸ID-07/A","m2",479.7,"铝方通",{"$f":"H89+M89+N89+O89","v":{"v":0,"d":"0.00"}},null,"MT-03木纹铝方通\n规格100*50","m",null,15,{"$f":"L89*K89","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"MT-03木纹铝方通甲控乙供，主材价暂定，按质定价",null,null,79]
[84,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.细木工板基层，防火涂料。\n4.MT-03木纹铝铝板粘贴。","m2",29.61,"铝板",{"$f":"H90+M90+N90+O90","v":{"v":0,"d":"0.00"}},null,"MT-03木纹铝铝板","m2",null,180,{"$f":"L90*K90","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价",null,null,80]
[85,"灯带（槽）","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.成品定制灯箱，规格150*80。\n4.详见图纸ID-07/A。","m",157.34,"定制灯箱",{"$f":"H91+N91+O91+M91","v":{"v":0,"d":"0.00"}},null,"成品定制灯箱\n规格150*80","m",null,180,{"$f":"K91*L91","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"成品定制灯箱甲控乙供，主材价暂定，按质定价",null,null,81]
[86,"天棚喷刷涂料","1.原顶喷PT-03黑色乳胶漆。","m2",551.2,"乳胶漆",{"$f":"H92+M92+N92+O92","v":{"v":0,"d":"0.00"}},null,"黑色乳胶漆","m2",null,null,{"$f":"L92*K92","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},82]
[87,"墙面装饰板","1.MT-03木纹铝方通@200。\n2.龙骨、基层板、石膏板另计。\n3.详见图纸DS-03/03。","m2",32.05,"铝方通",{"$f":"H93+M93+N93+O93","v":{"v":0,"d":"0.00"}},null,"MT-03木纹铝方通\n规格100*50","m",null,15,{"$f":"L93*K93","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"MT-03木纹铝方通甲控乙供，主材价暂定，按质定价",null,null,83]
[88,"木饰面隔板","1.WD-01木饰面，尺寸：400*60。\n2.细木工板基层，防火涂料。\n3.镀锌方管龙骨。\n4.暗藏灯带。\n5.详见图纸DS-03/01。","m",60.52,"木饰面",{"$f":"H94+M94+N94+O94","v":{"v":0,"d":"0.00"}},null,"WD-01木饰面","m2",null,320,{"$f":"L94*K94","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"WD-01木饰面甲控乙供，主材价暂定，按质定价",null,null,86]
[89,"收银台","1.WD-01木饰面弧形收银台。\n2.详见图纸DS-06/01、DS-06/02。","个",1,"收银台",{"$f":"H95+M95+N95+O95","v":{"v":0,"d":"0.00"}},null,"收银台","个",null,null,{"$f":"L95*K95","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},88]
[90,"吧台背柜","1.WD-01木饰面弧形收银台背柜。\n2.详见图纸DS-06/01、DS-06/02。","个",1,"吧台背柜",{"$f":"H96+M96+N96+O96","v":{"v":0,"d":"0.00"}},null,"弧形收银台背柜","个",null,null,{"$f":"L96*K96","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},89]
[91,"3.1.2后厨、更衣室",{"$nulls":13},{"v":0,"d":"0.00"}]
[92,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",1.52,"石材门槛石",{"$f":"H98+M98+N98+O98","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,92]
[93,"块料楼地面","1.CT-01白色地砖300*300水泥砂浆粘贴。","m2",62.85,"地砖",{"$f":"H99+N99+O99","v":{"v":0,"d":"0.00"}},null,"CT-01白色地砖\n规格300*300","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖主材甲供",null,null,93]
[94,"块料楼地面","1.CT-02灰色地砖300*300水泥砂浆粘贴。","m2",12.81,"地砖",{"v":0,"d":"0.00"},null,"CT-02灰色地砖\n规格300*300","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖主材甲供",null,null,94]
[95,"块料踢脚线","1.CT-01白色地砖踢脚线水泥砂浆粘贴。","m",28.63,"地砖踢脚线",{"v":0,"d":"0.00"},null,"CT-01白色地砖踢脚","m",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖踢脚线甲供",null,null,95]
[96,"块料踢脚线","1.CT-02灰色地砖踢脚线水泥砂浆粘贴。","m",19.62,"地砖踢脚线",{"v":0,"d":"0.00"},null,"CT-02灰色地砖踢脚","m",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖踢脚线甲供",null,null,96]
[97,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.铝合金扣板轻钢龙骨。\n3.MT-04白色铝扣板吊顶。","m2",29.24,"铝扣板",{"$f":"H103+M103+N103+O103","v":{"v":0,"d":"0.00"}},null,"MT-04白色铝扣板","m2",null,null,{"$f":"L103*K103","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},97]
[98,"块料墙面","1.300*600墙面墙砖水泥砂浆粘贴。\n2.密封","m2",51.97,"墙砖",{"$f":"H104+M104+N104+O104","v":{"v":0,"d":"0.00"}},null,"墙砖\n规格300*600","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"墙砖甲供",null,null,98]
[99,"石材窗台板","1.石材窗台板专用粘接剂安装。\n2.规格暂定120*40mm，倒角。","m2",1.6,"石材窗台板",{"$f":"H105+M105+N105+O105","v":{"v":0,"d":"0.00"}},null,"石材窗台板\n规格暂定120*40mm","m2",null,350,{"$f":"L105*K105","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"石材窗台板甲控乙供，主材价暂定，按质定价",null,null,100]
[100,"木质门带套","1.成品套装单开门，尺寸：850*2070\n2.门五金另计","樘",3,"成品套装门",{"$f":"H106+M106+N106+O106","v":{"v":0,"d":"0.00"}},null,"成品套装单开门\n尺寸：850*2070","樘",null,null,{"$f":"L106*K106","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},101]
[101,"木质门带套","1.成品套装双开门，尺寸：1500*2100\n2.门五金另计","樘",3,"成品套装门",{"$f":"H107+M107+N107+O107","v":{"v":0,"d":"0.00"}},null,"成品套装双开门\n尺寸：1500*2100","樘",null,null,{"$f":"L107*K107","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},102]
[102,"3.1.3电梯厅、洗碗间、预进间",{"$nulls":13},{"v":0,"d":"0.00"}]
[103,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",1.79,"石材门槛石",{"$f":"H109+M109+N109+O109","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,103]
[104,"块料楼地面","1.CT-01白色地砖300*300水泥砂浆粘贴。","m2",29.24,"地砖",{"$f":"H110+N110+O110","v":{"v":0,"d":"0.00"}},null,"CT-01白色地砖\n规格300*300","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖主材甲供",null,null,104]
[105,"块料踢脚线","1.CT-01白色地砖踢脚线水泥砂浆粘贴。","m",31.8,"地砖踢脚线",{"$f":"H111+N111+O111","v":{"v":0,"d":"0.00"}},null,"CT-01白色地砖踢脚","m",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖踢脚线甲供",null,null,105]
[106,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.铝合金扣板轻钢龙骨。\n3.MT-04白色铝扣板吊顶。","m2",29.24,"铝扣板",{"$f":"H112+M112+N112+O112","v":{"v":0,"d":"0.00"}},null,"MT-04白色铝扣板","m2",null,null,{"$f":"L112*K112","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},106]
[107,"石材窗台板","1.石材窗台板专用粘接剂安装。\n2.规格暂定120*40mm，倒角。","m2",0.8,"石材窗台板",{"$f":"H113+M113+N113+O113","v":{"v":0,"d":"0.00"}},null,"石材窗台板\n规格暂定120*40mm","m2",null,350,{"$f":"L113*K113","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"石材窗台板甲控乙供，主材价暂定，按质定价",null,null,108]
[108,"木质门带套","1.成品套装双开门，尺寸：1500*2100\n2.门五金另计","樘",2,"成品套装门",{"$f":"H114+M114+N114+O114","v":{"v":0,"d":"0.00"}},null,"成品套装双开门\n尺寸：1500*2100","樘",null,null,{"$f":"L114*K114","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},109]
[109,"3.1.4卫生间",{"$nulls":13},{"v":0,"d":"0.00"}]
[110,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",1.19,"石材门槛石",{"$f":"H116+M116+N116+O116","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,111]
[111,"石材楼地面","1.ST-01灰色石材规格300*600水泥砂浆铺贴。","m2",41.64,"石材",{"$f":"H117+N117+O117","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格300*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,112]
[112,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.双层防水9.5mm纸面石膏板。\n4.自粘胶带、腻子、乳胶漆另计。","m2",41.64,"纸面石膏板",{"$f":"H118+M118+N118+O118","v":{"v":0,"d":"0.00"}},null,"防水9.5mm纸面石膏板","m2",null,null,{"$f":"L118*K118","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},113]
[113,"开孔（打洞）","1.石膏板开灯孔。","个",13,null,{"$f":"H119+M119+N119+O119","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},114]
[114,"石材墙面","1.水泥砂浆粘贴。\n2.ST-01灰色石材规格300*600","m2",123.32,"石材",{"$f":"H120+N120+O120","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格300*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,115]
[115,"洗漱台","1.高度250mm,挡水板高度50mm。\n2.型钢骨架，ST-02白色石材饰面。\n3.台盆开工、磨边，挡水条及阳角倒角、磨\n边。\n4.详见图纸","m2",1.53,"石材",{"$f":"H121+M121+N121+O121","v":{"v":0,"d":"0.00"}},null,"ST-02白色石材","m2",null,350,{"$f":"L121*K121","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"ST-02白色石材甲控乙供，主材价暂定，按质定价",null,null,116]
[116,"成品木门窗套","1.成品WD-01木饰面门套。","m",6.84,"成品门套",{"v":0,"d":"0.00"},null,"成品WD-01木饰面门套","m",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},117]
[117,"木质门带套","1.成品套装单开门，尺寸：850*2070\n2.门五金另计","樘",4,"成品套装门",{"v":0,"d":"0.00"},null,"成品套装单开门\n尺寸：850*2070","樘",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},118]
[118,"卫生纸盒","1.不锈钢纸盒","个",8,"不锈钢纸盒",{"v":0,"d":"0.00"},null,"不锈钢纸盒","个",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},119]
[119,"镜面玻璃","1.MR-01银镜玻璃。\n2.带框","m2",2.16,"成品银镜",{"v":0,"d":"0.00"},null,"MR-01银镜玻璃","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},120]
[120,"卫生间扶手","1.洗漱台残疾人扶手","副",1,"残疾人扶手",{"v":0,"d":"0.00"},null,"洗漱台残疾人扶手","套",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},121]
[121,"卫生间扶手","1.坐便器残疾人扶手","副",1,"残疾人扶手",{"v":0,"d":"0.00"},null,"坐便器残疾人扶手","套",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},122]
[122,"成品隔断","1.卫生间蹲坑WD-01木饰面成品隔断间。\n2.含五金。","间",8,"成品隔断",{"v":0,"d":"0.00"},null,"WD-01木饰面成品隔断间","间",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},123]
[123,"成品隔断","1.卫生间WD-01木饰面成品小便斗隔断。","套",2,"小便斗隔断",{"v":0,"d":"0.00"},null,"小便斗隔断","套",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},124]
[124,"3.2二楼餐厅",{"$nulls":13},{"v":0,"d":"0.00"}]
[125,"3.2.1生态饮食餐厅、过道",{"$nulls":13},{"v":0,"d":"0.00"}]
[126,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",1.19,"石材门槛石",{"$f":"H132+M132+N132+O132","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,125]
[127,"石材楼地面","1.ST-01灰色石材规格900*1200水泥砂浆铺贴。","m2",441.85,"石材",{"$f":"H133+N133+O133","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格900*1200","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,126]
[128,"格栅吊顶","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.MT-03木纹铝方通，规格100*50。\n4.详见图纸ID-07/A","m2",482.3,"铝方通",{"$f":"H134+M134+N134+O134","v":{"v":0,"d":"0.00"}},null,"MT-03木纹铝方通\n规格100*50","m",null,15,{"$f":"L134*K134","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"MT-03木纹铝方通甲控乙供，主材价暂定，按质定价",null,null,127]
[129,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.细木工板基层，防火涂料。\n4.MT-03木纹铝铝板粘贴。","m2",31,"铝板",{"$f":"H135+M135+N135+O135","v":{"v":0,"d":"0.00"}},null,"MT-03木纹铝铝板","m2",null,180,{"$f":"L135*K135","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价",null,null,128]
[130,"灯带（槽）","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.成品定制灯箱，规格150*80。\n4.详见图纸ID-07/A","m",157.72,"定制灯箱",{"$f":"H136+N136+O136+M136","v":{"v":0,"d":"0.00"}},null,"成品定制灯箱\n规格150*80","m",null,180,{"$f":"K136*L136","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"成品定制灯箱甲控乙供，主材价暂定，按质定价",null,null,129]
[131,"天棚喷刷涂料","1.原顶喷PT-03黑色乳胶漆。","m2",625.3,"乳胶漆",{"$f":"H137+M137+N137+O137","v":{"v":0,"d":"0.00"}},null,"黑色乳胶漆","m2",null,null,{"$f":"L137*K137","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},130]
[132,"墙面装饰板","1.MT-03木纹铝折型铝板：规格50*70mm。\n2.铝扣板专用卡式龙骨\n4.基层龙骨另计\n5.详见图纸DS-04/02、DS-04/03、DS-05/02。","m2",102.88,"铝板",{"$f":"H138+M138+N138+O138","v":{"v":0,"d":"0.00"}},null,"MT-03木纹铝折型铝板\n规格50*70mm","m2\n（展开）",null,190,{"$f":"L138*K138","v":{"v":0,"d":"0.00"}},null,null,{"$f":"G138*E138","v":{"v":0,"d":"0.00"}},"铝板甲控乙供，主材价暂定，按质定价",null,null,132]
[133,"墙面装饰板","1.MT-03木纹铝板.\n2.铝扣板专用卡式龙骨\n4.基层龙骨另计\n5.详见图纸DS-04/02、DS-04/03、DS-05/02。","m2",20,"铝板",{"$f":"H139+M139+N139+O139","v":{"v":0,"d":"0.00"}},null,"MT-03木纹铝板","m2",null,180,{"$f":"L139*K139","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价",null,null,133]
[134,"3.2.2包间（12座）",{"$nulls":13},{"v":0,"d":"0.00"}]
[135,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",0.72,"石材门槛石",{"$f":"H141+M141+N141+O141","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,136]
[136,"竹、木（复合）地板","1..WD-02木地板。\n2.防潮垫。","m2",40.95,"木地板",{"v":0,"d":"0.00"},null,"WD-02木地板","m2",null,100,{"$f":"L142*K142","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"WD-02木地板甲控乙供，主材价暂定，按质定价",null,null,137]
[137,"木质踢脚线","1.WD-02木地板踢脚线","m",126.03,"木地板踢脚线",{"v":0,"d":"0.00"},null,"WD-02木地板踢脚线","m",null,null,{"$f":"L143*K143","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},138]
[138,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.双层9.5mm纸面石膏板。\n4.自粘胶带、腻子、乳胶漆另计。","m2",40.95,"纸面石膏板",{"v":0,"d":"0.00"},null,"纸面石膏板9.5mm厚","m2",null,null,{"$f":"L144*K144","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},139]
[139,"圆形灯带（槽）","1.Φ8吊筋，M8膨胀螺栓固定。\n2.阻燃夹板、9.5mm纸面石膏板。\n3.自粘胶带、腻子、乳胶漆另计。\n5.尺寸300+120+80。","m",7.47,"纸面石膏板",{"v":0,"d":"0.00"},null,"纸面石膏板9.5mm厚","m2",null,null,{"$f":"L145*K145","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},140]
[140,"开孔（打洞）","1.石膏板开灯孔。","个",6,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},141]
[141,"开孔（打洞）","1.石膏板开出风口孔。","个",2,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},142]
[142,"送风口、回风口","1.木基层风口基层。\n2.木基层防火涂料。\n3.成品风口其他单位施工","个",2,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},143]
[143,"石材窗台板","1.石材窗台板专用粘接剂安装。\n2.规格暂定120*40mm，倒角。","m2",1.2,"石材窗台板",{"v":0,"d":"0.00"},null,"石材窗台板\n规格暂定120*40mm","m2",null,350,{"$f":"L149*K149","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"石材窗台板甲控乙供，主材价暂定，按质定价",null,null,145]
[144,"木质门带套","1.成品套装双开门，尺寸：1500*2100\n2.门五金另计","樘",2,"成品套装门",{"v":0,"d":"0.00"},null,"成品套装双开门\n尺寸：1500*2100","樘",null,null,{"$f":"L150*K150","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},146]
[145,"3.2.3包间（8座）",{"$nulls":13},{"v":0,"d":"0.00"}]
[146,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",0.36,"石材门槛石",{"$f":"H152+M152+N152+O152","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,147]
[147,"竹、木（复合）地板","1.WD-02木地板。\n2.防潮垫。","m2",33.92,"木地板",{"v":0,"d":"0.00"},null,"WD-02木地板","m2",null,100,{"$f":"L153*K153","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"WD-02木地板甲控乙供，主材价暂定，按质定价",null,null,148]
[148,"木质踢脚线","1.WD-02木地板踢脚线","m",22.63,"木地板踢脚线",{"v":0,"d":"0.00"},null,"WD-02木地板踢脚线","m",null,null,{"$f":"L154*K154","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},149]
[149,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.双层纸面石膏板。\n4.自粘胶带、腻子、乳胶漆另计。","m2",33.92,"纸面石膏板",{"v":0,"d":"0.00"},null,"纸面石膏板9.5mm厚","m2",null,null,{"$f":"L155*K155","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},150]
[150,"圆形灯带（槽）","1.Φ8吊筋，M8膨胀螺栓固定。\n2.阻燃夹板、9.5mm纸面石膏板。\n3.自粘胶带、腻子、乳胶漆另计。\n5.尺寸300+120+80。","m",6.28,"纸面石膏板",{"v":0,"d":"0.00"},null,"纸面石膏板9.5mm厚","m2",null,null,{"$f":"L156*K156","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},151]
[151,"开孔（打洞）","1.石膏板开灯孔。","个",6,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},152]
[152,"开孔（打洞）","1.石膏板开出风口孔。","个",2,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},153]
[153,"送风口、回风口","1.木基层风口基层。\n2.木基层防火涂料。\n3.成品风口其他单位施工","个",2,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},154]
[154,"石材窗台板","1.石材窗台板专用粘接剂安装。\n2.规格暂定120*40mm，倒角。","m2",0.72,"石材窗台板",{"v":0,"d":"0.00"},null,"石材窗台板\n规格暂定120*40mm","m2",null,350,{"$f":"L160*K160","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"石材窗台板甲控乙供，主材价暂定，按质定价",null,null,156]
[155,"木质门带套","1.成品套装双开门，尺寸：1500*2100\n2.门五金另计","樘",1,"成品套装门",{"v":0,"d":"0.00"},null,"成品套装双开门\n尺寸：1500*2100","樘",null,null,{"$f":"L161*K161","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},157]
[156,"3.2.4卫生间",{"$nulls":13},{"v":0,"d":"0.00"}]
[157,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",1.06,"石材门槛石",{"$f":"H163+M163+N163+O163","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,159]
[158,"石材楼地面","1.ST-01灰色石材规格300*600水泥砂浆铺贴。","m2",34.93,"石材",{"$f":"H164+N164+O164","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格300*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,160]
[159,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.双层防水9.5mm纸面石膏板。\n4.自粘胶带、腻子、乳胶漆另计。","m2",34.93,"纸面石膏板",{"$f":"H165+M165+N165+O165","v":{"v":0,"d":"0.00"}},null,"防水9.5mm纸面石膏板","m2",null,null,{"$f":"L165*K165","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},161]
[160,"开孔（打洞）","1.石膏板开灯孔。","个",11,null,{"$f":"H166+M166+N166+O166","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},162]
[161,"石材墙面","1.水泥砂浆粘贴。\n2.ST-01灰色石材规格300*600","m2",99.4,"石材",{"$f":"H167+N167+O167","v":{"v":0,"d":"0.00"}},null,"ST-01灰色石材\n规格300*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,163]
[162,"洗漱台","1.高度250mm,挡水板高度50mm。\n2.型钢骨架，ST-02白色石材饰面。\n3.台盆开工、磨边，挡水条及阳角倒角、磨边。\n4.详见图纸","m2",1.6,"石材",{"$f":"H168+M168+N168+O168","v":{"v":0,"d":"0.00"}},null,"ST-02白色石材","m2",null,350,{"$f":"L168*K168","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"ST-02白色石材甲控乙供，主材价暂定，按质定价",null,null,164]
[163,"成品木门窗套","1.成品WD-01木饰面门套。","m",5.9,"成品门套",{"v":0,"d":"0.00"},null,"成品WD-01木饰面门套","m",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},165]
[164,"木质门带套","1.成品套装单开门，尺寸：850*2070\n2.门五金另计","樘",2,"成品套装门",{"v":0,"d":"0.00"},null,"成品套装单开门\n尺寸：850*2070","樘",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},166]
[165,"卫生纸盒","1.不锈钢纸盒","个",8,"不锈钢纸盒",{"v":0,"d":"0.00"},null,"不锈钢纸盒","个",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},167]
[166,"镜面玻璃","1.MR-01银镜玻璃。\n2.带框","m2",1.36,"成品银镜",{"v":0,"d":"0.00"},null,"MR-01银镜玻璃","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},168]
[167,"成品隔断","1.卫生间蹲坑WD-01木饰面成品隔断间。\n2.含五金。","间",8,"成品隔断",{"v":0,"d":"0.00"},null,"WD-01木饰面成品隔断间","间",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},169]
[168,"成品隔断","1.卫生间WD-01木饰面成品小便斗隔断。","套",2,"小便斗隔断",{"v":0,"d":"0.00"},null,"小便斗隔断","套",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},170]
[169,"3.2.5配菜间、更衣室",{"$nulls":13},{"v":0,"d":"0.00"}]
[170,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",2.5,"石材门槛石",{"$f":"H176+M176+N176+O176","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,171]
[171,"块料楼地面","1.CT-01白色地砖300*300水泥砂浆粘贴。","m2",41.73,"地砖",{"$f":"H177+N177+O177","v":{"v":0,"d":"0.00"}},null,"CT-01白色地砖\n规格300*300","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖主材甲供",null,null,172]
[172,"块料楼地面","1.CT-02灰色地砖300*300水泥砂浆粘贴。","m2",24.59,"地砖",{"$f":"H178+N178+O178","v":{"v":0,"d":"0.00"}},null,"CT-02灰色地砖\n规格300*300","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖主材甲供",null,null,173]
[173,"块料踢脚线","1.CT-01白色地砖踢脚线水泥砂浆粘贴。","m",24.71,"地砖踢脚线",{"$f":"H179+N179+O179","v":{"v":0,"d":"0.00"}},null,"CT-01白色地砖踢脚","m",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖踢脚线甲供",null,null,174]
[174,"块料踢脚线","1.CT-02灰色地砖踢脚线水泥砂浆粘贴。","m",23.52,"地砖踢脚线",{"$f":"H180+N180+O180","v":{"v":0,"d":"0.00"}},null,"CT-02灰色地砖踢脚","m",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖踢脚线甲供",null,null,175]
[175,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.铝合金扣板轻钢龙骨。\n3.MT-04白色铝扣板吊顶。","m2",66.32,"铝扣板",{"$f":"H181+M181+N181+O181","v":{"v":0,"d":"0.00"}},null,"MT-04白色铝扣板","m2",null,null,{"$f":"L181*K181","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},176]
[176,"石材窗台板","1.石材窗台板专用粘接剂安装。\n2.规格暂定120*40mm，倒角。","m2",0.8,"石材窗台板",{"$f":"H182+M182+N182+O182","v":{"v":0,"d":"0.00"}},null,"石材窗台板\n规格暂定120*40mm","m2",null,350,{"$f":"L182*K182","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"石材窗台板甲控乙供，主材价暂定，按质定价",null,null,178]
[177,"木质门带套","1.成品套装双开门，尺寸：1500*2100\n2.门五金另计","樘",3,"成品套装门",{"$f":"H183+M183+N183+O183","v":{"v":0,"d":"0.00"}},null,"成品套装双开门\n尺寸：1500*2100","樘",null,null,{"$f":"L183*K183","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},179]
[178,"木质门带套","1.成品套装单开门，尺寸：850*2070\n2.门五金另计","樘",2,"成品套装门",{"$f":"H184+M184+N184+O184","v":{"v":0,"d":"0.00"}},null,"成品套装单开门\n尺寸：850*2070","樘",null,null,{"$f":"L184*K184","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},180]
[179,"3.3办公室",{"$nulls":13},{"v":0,"d":"0.00"}]
[180,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",0.36,"石材门槛石",{"$f":"H186+M186+N186+O186","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,181]
[181,"块料楼地面","1.CT-02灰色地砖600*600水泥砂浆粘贴。","m2",56.09,"地砖",{"$f":"H187+N187+O187","v":{"v":0,"d":"0.00"}},null,"CT-02灰色\n地砖规格600*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖主材甲供",null,null,182]
[182,"块料踢脚线","1.CT-02灰色地砖踢脚线水泥砂浆粘贴。","m",48.51,"地砖踢脚线",{"$f":"H188+N188+O188","v":{"v":0,"d":"0.00"}},null,"CT-02灰色地砖踢脚","m",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖踢脚线甲供",null,null,183]
[183,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.双层9.5mm纸面石膏板。\n4.自粘胶带、腻子、乳胶漆另计。","m2",56.09,"纸面石膏板",{"$f":"H189+M189+N189+O189","v":{"v":0,"d":"0.00"}},null,"纸面石膏板9.5mm厚","m2",null,null,{"$f":"L189*K189","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},184]
[184,"开孔（打洞）","1.石膏板开灯孔。","个",12,null,{"$f":"H190+M190+N190+O190","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},185]
[185,"送风口、回风口","1.木基层风口基层。\n2.木基层防火涂料。\n3.成品风口其他单位施工","个",2,null,{"$f":"H191+M191+N191+O191","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},186]
[186,"石材窗台板","1.石材窗台板专用粘接剂安装。\n2.规格暂定120*40mm，倒角。","m2",1.6,"石材窗台板",{"$f":"H192+M192+N192+O192","v":{"v":0,"d":"0.00"}},null,"石材窗台板\n规格暂定120*40mm","m2",null,350,{"$f":"L192*K192","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"石材窗台板甲控乙供，主材价暂定，按质定价",null,null,188]
[187,"金属扶手、栏杆、栏板","1.楼梯栏杆扶手。\n2.做法暂定。","m",50.3,"栏杆扶手",{"$f":"M193","v":{"v":400,"d":"400.00"}},null,"栏杆扶手（含安装）","m",1,400,{"$f":"L193*K193","v":{"v":400,"d":"400.00"}},null,null,{"v":20120,"d":"20120.00"},"栏杆扶手甲控乙供，单价暂定，按质定价",null,null,189]
[188,"3.4楼梯间",{"$nulls":13},{"v":0,"d":"0.00"}]
[189,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",1.5,"石材门槛石",{"$f":"H195+M195+N195+O195","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,190]
[190,"块料楼地面","1.CT-02灰色地砖600*600水泥砂浆粘贴。","m2",63.31,"地砖",{"$f":"H196+N196+O196","v":{"v":0,"d":"0.00"}},null,"CT-02灰色\n地砖规格600*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖主材甲供",null,null,191]
[191,"块料台阶面","1.CT-02灰色地砖600*600水泥砂浆粘贴。\n2.嵌三道金属防滑条。","m2",10.84,"地砖",{"$f":"H197+N197+O197","v":{"v":0,"d":"0.00"}},null,"CT-02灰色\n地砖规格600*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖主材甲供",null,null,192]
[192,"块料踢脚线","1.CT-02灰色地砖踢脚线水泥砂浆粘贴。\n2.水平段。","m",56.92,"地砖踢脚线",{"$f":"H198+N198+O198","v":{"v":0,"d":"0.00"}},null,"CT-02灰色地砖踢脚","m",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖踢脚线甲供",null,null,193]
[193,"块料踢脚线","1.CT-02灰色地砖踢脚线水泥砂浆粘贴。\n2.踏步段，含三角板。","m",56.92,"地砖踢脚线",{"$f":"H199+N199+O199","v":{"v":0,"d":"0.00"}},null,"CT-02灰色地砖踢脚","m",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖踢脚线甲供",null,null,194]
[194,"金属扶手、栏杆、栏板","1.楼梯栏杆扶手。\n2.做法暂定。","m",24.6,"栏杆扶手",{"$f":"M200","v":{"v":400,"d":"400.00"}},null,"栏杆扶手（含安装）","m",1,400,{"$f":"L200*K200","v":{"v":400,"d":"400.00"}},null,null,{"v":9840,"d":"9840.00"},"栏杆扶手甲控乙供，单价暂定，按质定价",null,null,195]
[195,"石材窗台板","1.石材窗台板专用粘接剂安装。\n2.规格暂定120*40mm，倒角。","m2",2.4,"石材窗台板",{"$f":"H201+M201+N201+O201","v":{"v":0,"d":"0.00"}},null,"石材窗台板\n规格暂定120*40mm","m2",null,350,{"$f":"L201*K201","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"石材窗台板甲控乙供，主材价暂定，按质定价",null,null,198]
[196,"4办公、管理区",{"$nulls":13},{"$f":"G202*E202","v":{"v":0,"d":"0.00"}}]
[197,"4.1安防大厅",{"$nulls":13},{"v":0,"d":"0.00"}]
[198,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",0.72,"石材门槛石",{"$f":"H204+M204+N204+O204","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,199]
[199,"块料楼地面","1.CT-04灰色地砖800*800水泥砂浆粘贴。","m2",116.63,"地砖",{"$f":"H205+N205+O205","v":{"v":0,"d":"0.00"}},null,"CT-04灰色地砖\n规格800*800","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖主材甲供",null,null,200]
[200,"块料踢脚线","1.CT-02灰色地砖踢脚线水泥砂浆粘贴。","m",40.02,"地砖踢脚线",{"$f":"H206+N206+O206","v":{"v":0,"d":"0.00"}},null,"CT-02灰色地砖踢脚","m",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖踢脚线甲供",null,null,201]
[201,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.铝合金扣板轻钢龙骨。\n3.MT-04白色铝扣板吊顶。","m2",116.63,"铝扣板",{"$f":"H207+M207+N207+O207","v":{"v":0,"d":"0.00"}},null,"MT-04白色铝扣板","m2",null,null,{"$f":"L207*K207","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},202]
[202,"石材窗台板","1.石材窗台板专用粘接剂安装。\n2.规格暂定120*40mm，倒角。","m2",1.6,"石材窗台板",{"$f":"H208+M208+N208+O208","v":{"v":0,"d":"0.00"}},null,"石材窗台板\n规格暂定120*40mm","m2",null,350,{"$f":"L208*K208","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"石材窗台板甲控乙供，主材价暂定，按质定价",null,null,204]
[203,"4.2电信机房",{"$nulls":13},{"v":0,"d":"0.00"}]
[204,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",0.36,"石材门槛石",{"$f":"H210+M210+N210+O210","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,205]
[205,"竹、木（复合）地板","1.CT-02防静电地板（含骨架）600*600。","m2",82.65,"防静电地板",{"$f":"H211+M211+N211+O211","v":{"v":0,"d":"0.00"}},null,"CT-02防静电地板（含骨架）\n规格600*600","m2",null,null,{"$f":"L211*K211","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},206]
[206,"木质踢脚线","1.WD-02木地板踢脚线","m",36.38,"木地板踢脚线",{"$f":"H212+M212+N212+O212","v":{"v":0,"d":"0.00"}},null,"WD-02木地板踢脚线","m",null,null,{"$f":"L212*K212","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},207]
[207,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.铝合金扣板轻钢龙骨。\n3.MT-04白色铝扣板吊顶。","m2",82.65,"铝扣板",{"$f":"H213+M213+N213+O213","v":{"v":0,"d":"0.00"}},null,"MT-04白色铝扣板","m2",null,null,{"$f":"L213*K213","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},208]
[208,"4.2办公室",{"$nulls":13},{"v":0,"d":"0.00"}]
[209,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",0.72,"石材门槛石",{"$f":"H215+M215+N215+O215","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,210]
[210,"块料楼地面","1.CT-04灰色地砖800*800水泥砂浆粘贴。","m2",132.89,"地砖",{"$f":"H216+N216+O216","v":{"v":0,"d":"0.00"}},null,"CT-04灰色地砖\n规格800*800","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖主材甲供",null,null,211]
[211,"块料踢脚线","1.CT-02灰色地砖踢脚线水泥砂浆粘贴。","m",49.87,"地砖踢脚线",{"$f":"H217+N217+O217","v":{"v":0,"d":"0.00"}},null,"CT-02灰色地砖踢脚","m",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖踢脚线甲供",null,null,212]
[212,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.铝合金扣板轻钢龙骨。\n3.MT-04白色铝扣板吊顶。","m2",132.89,"铝扣板",{"$f":"H218+M218+N218+O218","v":{"v":0,"d":"0.00"}},null,"MT-04白色铝扣板","m2",null,null,{"$f":"L218*K218","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},213]
[213,"4.4医疗室、消防控制室、广播室",{"$nulls":13},{"v":0,"d":"0.00"}]
[214,"石材门槛石","1.ST-01石材门槛石水泥砂浆粘贴。","m2",0.96,"石材门槛石",{"$f":"H220+M220+N220+O220","v":{"v":0,"d":"0.00"}},null,"ST-01石材","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"石材甲供",null,null,215]
[215,"块料楼地面","1.CT-02灰色地砖600*600水泥砂浆粘贴。","m2",94.08,"地砖",{"$f":"H221+N221+O221","v":{"v":0,"d":"0.00"}},null,"CT-02灰色\n地砖规格600*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖主材甲供",null,null,216]
[216,"块料踢脚线","1.CT-02灰色地砖踢脚线水泥砂浆粘贴。","m",60.21,"地砖踢脚线",{"$f":"H222+N222+O222","v":{"v":0,"d":"0.00"}},null,"CT-02灰色地砖踢脚","m",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖踢脚线甲供",null,null,217]
[217,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.铝合金扣板轻钢龙骨。\n3.MT-04白色铝扣板吊顶。","m2",94.08,"铝扣板",{"$f":"H223+M223+N223+O223","v":{"v":0,"d":"0.00"}},null,"MT-04白色铝扣板","m2",null,null,{"$f":"L223*K223","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},218]
[218,"石材窗台板","1.石材窗台板专用粘接剂安装。\n2.规格暂定120*40mm，倒角。","m2",0.72,"石材窗台板",{"$f":"H224+M224+N224+O224","v":{"v":0,"d":"0.00"}},null,"石材窗台板\n规格暂定120*40mm","m2",null,350,{"$f":"L224*K224","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"石材窗台板甲控乙供，主材价暂定，按质定价",null,null,220]
[219,"5.基础施工工项",{"$nulls":13},{"v":0,"d":"0.00"}]
[220,"涂膜防水","1.JS涂抹防水两遍。\n2.综合墙地面","m2",{"$f":"58.76+12.42+83.32+6.24+114+56.8+47.05","v":378.59},"防水涂料",{"$f":"H226+M226+N226+O226","v":{"v":0,"d":"0.00"}},null,"JS","m2",null,null,{"$f":"L226*K226","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},1]
[221,"砌砖墙","1.水泥砖水泥砂浆砌120mm墙","m3",40,"水泥砖",{"$f":"H227+M227+N227+O227","v":{"v":0,"d":"0.00"}},null,"水泥砖","m3",null,null,{"$f":"L227*K227","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},2]
[222,"砌砖墙","1.水泥砖水泥砂浆砌240mm墙","m3",60,"水泥砖",{"$f":"H228+M228+N228+O228","v":{"v":0,"d":"0.00"}},null,"水泥砖","m3",null,null,{"$f":"L228*K228","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},3]
[223,"零星砌体","1.水泥砖水泥砂浆砌蹲坑等零星砌体","m3",20,"水泥砖",{"v":0,"d":"0.00"},null,"水泥砖","m3",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},4]
[224,"水泥砂浆抹灰","1.墙面水泥砂浆抹灰找平","m2",200,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},5]
[225,"水泥砂浆找平层","1.20mm水泥砂浆找平","m2",2713.5,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},6]
[226,"镀锌方钢龙骨","1.预埋铁件，镀锌方钢龙骨\n2.焊点防锈处理","t",{"$f":"1.95+0.641+0.0989+0.9889+0.2909+0.2909+0.1816+0.02474+0.4199+1.028+1.543+0.2+0.3+0.0613+1.0419","v":{"v":9.06104,"d":"9.061"}},"钢材",{"v":0,"d":"0.00"},null,"镀锌方钢","t",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},7]
[226,"镀锌型钢转换层","1.预埋铁件，镀锌型钢转换层\n2.焊点防锈处理","t",{"v":3,"d":"3.000"},"钢材",{"v":0,"d":"0.00"},null,"镀锌方钢","t",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},7]
[227,"方木平面龙骨","1.方木龙骨30*40，间距300*300\n2.按完成面投影面计算","m2",{"$f":"47.4+98","v":{"v":145.4,"d":"145.400"}},"木方",{"v":0,"d":"0.00"},null,"木方30*40","m2\n（投影）",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},8]
[228,"方木框架龙骨","1.方木龙骨30*40，间距300*300\n2.框架进深400\n3.按完成面投影面计算","m2",{"$f":"47.4+62.5","v":{"v":109.9,"d":"109.900"}},"木方",{"v":0,"d":"0.00"},null,"木方30*40","m2\n（投影）",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},9]
[229,"细木工板封板","1.细木工板封板18mm\n2.综合墙面、顶面","m2",{"$f":"47.4+62.5+32+98+29+24.7+113.91+61.29+60.24","v":529.04},"细木工板",{"v":0,"d":"0.00"},null,"细木工板板18mm","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},10]
[230,"阻燃夹板封板","1.细木工板封板12mm\n2.综合墙面、顶面","m2",45,"阻燃夹板",{"v":0,"d":"0.00"},null,"阻燃夹板","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},11]
[231,"纸面石膏板封板","1.纸面石膏板9.5mm\n2.综合墙面、顶面","m2",32,"纸面石膏板",{"v":0,"d":"0.00"},null,"纸面石膏板9.5mm厚","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},12]
[232,"木饰面","1.成品WD-01木饰面安装","m2",{"$f":"9.15+62.5+98+24.7+113.91+61.29+60.24","v":429.79},"木饰面",{"v":0,"d":"0.00"},null,"WD-01木饰面","m2",null,320,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"WD-01木饰面甲控乙供，主材价暂定，按质定价",null,null,13]
[233,"自粘胶带密封","1.石膏板面自粘胶带密封，自攻钉防锈处理。","m2",{"$f":"48.2+52.06+10.06+67.98+17.1+4.6+41.6+33+10+34.93","v":319.53},null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},14]
[234,"基层批腻子腻子","1.腻子两遍\n2.综合墙、顶面及抹灰面、石膏板面","m2",{"$f":"104.5+48.2+50.06+10.06+67.98+17.1+4.6+31.6+32+123+41.6+122.8+40.95+33+10+34.93+120.34+56.4+26.53+79.57+644+400","v":2099.22},"腻子",{"v":0,"d":"0.00"},null,"腻子","m2",null,null,{"$f":"L241*K241","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},{"$nulls":3},15]
[235,"乳胶漆","1.两遍PT-01白色乳胶漆\n2.综合墙面、顶面","m2",{"$f":"104.5+48.2+17.1+31.6+32+123+122.8+40.95+33+10+120.34+56.4+26.53+79.57+644+400","v":1889.99},"乳胶漆",{"v":0,"d":"0.00"},null,"PT-01白色乳胶漆","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},16]
[236,"防潮乳胶漆","1.两遍PT-02白色防水防潮乳胶漆\n2.综合墙面、顶面","m2",{"$f":"50.06+10.06+67.98+4.6+41.6+34.93","v":209.23},"乳胶漆",{"v":0,"d":"0.00"},null,"PT-02白色防水防潮乳胶漆","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},17]
[237,"木龙骨防火涂料","1.木龙骨防火涂料2遍\n2.按完成面投影面计算","m2",253.5,"防火涂料",{"v":0,"d":"0.00"},null,"防火涂料","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},18]
[238,"细木工板防火涂料","1.细木工板防火涂料2遍\n2.按单面计算","m3",529.04,"防火涂料",{"v":0,"d":"0.00"},null,"防火涂料","m3",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},19]
[239,"门铰链","1.平开门铰链安装","套",{"$f":"6+6+3+3+9+18+6+12+6+3+6+9+6","v":93},"五金",{"v":0,"d":"0.00"},null,"平开门铰链","套",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},20]
[240,"门执手锁","1.平开门执手锁安装","套",{"$f":"1+1+1+1+3+3+2+4+2+1+2+3+2","v":26},"五金",{"v":0,"d":"0.00"},null,"平开门执手锁","套",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},21]
[241,"门吸","1.平开门门吸安装","套",{"$f":"2+2+1+1+3+6+4+4+4+1+2+6+2","v":38},"五金",{"v":0,"d":"0.00"},null,"平开门门吸","套",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},22]
[242,"门插销","1.平开门插销安装","套",{"$f":"1+1+3+1+2+3","v":11},"五金",{"v":0,"d":"0.00"},null,"平开门插销","套",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},23]
[243,"长拉手","1.包间门长拉手\n2.两副/套","套",3,"拉手",{"v":0,"d":"0.00"},null,"长拉手","套",null,1200,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"长拉手甲控乙供，主材价暂定，按质定价",null,null,24]
[244,"轻钢龙骨双面石膏板隔墙","1.75型轻钢龙骨\n2.隔音棉\n3.双面单层纸面石膏板9.5mm","m2",120,"纸面石膏板",{"v":0,"d":"0.00"},null,"纸面石膏板9.5mm厚","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},25]
[245,"石膏板封堵洞口","1.木基层\n2.单层纸面石膏板9.5mm","m2",60,"纸面石膏板",{"v":0,"d":"0.00"},null,"单层纸面石膏板9.5mm","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},26]
[246,"砌体封堵洞口","1.水泥砖水泥砂浆封堵","m2",20,"水泥砖",{"v":0,"d":"0.00"},null,"水泥砖","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},27]
[247,"石材地面抛光","1.石材面做缝、修补、抛光","m2",1828,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"$nulls":3},28]
[248,"小计",{"$nulls":13},{"$f":"SUM(P7:P254)","v":{"v":29960,"d":"29960.00"}}]
[249,"计费明细","管理费","项",{"v":0.04,"d":"4%"},{"$nulls":10},{"$f":"P255*E256","v":{"v":1198.4,"d":"1198.40"}}]
[250,null,"利润","项",{"v":0.1,"d":"10%"},{"$nulls":10},{"$f":"P255*E257","v":{"v":2996,"d":"2996.00"}}]
[251,null,"税金","项",{"v":0.09,"d":"9%"},{"$nulls":10},{"$f":"(P257+P256+P255)*E258","v":{"v":3073.896,"d":"3073.90"}}]
[252,"工程总造价",{"$nulls":13},{"$f":"P258+P257+P256+P255","v":{"v":37228.296,"d":"37228.30"}}]
["1、综合单价为包含人工费（包括人员加班工资、差旅及窝工费）、材料费、机械费、风险的包工包料价格，包含深化设计、监理资料及竣工图绘制费用，包括水电、卸货、材料保管、二次搬运、上楼、各种保险、加班、临时设施、赶工措施、已完工项目成品保护措施、夜间照明、安全文明施工等费用，施工人员的食宿费、劳保费用、办公费、生活生产水电费、保险费也包含在报价里。其中：主材费单价包含主要材料费、运输费、运输损耗费、施工损耗费。施工单价包含人工费、机械费及除主要材料费以外辅材及其他所有费用。"]
["2、报价税率按9%考虑，提供9%税率的增值税专用发票。"]
["3、甲控乙供材料按提供的单价暂定，投标时价格不可调整，施工过程中投标人送样，招标人按质定价。"]
[null,"投标单位（公章）："]
[null,"授权委托人："]
[null,"日    期：     2020   年    月     日"]

{"sheet":"游客中心-安装","index":2,"n_rows":119,"n_cols":17,"rows_kept":119,"merged":[[0,0,0,16],[1,0,1,16],[2,0,5,0],[2,1,5,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6],[2,7,2,14],[2,15,5,15],[2,16,5,16],[3,7,5,7],[3,8,3,13],[4,8,4,12],[4,14,5,14],[113,0,113,16],[114,0,114,17],[115,0,115,17]]}
["安装工程量报价清单"]
["工程名称：第四届中国绿博会游客服务中心装饰装修专业分包工程"]
["序号","分项工程名称","项目特征","单位","数量","主材名称","综合单价","其        中：",{"$nulls":7},"合价","备注"]
[{"$nulls":7},"人工费","材    料    费"]
[{"$nulls":8},"主材费",{"$nulls":5},"机械费"]
[{"$nulls":8},"名称及规格","单位","单位耗量","单价","单位主材费合价","辅材"]
[1,"电气工程"]
[2,"配电箱","1.名称：消防柜配电箱4-1ATXK\n2.规格：15kw,12回路，ATS-40A/4P PC级，详见图纸\n3.安装方式：挂墙明装","台",1,"配电箱",{"$f":"H8+M8+N8+O8","v":0},null,"配电箱","套",null,"/",0,null,null,{"$f":"G8*E8","v":{"v":0,"d":"0.00"}},"配电箱甲供"]
[3,"配电箱","1.名称：架空层配电箱4-1ALz5\n2.规格：10kw,9回路，详见图纸\n3.安装方式：挂墙明装","台",1,"配电箱",{"$f":"H9+M9+N9+O9","v":0},null,"配电箱","套",null,"/",0,null,null,{"$f":"G9*E9","v":{"v":0,"d":"0.00"}},"配电箱甲供"]
[4,"配电箱","1.名称：广播室配电箱4-1ALgb\n2.规格：10kw,9回路，ATS-40A/4P CB级，详见图纸\n3.安装方式：挂墙明装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[5,"配电箱","1.名称：办公医疗配电箱4-1ALbg\n2.规格：20kw,11回路，详见图纸\n3.安装方式：嵌墙暗装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[6,"配电箱","1.名称：医疗照明配电箱4-1ALyl\n2.规格：6kw,6回路，详见图纸\n3.安装方式：嵌墙暗装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[7,"配电箱","1.名称：餐厅照明总配电箱4-1ALz4\n2.规格：50KW,22回路，ATS-160/4 PC级,详见图纸\n3.安装方式：落地安装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[8,"配电箱","1.名称：餐厅照明配电箱4-2AL1\n2.规格：30kw,22回路，详见图纸\n3.安装方式：挂墙明装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[9,"配电箱","1.名称：食堂照明配电箱4-1AL1\n2.规格：4kw,7回路，详见图纸\n3.安装方式：嵌墙暗装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[10,"配电箱","1.名称：餐厅保障负荷总箱4-1APZ、4-1APZE\n2.规格：70kw,3回路，详见图纸\n3.安装方式：嵌墙暗装","台",2,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[11,"配电箱","1.名称：餐厅公共照明配电箱4-2ATgg3\n2.规格：10KW，12回路，ATS-63/4 PC级，详见图纸\n3.安装方式：挂墙明装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[12,"配电箱","1.名称：厨房配电箱4-2ATcf\n2.规格：30KW，7回路，ATS-80/4 CB级，详见图纸\n3.安装方式：挂墙明装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[13,"配电箱","1.名称：电梯配电箱4-2ATdt\n2.规格：30KW,7回路，ATS-160/4 PC级，详见图纸\n3.安装方式：挂墙明装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[14,"配电箱","1.名称：室外展厅配电箱4-1ALzl\n2.规格：70KW，ATS-160/4 CB级，详见图纸\n3.安装方式：落地安装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[15,"配电箱","1.名称：室外展厅配电箱4-1APzl\n2.规格：140KW，ATS-250/4 CB级，详见图纸\n3.安装方式：落地安装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[16,"配电箱","1.名称：半开放多媒体厅兼会议室配电箱4-1AL3\n2.规格：20KW，ATS-63/4 CB级，详见图纸\n3.安装方式：落地安装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[17,"配电箱","1.名称：中央空调室外机组配电箱4-1APkt1\n2.规格：70.65KW,5回路，详见图纸\n3.安装方式：落地安装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[18,"配电箱","1.名称：中央空调室外机组配电箱4-1APkt2\n2.规格：36.02KW,3回路，详见图纸\n3.安装方式：落地安装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[19,"配电箱","1.名称：商店照明配电箱4-1ALz2\n2.规格：32KW,18回路，详见图纸\n3.安装方式：挂墙明装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[20,"配电箱","1.名称：电信机房配电箱4-1ATrd\n2.规格：50KW,5回路，ATS-160/4 CB级，详见图纸\n3.安装方式：落地靠墙","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[21,"配电箱","1.名称：应急照明总配电箱4-1ALeZ、4-1ALeZE\n2.规格：10KW,5回路，详见图纸\n3.安装方式：挂墙明装","台",2,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[22,"配电箱","1.名称：应急照明双电源配电箱4-1ALe1\n2.规格：2KW,3回路，ATS-32/4 PC级，详见图纸\n3.安装方式：挂墙明装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[23,"配电箱","1.名称：应急照明双电源配电箱4-1ALe2\n2.规格：2KW,3回路，ATS-32/4 PC级，详见图纸\n3.安装方式：挂墙明装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[24,"配电箱","1.名称：应急照明双电源配电箱4-1ALe3\n2.规格：2KW,5回路，ATS-32/4 PC级，详见图纸\n3.安装方式：挂墙明装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[25,"配电箱","1.名称：应急照明双电源配电箱4-1ALe4\n2.规格：2KW,3回路，ATS-32/4 PC级，详见图纸。\n3.安装方式：挂墙明装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[26,"配电箱","1.名称：安防大厅配电箱4-1ATaf\n2.规格：50KW,5回路，ATS-160/4P PC级，详见图纸\n3.安装方式：落地靠墙","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[27,"配电箱","1.名称：大厅照明配电箱4-1ALz1\n2.规格：50KW,35回路，ATS-160/4P CB级，详见图纸\n3.安装方式：落地靠墙","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[28,"配电箱","1.名称：服务台配电箱4-1ALfw1\n2.规格：6KW,6回路，详见图纸\n3.安装方式：挂墙明装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[29,"配电箱","1.名称：ATM机配电箱4-1ALatm\n2.规格：6KW,6回路，详见图纸\n3.安装方式：挂墙明装","台",1,"配电箱",0,null,"配电箱","套",null,"/",0,null,null,{"v":0,"d":"0.00"},"配电箱甲供"]
[30,"凿（压)槽","1.名称:砖墙开槽\n2.填充(恢复)方式:水泥砂浆恢复","m",372.4,"/",0,null,"/","/",null,null,{"$f":"L36*K36","v":0},null,null,{"v":0,"d":"0.00"}]
[31,"配管","1.名称:硬塑料管（PVC）\n2.规格:PC20\n3.配置形式:砖、混凝土结构暗配","m",450,"PVC电线管",0,null,"PVC电线管20","m",null,null,{"$f":"L37*K37","v":0},null,null,{"v":0,"d":"0.00"}]
[32,"配管","1.名称:硬塑料管（PVC）\n2.规格:PC20\n3.配置形式:砖、混凝土结构明配","m",2250,"PVC电线管",0,null,"PVC电线管20","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[33,"配管","1.名称:硬塑料管（PVC）\n2.规格:PC25\n3.配置形式:砖、混凝土结构暗配","m",150,"PVC电线管",0,null,"PVC电线管25","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[34,"配管","1.名称:硬塑料管（PVC）\n2.规格:PC25\n3.配置形式:砖、混凝土结构明配","m",1350,"PVC电线管",0,null,"PVC电线管25","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[35,"配管","1.名称:硬塑料管（PVC）\n2.规格:PC32\n3.配置形式:砖、混凝土结构暗配","m",110,"PVC电线管",0,null,"PVC电线管32","m",null,null,0,null,null,{"$f":"G41*E41","v":{"v":0,"d":"0.00"}}]
[36,"配管","1.名称:硬塑料管（PVC）\n2.规格:PC32\n3.配置形式:砖、混凝土结构明配","m",450,"PVC电线管",0,null,"PVC电线管32","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[37,"配管","1.名称:紧定式镀锌钢导管\n2.规格:JDG20\n3.配置形式:砖、混凝土结构暗配","m",15,"紧定式镀锌钢导管",0,null,"紧定式镀锌钢导管20","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[38,"配管","1.名称:紧定式镀锌钢导管\n2.规格:JDG20\n3.配置形式:砖、混凝土结构明配","m",25,"紧定式镀锌钢导管",0,null,"紧定式镀锌钢导管20","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[39,"配管","1.名称:紧定式镀锌钢导管\n2.规格:JDG40\n3.配置形式:砖、混凝土结构暗配","m",35,"紧定式镀锌钢导管",0,null,"紧定式镀锌钢导管40","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[40,"配管","1.名称:紧定式镀锌钢导管\n2.规格:JDG40\n3.配置形式:砖、混凝土结构明配","m",72,"紧定式镀锌钢导管",0,null,"紧定式镀锌钢导管40","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[41,"配管","1.名称:紧定式镀锌钢导管\n2.规格:JDG50\n3.配置形式:砖、混凝土结构暗配","m",22,"紧定式镀锌钢导管",0,null,"紧定式镀锌钢导管50","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[42,"配管","1.名称:紧定式镀锌钢导管\n2.规格:JDG50\n3.配置形式:砖、混凝土结构明配","m",32,"紧定式镀锌钢导管",0,null,"紧定式镀锌钢导管50","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[43,"桥架","1.名称:钢制桥架\n2.规格:300*150","m",113.73,"桥架",{"$f":"H49+M49+N49+O49","v":0},null,"成品镀锌钢桥架300*150","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[44,"桥架","1.名称:钢制桥架\n2.规格:200*100","m",27.48,"桥架",0,null,"成品镀锌钢桥架200*100","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[45,"电力电缆","1.名称:铜芯电缆\n2.型号:WDZ-YJV-4*35+1*16\n3.敷设方式、部位:穿管","m",45,"铜芯电缆",0,null,"DZ-YJV-4*35+1*16\n3.敷设方式、","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[46,"电力电缆","1.名称:铜芯电缆\n2.型号:WDZ-BYJ-4*25+1*16\n3.敷设方式、部位:穿管","m",65,"铜芯电缆",0,null,"WDZ-BYJ-4*25+1*16","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[47,"电力电缆","1.名称:铜芯电缆\n2.型号:WDZN-YJV-4*25\n3.敷设方式、部位:穿管","m",45,"铜芯电缆",0,null,"WDZN-YJV-4*25","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[48,"电力电缆","1.名称:铜芯电缆\n2.型号:WDZ-YJV-5*16\n3.敷设方式、部位:穿管","m",60,"铜芯电缆",0,null,"WDZ-YJV-5*16","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[49,"电力电缆","1.名称:铜芯电缆\n2.型号:WDZ-YJV-5*10\n3.敷设方式、部位:穿管","m",48,"铜芯电缆",0,null,"WDZ-YJV-5*10","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[50,"电力电缆","1.名称:铜芯电缆\n2.型号:NG-A-5*6\n3.敷设方式、部位:穿管","m",120,"铜芯电缆",0,null,"NG-A-5*6","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[51,"配线","1.名称:铜芯电线\n2.型号:WDZ-BYJ-10","m",320,"铜芯电线",0,null,"WDZ-BYJ-10","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[52,"配线","1.名称:铜芯电线\n2.型号:WDZ-BYJ-10","m",930,"铜芯电线",0,null,"WDZ-BYJ-10","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[53,"配线","1.名称:铜芯电线\n2.型号:WDZN-BYJ-6","m",1056,"铜芯电线",0,null,"WDZN-BYJ-6","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[54,"配线","1.名称:铜芯电线\n2.型号:WDZN-BYJ-6","m",495,"铜芯电线",0,null,"WDZN-BYJ-6","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[55,"配线","1.名称:铜芯电线\n2.型号:WDZ-BYJ-4","m",3630,"铜芯电线",0,null,"WDZ-BYJ-4","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[56,"配线","1.名称:铜芯电线\n2.型号:WDZN-BYJ-4","m",405,"铜芯电线",0,null,"DZN-BYJ-4","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[57,"配线","1.名称:铜芯电线\n2.型号:WDZ-BYJ-2.5","m",10575,"铜芯电线",0,null,"WDZ-BYJ-2.5","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[58,"配线","1.名称:铜芯电线\n2.型号:WDZN-BYJ-2.5","m",1356,"铜芯电线",0,null,"WDZN-BYJ-2.5","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[59,"电力电缆头","1.名称:成套型电缆头\n2.规格:电缆截面35mm2以下","个",65,"电缆头",0,null,"电缆头截面35mm2以下","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[60,"接线盒","1.名称:接线盒\n2.材质:镀锌","个",450,"镀锌接线盒",0,null,"镀锌接线盒","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[61,"普通灯具","1.名称:嵌入式筒灯\n2.类型:LED","套",101,"灯具",0,null,"嵌入式筒灯","套",null,null,0,null,null,{"v":0,"d":"0.00"}]
[62,"普通灯具","1.名称:嵌入式防潮筒灯\n2.类型:LED","套",56,"灯具",0,null,"嵌入式防潮筒灯","套",null,null,0,null,null,{"v":0,"d":"0.00"}]
[63,"普通灯具","1.名称:日光灯\n2.类型:LED","套",28,"灯具",0,null,"日光灯","套",null,null,0,null,null,{"v":0,"d":"0.00"}]
[64,"普通灯具","1.名称:格栅灯\n2.类型:LED","套",19,"灯具",0,null,"格栅灯","套",null,null,{"$f":"L70*K70","v":0},null,null,{"v":0,"d":"0.00"}]
[65,"普通灯具","1.名称:灯带\n2.类型:LED","m",125,"灯具",{"$f":"H71+M71+N71+O71","v":0},null,"LED灯带","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[66,"普通灯具","1.名称:应急照明筒灯\n2.类型:LED","套",35,"灯具",0,null,"应急照明筒灯","套",null,null,0,null,null,{"v":0,"d":"0.00"}]
[67,"普通灯具","1.名称:应急照明格栅灯\n2.类型:LED","套",5,"灯具",0,null,"应急照明格栅灯","套",null,null,0,null,null,{"$f":"G73*E73","v":{"v":0,"d":"0.00"}}]
[68,"普通灯具","1.名称:应急照明挂壁式\n2.类型:LED","套",25,"灯具",0,null,"应急照明挂壁式","套",null,null,0,null,null,{"v":0,"d":"0.00"}]
[69,"普通灯具","1.名称:应急出口指示灯\n2.类型:LED","套",125,"灯具",0,null,"应急出口指示灯","套",null,null,0,null,null,{"v":0,"d":"0.00"}]
[70,"小电器","1.名称:单联单控开关","个",35,"开关",0,null,"单联单控开关","个",null,null,{"$f":"H76*K76","v":0},null,null,{"v":0,"d":"0.00"}]
[71,"小电器","1.名称:双联单控开关","个",18,"开关",0,null,"双联单控开关","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[72,"小电器","1.名称:三联单控开关","个",15,"开关",0,null,"三联单控开关","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[73,"小电器","1.名称:单联双控开关","个",35,"开关",0,null,"单联双控开关","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[74,"小电器","1.名称:地面铜插座\n2.型号:15A","个",33,"插座",0,null,"地面铜插座","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[75,"小电器","1.名称:五孔普通插座\n2.型号:15A","个",58,"插座",0,null,"五孔普通插座","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[76,"小电器","1.名称:轴流排风扇","个",12,"轴流排风扇",0,null,"轴流排风扇","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[77,"网络、电视、电话",{"$nulls":4},0,{"$nulls":5},{"$f":"L83*K83","v":0},null,null,{"v":0,"d":"0.00"}]
[78,"光缆终端盒","1.弱电箱","个",3,"弱电箱",0,null,"弱电箱","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[79,"配线","1.名称:视频同轴电缆\n2.配线形式:穿管","m",325,"同轴电缆",0,null,"视频同轴电缆","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[80,"配线","1.名称:双绞线（6芯）\n2.配线形式:穿管","m",898,"双绞线",0,null,"双绞线（6芯）","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[81,"小电器","1.名称:有线电视插座\n2.安装方式:墙面安装","个",35,"插座",0,null,"有线电视插座","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[82,"小电器","1.名称:网络插座单口\n2.安装方式:墙面安装","个",5,"插座",0,null,"网络插座单口","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[83,"小电器","1.名称:网络插座单口\n2.安装方式:地面安装","个",5,"插座",0,null,"网络插座单口","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[84,"给排水、洁具安装工程",{"$nulls":10},0,null,null,{"v":0,"d":"0.00"}]
[85,"塑料管","1.材质、规格:PPR管DN20\n2.连接形式:热熔\n3.压力试验及吹、洗设计要求:符合规范及设计要求","m",320,"PPR管",0,null,"PPR管DN20","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[86,"塑料管","1.材质、规格:PPR管DN25\n2.连接形式:热熔\n3.压力试验及吹、洗设计要求:符合规范及设计要求","m",160,"PPR管",0,null,"PPR管DN25","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[87,"塑料管","1.材质、规格:PPR管DN32\n2.连接形式:热熔\n3.压力试验及吹、洗设计要求:符合规范及设计要求","m",120,"PPR管",0,null,"PPR管DN32","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[88,"塑料管","1.材质、规格:U-PVCP排水管Φ50\n2.连接形式:胶粘\n3.压力试验及吹、洗设计要求:符合规范及设计要求","m",120,"排水管",0,null,"U-PVCP排水管Φ50","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[89,"塑料管","1.材质、规格:U-PVCP排水管Φ75\n2.连接形式:胶粘\n3.压力试验及吹、洗设计要求:符合规范及设计要求","m",250,"排水管",0,null,"U-PVCP排水管Φ75","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[90,"塑料管","1.材质、规格:U-PVCP排水管Φ110\n2.连接形式:胶粘\n3.压力试验及吹、洗设计要求:符合规范及设计要求","m",420,"排水管",0,null,"U-PVCP排水管Φ110","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[91,"洗脸盆","1.材质:陶瓷\n2.规格、类型:成套立式洗手盆\n3.附件名称、数量:含下水","组",4,"立式洗手盆",0,null,"成套立式洗手盆","组",null,500,{"$f":"L97*K97","v":0},null,null,{"v":0,"d":"0.00"},"成套立式洗手盆甲控乙供，主材价暂定，按质定价"]
[92,"洗脸盆龙头","1.立式洗脸盆冷热水龙头","套",4,"冷热水龙头",0,null,"立式洗脸盆冷热水龙头","套",null,200,0,null,null,{"v":0,"d":"0.00"},"立式洗脸盆冷热水龙头甲控乙供，主材价暂定，按质定价"]
[93,"洗脸盆","1.材质:陶瓷\n2.规格、类型:嵌入式台上式洗脸盆\n3.附件名称、数量:含下水","组",12,"洗脸盆",0,null,"嵌入式台上式洗脸盆","组",null,550,0,null,null,{"v":0,"d":"0.00"},"嵌入式台上式洗脸盆甲控乙供，主材价暂定，按质定价"]
[94,"洗脸盆龙头","1.台上盆冷热水龙头","套",12,"台上盆冷热水龙头",0,null,"台上盆冷热水龙头","套",null,350,0,null,null,{"v":0,"d":"0.00"},"台上盆冷热水龙头甲控乙供，主材价暂定，按质定价"]
[95,"大便器","1.材质:陶瓷\n2.规格、类型:蹲便器","组",43,"蹲便器",0,null,"蹲便器","组",null,350,0,null,null,{"v":0,"d":"0.00"},"蹲便器甲控乙供，主材价暂定，按质定价"]
[96,"大便器脚踏阀","1.大便器脚踏阀","套",43,"大便器脚踏阀",0,null,"大便器脚踏阀","套",null,90,0,null,null,{"v":0,"d":"0.00"},"大便器脚踏阀甲控乙供，主材价暂定，按质定价"]
[97,"大便器","1.材质:陶瓷\n2.规格、类型:坐便器","组",2,"坐便器",0,null,"坐便器","组",null,2800,0,null,null,{"v":0,"d":"0.00"},"坐便器甲控乙供，主材价暂定，按质定价"]
[98,"大便器","1.材质:陶瓷\n2.规格、类型:坐便器（儿童）","组",1,"坐便器（儿童）",0,null,"坐便器（儿童）","组",null,1000,0,null,null,{"v":0,"d":"0.00"},"坐便器（儿童）甲控乙供，主材价暂定，按质定价"]
[99,"小便器","1.材质:陶瓷\n2.规格、类型:成品小便斗","组",13,"成品小便斗",0,null,"感应阀","组",null,680,0,null,null,{"v":0,"d":"0.00"},"感应阀甲控乙供，主材价暂定，按质定价"]
[100,"小便器感应阀","1.小便器感应阀","组",13,"小便器感应阀",0,null,"小便器感应阀","组",null,320,0,null,null,{"v":0,"d":"0.00"},"小便器感应阀甲控乙供，主材价暂定，按质定价"]
[101,"烘手器","1.型号、规格:成品烘手器","个",4,"成品烘手器",0,null,"成品烘手器","个",null,220,0,null,null,{"v":0,"d":"0.00"},"成品烘手器甲控乙供，主材价暂定，按质定价"]
[102,"洗涤盆","1.材质:陶瓷\n2.规格、类型:拖把池","组",4,"拖把池",0,null,"拖把池","组",null,450,0,null,null,{"v":0,"d":"0.00"},"拖把池甲控乙供，主材价暂定，按质定价"]
[103,"小计",{"$nulls":13},{"$f":"SUM(P3:P108)","v":{"v":0,"d":"0.00"}}]
[104,"计费明细","管理费","项",{"v":0.04,"d":"4%"},{"$nulls":10},{"$f":"P109*E110","v":{"v":0,"d":"0.00"}}]
[105,null,"利润","项",{"v":0.1,"d":"10%"},{"$nulls":10},{"$f":"P109*E111","v":{"v":0,"d":"0.00"}}]
[106,null,"税金","项",{"v":0.09,"d":"9%"},{"$nulls":10},{"$f":"(P111+P110+P109)*E112","v":{"v":0,"d":"0.00"}}]
[107,"工程总造价",{"$nulls":13},{"$f":"P112+P111+P110+P109","v":{"v":0,"d":"0.00"}}]
["1、综合单价为包含人工费（包括人员加班工资、差旅及窝工费）、材料费、机械费、风险的包工包料价格，包含深化设计、监理资料及竣工图绘制费用，包括水电、卸货、材料保管、二次搬运、上楼、各种保险、加班、临时设施、赶工措施、已完工项目成品保护措施、夜间照明、安全文明施工等费用，施工人员的食宿费、劳保费用、办公费、生活生产水电费、保险费也包含在报价里。其中：主材费单价包含主要材料费、运输费、运输损耗费、施工损耗费。施工单价包含人工费、机械费及除主要材料费以外辅材及其他所有费用。"]
["2、报价税率按9%考虑，提供9%税率的增值税专用发票。"]
["3、甲控乙供材料按提供的单价暂定，投标时价格不可调整，施工过程中投标人送样，招标人按质定价。"]
[null,"投标单位（公章）："]
[null,"授权委托人："]
[null,"日    期：     2020   年    月     日"]

{"sheet":"游客中心措施费","index":3,"n_rows":20,"n_cols":6,"rows_kept":20,"merged":[[0,0,0,5],[1,0,1,5],[14,1,14,5]]}
["措施费项目计价表"]
["工程名称：第四届中国绿博会游客服务中心装饰装修专业分包工程"]
["序号","项目名称","单位","数量"," 金额（元）","备注"]
[1,"安全文明施工费","项",1,null,"专项包干费"]
[2,"成品保护费","项",1,null,"专项包干费"]
[3,"开荒清洁、垃圾清运费","项",1,null,"专项包干费"]
[4,"临时设施费","项",1,null,"专项包干费"]
[5,"专业交叉施工增加费","项",1,null,"专项包干费"]
[6,"脚手架","项",1,null,"专项包干费"]
[7,"运杂费（二次搬运费等）","项",1,null,"专项包干费"]
[8,"其它配合费","项",1,null,"专项包干费"]
[10,"工地开放日保洁","项",1,null,"专项包干费"]
[null,"合价",null,null,{"$f":"(SUM(E4:E12))*0.7","v":{"v":0,"d":"0.00"}}]
[]
["说明：","措施费用各项应为含税包干报价，不因任何情况调整，措施费按实际发生计取，不发生不计取。。"]
[]
[]
[null,"投标单位（公章）："]
[null,"授权委托人："]
[null,"日    期：     2020   年    月     日"]

{"sheet":"花园餐厅装饰","index":4,"n_rows":139,"n_cols":17,"rows_kept":139,"merged":[[0,0,0,16],[1,0,1,16],[2,0,5,0],[2,1,5,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6],[2,7,2,14],[2,15,5,15],[2,16,5,16],[3,7,5,7],[3,8,3,13],[4,8,4,12],[4,14,5,14],[133,0,133,16],[134,0,134,16]]}
["装饰工程量报价清单"]
["工程名称：第四届中国绿博会花园餐厅装饰装修专业分包工程"]
["序号","分项工程名称","项目特征","单位","数量","主材名称","综合单价","其        中：",{"$nulls":7},"合价","备注"]
[{"$nulls":7},"人工费","材    料    费"]
[{"$nulls":8},"主材费",{"$nulls":5},"机械费"]
[{"$nulls":8},"名称及规格","单位","单位耗量","单价","单位主材费合价","辅材"]
[1,"1#、2#、3#入口"]
[2,"石材零星项目","1.地台深色石材水泥砂浆粘贴","m2",19.7,"石材",{"$f":"H8+N8+O8","v":{"v":0,"d":"0.00"}},null,"深色石材","m2",null,"/","/",null,null,{"$f":"G8*E8","v":{"v":0,"d":"0.00"}},"石材甲供"]
[3,"石材楼地面","1.灰色石材（火烧面）水泥砂浆铺贴。","m2",321.11,"石材",{"$f":"H9+N9+O9","v":{"v":0,"d":"0.00"}},null,"灰色石材（火烧面）","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供"]
[4,"石材楼地面","1.灰色石材（光面）水泥砂浆铺贴。","m2",32.54,"石材",{"$f":"H10+N10+O10","v":{"v":0,"d":"0.00"}},null,"灰色石材（火烧面）","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供"]
[5,"天棚喷刷涂料","1.原楼板、梁喷灰色涂料。","m2",308.36,"乳胶漆",{"$f":"H11+M11+N11+O11","v":{"v":0,"d":"0.00"}},null,"黑色乳胶漆","m2",null,null,{"$f":"L11*K11","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[6,"格栅吊顶","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.铝方通(表面木纹转印处理)@300mm，规格40*150。","m2",308.36,"铝方通",{"$f":"H12+M12+N12+O12","v":{"v":0,"d":"0.00"}},null,"铝方通(表面木纹转印处理)\n规格40*150。","m",null,15,{"$f":"L12*K12","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"铝方通(表面木纹转印处理)甲控乙供，主材价暂定，按质定价"]
[7,"墙面装饰板","1.白色铝单板3mm厚，拼接自然缝，内塞密封胶条\n2.铝单板专用挂件\n4.基层另计","m2",439.84,"铝板",{"$f":"H13+M13+N13+O13","v":{"v":0,"d":"0.00"}},null,"白色铝单板3mm厚","m2",null,240,{"$f":"L13*K13","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价"]
[8,"弧形铝板包圆柱","1.白色弧形铝单板3mm厚，拼接自然缝，内塞密封胶条\n2.铝单板专用挂件\n4.基层另计","m2",59.99,"铝板",{"$f":"H14+M14+N14+O14","v":{"v":0,"d":"0.00"}},null,"弧形白色铝单板3mm厚","m2",null,300,{"$f":"L14*K14","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价"]
[9,"餐厅01、02"]
[10,"石材门槛石","1.灰色石材门槛石水泥砂浆粘贴。","m2",4.8,"石材门槛石",{"$f":"H16+N16+O16","v":{"v":0,"d":"0.00"}},null,"灰色石材门槛石","m2",null,"/","/",null,null,{"$f":"G16*E16","v":{"v":0,"d":"0.00"}},"石材甲供"]
[11,"现浇水磨石楼地面","1.水磨石地面800*800mm","m2",1784.88,null,{"$f":"H17+M17+N17+O17","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[12,"竹、木（复合）地板","1.木地板。\n2.防潮垫。","m2",37.15,"木地板",{"v":0,"d":"0.00"},null,"木地板","m2",null,100,{"$f":"L18*K18","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"木地板甲控乙供，主材价暂定，按质定价"]
[13,"天棚喷刷涂料","1.原楼板、梁喷灰色涂料。","m2",1500,"乳胶漆",{"v":0,"d":"0.00"},null,"黑色乳胶漆","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[14,"格栅吊顶","1.Φ8吊筋，M8膨胀螺栓固定\n2.轻钢龙骨\n3.铝方通(表面木纹转印处理)@300mm，规格40*150\n4.详见图纸1F-P02、1#CT-PM-02/3、4","m2",1091.42,"铝方通",{"v":0,"d":"0.00"},null,"铝方通(表面木纹转印处理)\n规格40*150。","m",null,15,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"铝方通(表面木纹转印处理)甲控乙供，主材价暂定，按质定价"]
[15,"格栅吊顶","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨。\n3.铝方通(表面木纹转印处理)详见图纸，规格40*150。\n4.详见图纸1F-P01、1#CT-PM-01/2","m2",165.8,"铝方通",{"v":0,"d":"0.00"},null,"铝方通(表面木纹转印处理)\n规格40*150。","m",null,15,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"铝方通(表面木纹转印处理)甲控乙供，主材价暂定，按质定价"]
[16,"格栅吊顶","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨。\n3.铝方通(表面木纹转印处理)间距详见图纸，规格40*250。\n4.详见图纸1F-P01、1#CT-PM-01/1","m2",430,"铝方通",{"v":0,"d":"0.00"},null,"铝方通(表面木纹转印处理)\n规格40*150。","m",null,18,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"铝方通(表面木纹转印处理)甲控乙供，主材价暂定，按质定价"]
[17,"吊顶天棚","1.镀锌钢龙骨另计\n2.18厚防火板基层板、侧板\n3.纸面石膏板,自粘胶带密封，自攻钉防锈处理\n4.自粘胶带、腻子、乳胶漆另计。\n5.成品嵌入式条形灯具另计。\n6.详见图纸1#CT-PM-03/6","m2",30.58,null,{"v":0,"d":"0.00"},null,"防火板\n18mm厚","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[18,"铝板饰面装饰壁柜-柜体","1.尺寸：680*3650\n2.预埋铁件、镀锌方管另计\n3.18厚防火板柜体基层板\n4.铝板饰面柜体板,玫瑰金色喷涂另计\n5.内壁纸面石膏板、膏板外贴壁纸另计\n5.铝板饰面柜体隔板,玫瑰金色喷涂另计\n6.暗藏LED灯带，灯带另计\n7.详见图纸1#CT-PM-05\n8.投影面计算","m2",124.1,"防火板",{"v":0,"d":"0.00"},null,"防火板\n18mm厚","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[19,"铝板饰面装饰壁柜-铝板饰面柜体板","1.铝板饰面柜体板,玫瑰金色喷涂\n2.展开面积计算","m2",242,"铝板",{"v":0,"d":"0.00"},null,"铝板玫瑰金色喷涂","m2",null,240,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价"]
[20,"铝板饰面装饰壁柜-内壁纸面石膏板封板","1.纸面石膏板封板\n2.展开面积计算","m2",120,"纸面石膏板",{"v":0,"d":"0.00"},null,"纸面石膏板9.5mm","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[21,"铝板饰面装饰壁柜-内壁墙纸","1.墙纸专用墙纸胶粘贴\n2.展开面积计算","m2",120,"墙纸",{"v":0,"d":"0.00"},null,"墙纸","m2",null,30,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"墙纸甲控乙供，主材价暂定，按质定价"]
[22,"铝板饰面装饰壁柜-铝板饰面柜体隔板","1.镀锌方管龙骨。\n2.18厚防火板基层板\n4.铝板饰面柜体板,玫瑰金色喷涂\n5、暗藏灯带\n6.延长米计算","m",35,"铝板",{"v":0,"d":"0.00"},null,"铝板玫瑰金色喷涂","m2",null,240,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价"]
[23,"墙面装饰板","1.铝单板面层面层木纹色转印3mm厚\n2.铝单板专用挂件\n3.镀锌钢龙骨另计","m2",29.42,"铝板",{"v":0,"d":"0.00"},null,"铝单板木纹色转印3mm厚","m2",null,240,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价"]
[24,"人造绿植墙饰面基层","1.镀锌钢龙骨另计\n2.18厚防火板柜体基层板\n2.定制人造绿植墙饰面另计\n3.详见图纸1#-CT-PM-04","m2",171.44,"防火板",{"v":0,"d":"0.00"},null,"防火板\n18mm厚","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[25,"水泥板饰面墙面装饰板","1.水泥板装饰饰面\n2.镀锌钢龙骨另计\n3.18厚防火板柜体基层板另计\n4.详见图纸1#-CT-PM-04","m2",431.38,"水泥板",{"v":0,"d":"0.00"},null,"水泥板","m2",null,65,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"水泥板甲控乙供，主材价暂定，按质定价"]
[26,"挑高处梁饰面-基层","1.18厚防火板做梁基层，，暗藏灯带\n3.详见图纸1#CT-PM-05","m",168,"防火板",{"v":0,"d":"0.00"},null,"防火板\n18mm厚","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[27,"挑高处梁饰面-铝单板面层","1.铝单板面层面层木纹色转印3mm厚做梁\n2.详见图纸1#CT-PM-05","m2",84.21,"铝板",{"v":0,"d":"0.00"},null,"铝单板木纹色转印3mm厚","m2",null,240,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价"]
[28,"铝板圆柱包方柱","1.铝单板面层面层木纹色转印3mm厚包柱\n2.铝单板专用挂件\n3.镀锌钢龙骨另计\n4.玫瑰金色金属收边条40*20另计\n5.详见图纸1#CT-PM-05","m2",93.45,"铝板",{"v":0,"d":"0.00"},null,"铝单板木纹色转印3mm厚","m2",null,240,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价"]
[29,"弧形铝板包圆柱","1.白色弧形铝单板3mm厚，拼接自然缝，内塞密封胶条\n2.铝单板专用挂件\n4.基层另计","m2",148.16,"铝板",{"v":0,"d":"0.00"},null,"弧形白色铝单板3mm厚","m2",null,300,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价"]
[30,"金属装饰线","1.玫瑰金色金属收边条40*20","m",1057.41,"不锈钢线条",{"v":0,"d":"0.00"},null,"玫瑰金色金属收边条40*20","m",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[31,"装饰空心砖造型墙","1.装饰空心砖造型墙\n2.预埋铁件，上下固定\n3.详见图纸1#CT-PM-05","m2",205.2,"成品空心砖造型墙",{"v":0,"d":"0.00"},null,"成品空心砖造型墙","m2",null,450,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"成品空心砖造型墙甲控乙供，主材价暂定，按质定价"]
[32,"木质门带套","1.成品套装双开门，尺寸：1500*2100\n2.门五金另计","樘",4,"成品套装门",{"v":0,"d":"0.00"},null,"成品套装双开门\n尺寸：1500*2100","樘",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[33,"收银服务台","1.收银服务台制作安装，尺寸：3000*1500\n2.基层制作,暗藏灯带\n3.木饰面台面,\n4.深色石材饰面另计,铝板木纹转印饰面另计\n4.定制亚克力饰面灯\n5.自行深化，详见图纸1#CT-DY-01","个",2,"收银服务台",{"v":0,"d":"0.00"},null,"收银服务台3000*1500","个",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[34,"收银服务台-石材饰面","1.收银服务台深色石材饰面\n2.详见图纸1#CT-DY-01","m2",5.5,"石材",{"$f":"H40+N40+O40","v":{"v":0,"d":"0.00"}},null,"深色石材","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供"]
[35,"收银服务台-铝板饰面","1.收银服务台铝板木纹转印饰面饰面\n2.详见图纸1#CT-DY-01","m2",4.8,"铝板",{"$f":"H41+M41+N41+O41","v":{"v":0,"d":"0.00"}},null,"铝单板木纹色转印3mm厚","m2",null,240,{"$f":"L41*K41","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价"]
[36,"景观展示台","1.服务台制作安装，尺寸：7600*1500\n2.基层制作,暗藏灯带,\n3.深色石材饰面另计\n4.不含定制成品雕塑及成品人造植物等摆件\n5.自行深化，详见图纸1#CT-DY-01","个",2,"景观展示台",{"$f":"H42+M42+N42+O42","v":{"v":0,"d":"0.00"}},null,"景观展示台7600*1500","个",null,null,{"$f":"L42*K42","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[37,"景观展示台-石材饰面","1.景观展示台深色石材饰面\n2.详见图纸1#CT-DY-01","m2",10.5,"石材",{"$f":"H43+N43+O43","v":{"v":0,"d":"0.00"}},null,"深色石材","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供"]
[38,"餐厅03、04"]
[39,"石材门槛石","1.灰色石材门槛石水泥砂浆粘贴。","m2",3.6,"石材门槛石",{"$f":"H45+N45+O45","v":{"v":0,"d":"0.00"}},null,"灰色石材门槛石","m2",null,"/","/",null,null,{"$f":"G45*E45","v":{"v":0,"d":"0.00"}},"石材甲供"]
[40,"现浇水磨石楼地面","1.水磨石地面800*800mm","m2",832.63,null,{"$f":"H46+M46+N46+O46","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[41,"竹、木（复合）地板","1.木地板。\n2.防潮垫。","m2",88,"木地板",{"v":0,"d":"0.00"},null,"木地板","m2",null,100,{"$f":"L47*K47","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"木地板甲控乙供，主材价暂定，按质定价"]
[42,"灯带（槽）","1.地台木基层灯带","m",34.25,"防火板",{"v":0,"d":"0.00"},null,"防火板\n18mm厚","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[43,"天棚喷刷涂料","1.原楼板、梁喷灰色涂料。","m2",790.08,"乳胶漆",{"v":0,"d":"0.00"},null,"黑色乳胶漆","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[44,"格栅吊顶","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨。\n3.铝方通(表面木纹转印处理)间距详见图纸，规格40*250。\n4.详见图纸1F-P02、1#CT-PM-01/1","m2",790.08,"铝方通",{"v":0,"d":"0.00"},null,"铝方通(表面木纹转印处理)\n规格40*150。","m",null,18,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"铝方通(表面木纹转印处理)甲控乙供，主材价暂定，按质定价"]
[45,"铝板饰面装饰壁柜","1.尺寸：680*3650\n2.预埋铁件、镀锌方管另计\n3.18厚防火板柜体基层板\n4.铝板饰面柜体板,玫瑰金色喷涂另计\n5.内壁纸面石膏板、膏板外贴壁纸另计\n5.铝板饰面柜体隔板,玫瑰金色喷涂另计\n6.暗藏LED灯带，灯带另计\n7.详见图纸1#CT-PM-05\n8.投影面计算","m2",44.68,"防火板",{"v":0,"d":"0.00"},null,"防火板\n18mm厚","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[46,"铝板饰面装饰壁柜-铝板饰面柜体板","1.铝板饰面柜体板,玫瑰金色喷涂\n2.展开面积计算","m2",88.3,"铝板",{"v":0,"d":"0.00"},null,"铝板玫瑰金色喷涂","m2",null,240,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价"]
[47,"铝板饰面装饰壁柜-内壁纸面石膏板封板","1.纸面石膏板封板\n2.展开面积计算","m2",42,"纸面石膏板",{"v":0,"d":"0.00"},null,"纸面石膏板9.5mm","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[48,"铝板饰面装饰壁柜-内壁墙纸","1.墙纸专用墙纸胶粘贴\n2.展开面积计算","m2",42,"墙纸",{"v":0,"d":"0.00"},null,"墙纸","m2",null,30,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"墙纸甲控乙供，主材价暂定，按质定价"]
[49,"铝板饰面装饰壁柜-铝板饰面柜体隔板","1.镀锌方管龙骨。\n2.18厚防火板基层板\n4.铝板饰面柜体板,玫瑰金色喷涂\n5、暗藏灯带\n6.延长米计算","m",41,"铝板",{"v":0,"d":"0.00"},null,"铝板玫瑰金色喷涂","m2",null,240,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价"]
[50,"人造绿植墙饰面基层","1.镀锌钢龙骨另计\n2.18厚防火板柜体基层板\n2.定制人造绿植墙饰面另计\n3.详见图纸1#-CT-PM-04","m2",236,"防火板",{"v":0,"d":"0.00"},null,"防火板\n18mm厚","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[51,"铝板圆柱包方柱","1.铝单板面层面层木纹色转印3mm厚包柱\n2.铝单板专用挂件\n3.镀锌钢龙骨另计\n4.玫瑰金色金属收边条40*20另计\n5.详见图纸1#CT-PM-05","m2",12.85,"铝板",{"v":0,"d":"0.00"},null,"铝单板木纹色转印3mm厚","m2",null,240,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价"]
[52,"弧形铝板包圆柱","1.白色弧形铝单板3mm厚，拼接自然缝，内塞密封胶条\n2.铝单板专用挂件\n4.基层另计","m2",97,"铝板",{"v":0,"d":"0.00"},null,"弧形白色铝单板3mm厚","m2",null,300,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"铝板甲控乙供，主材价暂定，按质定价"]
[53,"块料墙面","1.凹凸条形砖饰面\n2.预镀锌钢龙骨另计\n3.不锈钢干挂件干挂","m2",133.52,"墙砖",{"v":0,"d":"0.00"},null,"凹凸条形墙砖","m2",null,100,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"凹凸条形墙砖甲控乙供，主材价暂定，按质定价"]
[54,"玻璃隔断","1.明档式后厨玻璃隔断\n2.钢化玻璃10mm厚，玫瑰金不锈钢框20*20\n3.玫瑰金不锈钢框60*80mm\n4.详见图纸DY-01","m2",24.92,"玻璃隔断",{"v":0,"d":"0.00"},null,"玻璃隔断，玫瑰金边框","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[55,"明档式后厨地柜","1.明档式后厨地柜\n2.预埋铁件,40*40镀锌钢骨架,木基层板柜体,暗藏灯带\n3.免漆柜体板,\n4.灰色石材台面另计\n5.详见图纸DY-01","m",17.8,"后厨地柜",{"v":0,"d":"0.00"},null,"后厨地柜","m",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[56,"明档式后厨地柜-灰色石材台面",null,"m2",2.5,"石材",{"$f":"H62+N62+O62","v":{"v":0,"d":"0.00"}},null,"灰色石材","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供"]
[57,"平面、箱式招牌","1.明档式后厨定制成品广告灯箱","m2",10.68,"成品灯箱",{"$f":"H63+M63+N63+O63","v":{"v":0,"d":"0.00"}},null,"成品灯箱","m2",null,null,{"$f":"L63*K63","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[58,"金属门窗套基层","1.明档式后厨窗口套\n2.预埋铁件,镀锌型钢骨架另计\n3.防火板基层,\n4.玫瑰金不锈钢饰面另计","m2",51.94,"防火板",{"$f":"H64+M64+N64+O64","v":{"v":0,"d":"0.00"}},null,"防火板\n18mm厚","m2",null,null,{"$f":"L64*K64","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[59,"金属门窗套-玫瑰金不锈钢饰面","1.玫瑰金不锈钢饰面\n2.计算方式，展开面积","m2",51.94,"玫瑰金不锈钢饰面",{"$f":"H65+M65+N65+O65","v":{"v":0,"d":"0.00"}},null,"玫瑰金不锈钢饰面1.0","m2",null,null,{"$f":"L65*K65","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[60,"木质门带套","1.成品套装双开门，尺寸：1500*2100\n2.门五金另计","樘",4,"成品套装门",{"$f":"H66+M66+N66+O66","v":{"v":0,"d":"0.00"}},null,"成品套装双开门\n尺寸：1500*2100","樘",null,null,{"$f":"L66*K66","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[61,"景观展示台","1.服务台制作安装，尺寸：7600*1500\n2.基层制作,暗藏灯带,\n3.深色石材饰面另计\n4.不含定制成品雕塑及成品人造植物等摆件\n5.自行深化，详见图纸1#CT-DY-01","个",2,"景观展示台",{"$f":"H67+M67+N67+O67","v":{"v":0,"d":"0.00"}},null,"景观展示台7600*1500","个",null,null,{"$f":"L67*K67","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[62,"景观展示台-石材饰面","1.景观展示台深色石材饰面\n2.详见图纸1#CT-DY-01","m2",10.5,"石材",{"$f":"H68+N68+O68","v":{"v":0,"d":"0.00"}},null,"深色石材","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"石材甲供"]
[63,"1#、2#卫生间4个"]
[64,"现浇水磨石楼地面","1.水磨石地面800*800mm","m2",28.17,null,{"$f":"H70+M70+N70+O70","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"$f":"G70*E70","v":{"v":0,"d":"0.00"}}]
[65,"块料楼地面","1.防滑地砖600*600水泥砂浆粘贴。","m2",36.91,"地砖",{"$f":"H71+N71+O71","v":{"v":0,"d":"0.00"}},null,"防滑地砖\n规格600*600","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖主材甲供"]
[66,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.双层防水9.5mm纸面石膏板。\n4.自粘胶带、腻子、乳胶漆另计。","m2",65.08,"纸面石膏板",{"$f":"H72+M72+N72+O72","v":{"v":0,"d":"0.00"}},null,"防水9.5mm纸面石膏板","m2",null,null,{"$f":"L72*K72","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[67,"灯带（槽）","1.Φ8吊筋，M8膨胀螺栓固定。\n2.阻燃夹板、双层防水9.5mm纸面石膏板。\n3.自粘胶带、腻子、乳胶漆另计。\n5.尺寸300+120+80。","m",40,"纸面石膏板",{"v":0,"d":"0.00"},null,"防水9.5mm纸面石膏板","m2",null,null,{"$f":"L73*K73","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[68,"开孔（打洞）","1.石膏板开灯孔。","个",60,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[69,"开孔（打洞）","1.石膏板开出风口孔。","个",24,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[70,"送风口、回风口","1.木基层风口基层。\n2.木基层防火涂料。\n3.成品风口。","个",24,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[71,"石材墙面","1.水泥砂浆粘贴。\n2.水磨石石材规格600*600","m2",245,"水磨石石材",{"v":0,"d":"0.00"},null,"水磨石石材规格600*600","m2",null,350,{"$f":"L77*K77","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"水磨石石材甲控乙供，主材价暂定，按质定价"]
[72,"块料墙面","1.墙面300*600灰色墙砖水泥砂浆粘贴。\n2.密封","m2",350,"墙砖",{"v":0,"d":"0.00"},null,"墙砖\n规格300*600","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"墙砖甲供"]
[73,"洗漱台","1.高度250mm,挡水板高度50mm。\n2.型钢骨架，水磨石石材台面。\n3.台盆开工、磨边，挡水条及阳角倒角、磨边。\n4.详见图纸","m2",9.8,"水磨石石材",{"v":0,"d":"0.00"},null,"水磨石石材","m2",null,350,{"$f":"L79*K79","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"},"水磨石石材石材甲控乙供，主材价暂定，按质定价"]
[74,"镜面玻璃","1.木工板基层、暗藏灯带、银镜玻璃\n2.玫瑰金不锈钢收边10mm宽","m2",3.5,"成品银镜",{"v":0,"d":"0.00"},null,"MR-01银镜玻璃","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[75,"成品隔断","1.卫生间蹲坑成品隔断间。\n2.含五金。","间",16,"成品隔断",{"v":0,"d":"0.00"},null,"木饰面成品隔断间","间",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[76,"成品隔断","1.卫生间成品小便斗隔断。","套",8,"小便斗隔断",{"v":0,"d":"0.00"},null,"小便斗隔断","套",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[77,"木质门带套","1.成品套装单开门，尺寸：1000*2100\n2.门五金另计","樘",14,"成品套装门",{"v":0,"d":"0.00"},null,"成品套装单开门\n尺寸：1000*2070","樘",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[78,"金属门窗套基层","1.防火板基层\n2.不锈钢门套另计","m2",4.8,"防火板",{"v":0,"d":"0.00"},null,"防火板\n18mm厚","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[79,"金属门窗套-不锈钢饰面","1.不锈钢门套","m2",4.8,"玫瑰金不锈钢饰面",{"v":0,"d":"0.00"},null,"玫瑰金不锈钢饰面1.0","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[80,"卫生纸盒","1.不锈钢纸盒","个",16,"不锈钢纸盒",{"v":0,"d":"0.00"},null,"不锈钢纸盒","个",null,null,{"v":0,"d":"0.00"},null,null,{"$f":"G86*'游客中心-装饰'!E64","v":{"v":0,"d":"0.00"}}]
[81,"卫生间扶手","1.坐便器残疾人扶手","副",4,"残疾人扶手",{"v":0,"d":"0.00"},null,"洗漱台残疾人扶手","套",null,null,{"v":0,"d":"0.00"},null,null,{"$f":"G87*E87","v":{"v":0,"d":"0.00"}}]
[82,"餐厅厨房、明档式厨房"]
[83,"石材门槛石","1.石材门槛石水泥砂浆粘贴。","m2",2.64,"石材门槛石",{"$f":"H89+N89+O89","v":{"v":0,"d":"0.00"}},null,"灰色石材门槛石","m2",null,"/","/",null,null,{"$f":"G89*E89","v":{"v":0,"d":"0.00"}},"石材甲供"]
[84,"块料楼地面","1.防滑地砖600*600水泥砂浆粘贴。","m2",416.9,"地砖",{"$f":"H90+N90+O90","v":{"v":0,"d":"0.00"}},null,"防滑地砖\n规格600*600","m2",null,"/","/",null,null,{"$f":"G90*E90","v":{"v":0,"d":"0.00"}},"地砖主材甲供"]
[85,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.铝合金扣板轻钢龙骨。\n3.600*600铝扣板吊顶。","m2",416.9,"铝扣板",{"$f":"H91+M91+N91+O91","v":{"v":0,"d":"0.00"}},null,"MT-04白色铝扣板","m2",null,null,{"$f":"L91*K91","v":{"v":0,"d":"0.00"}},null,null,{"$f":"G91*E91","v":{"v":0,"d":"0.00"}}]
[86,"块料墙面","1.300*600灰色墙砖水泥砂浆粘贴。\n2.密封","m2",697.79,"墙砖",{"$f":"H92+M92+N92+O92","v":{"v":0,"d":"0.00"}},null,"墙砖\n规格300*600","m2",null,"/",{"v":0,"d":"0.00"},null,null,{"$f":"G92*E92","v":{"v":0,"d":"0.00"}},"墙砖甲供"]
[87,"1#-4#楼梯间"]
[88,"石材门槛石","1.石材门槛石水泥砂浆粘贴。","m2",4.5,"石材门槛石",{"$f":"H94+N94+O94","v":{"v":0,"d":"0.00"}},null,"灰色石材门槛石","m2",null,"/","/",null,null,{"$f":"G94*E94","v":{"v":0,"d":"0.00"}},"石材甲供"]
[89,"现浇水磨石楼地面","1.水磨石地面台阶面","m2",268,null,{"$f":"H95+M95+N95+O95","v":{"v":0,"d":"0.00"}},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"$f":"G95*E95","v":{"v":0,"d":"0.00"}}]
[90,"金属扶手、栏杆、栏板","1.楼梯栏杆扶手。\n2.做法暂定。","m",135,"栏杆扶手",{"$f":"M96","v":{"v":400,"d":"400.00"}},null,"栏杆扶手（含安装）","m",1,400,{"$f":"L96*K96","v":{"v":400,"d":"400.00"}},"/","/",{"$f":"G96*E96","v":{"v":54000,"d":"54000.00"}},"栏杆扶手甲控乙供，单价暂定，按质定价"]
[91,"天棚喷刷涂料","1.两遍腻子。\n2.两遍PT-01白色乳胶漆。","m2",79.57,"乳胶漆",{"$f":"H97+M97+N97+O97","v":{"v":0,"d":"0.00"}},null,"黑色乳胶漆","m2",null,null,{"$f":"L97*K97","v":{"v":0,"d":"0.00"}},null,null,{"$f":"G97*E97","v":{"v":0,"d":"0.00"}}]
[92,"生活泵房、消控中心、配电间、储藏间"]
[93,"石材门槛石","1.灰色石材门槛石水泥砂浆粘贴。","m2",4.4,"石材门槛石",{"$f":"H99+N99+O99","v":{"v":0,"d":"0.00"}},null,"灰色石材门槛石","m2",null,"/","/",null,null,{"$f":"G99*E99","v":{"v":0,"d":"0.00"}},"石材甲供"]
[94,"块料楼地面","1.玻化地砖800*800水泥砂浆粘贴。","m2",281.87,"地砖",{"$f":"H100+N100+O100","v":{"v":0,"d":"0.00"}},null,"玻化地砖\n规格800*800","m2",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖主材甲供"]
[95,"块料踢脚线","1.地砖踢脚线水泥砂浆粘贴。","m",241,"地砖踢脚线",{"$f":"H101+N101+O101","v":{"v":0,"d":"0.00"}},null,"地砖踢脚线","m",null,"/","/",null,null,{"v":0,"d":"0.00"},"地砖踢脚线甲供"]
[96,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.双层防水9.5mm纸面石膏板。\n4.自粘胶带、腻子、乳胶漆另计。","m2",160.56,"纸面石膏板",{"$f":"H102+M102+N102+O102","v":{"v":0,"d":"0.00"}},null,"防水9.5mm纸面石膏板","m2",null,null,{"$f":"L102*K102","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[97,"吊顶天棚","1.Φ8吊筋，M8膨胀螺栓固定。\n2.轻钢主龙骨、副龙、连接件。\n3.双层9.5mm纸面石膏板。\n4.自粘胶带、腻子、乳胶漆另计。","m2",110.15,"纸面石膏板",{"$f":"H103+M103+N103+O103","v":{"v":0,"d":"0.00"}},null,"纸面石膏板9.5mm厚","m2",null,null,{"$f":"L103*K103","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[98,"5.基础施工工项",{"$nulls":13},{"v":0,"d":"0.00"}]
[99,"涂膜防水","1.JS涂抹防水两遍。\n2.综合墙地面","m2",874.41,"防水涂料",{"$f":"H105+M105+N105+O105","v":{"v":0,"d":"0.00"}},null,"JS","m2",null,null,{"$f":"L105*K105","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[100,"砌砖墙","1.水泥砖水泥砂浆砌120mm墙","m3",null,"水泥砖",{"v":0,"d":"0.00"},null,"水泥砖","m3",null,null,{"$f":"L106*K106","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[101,"砌砖墙","1.水泥砖水泥砂浆砌240mm墙","m3",null,"水泥砖",{"v":0,"d":"0.00"},null,"水泥砖","m3",null,null,{"$f":"L107*K107","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[102,"零星砌体","1.水泥砖水泥砂浆砌蹲坑等零星砌体","m3",11.6,"水泥砖",{"v":0,"d":"0.00"},null,"水泥砖","m3",null,null,{"$f":"L108*K108","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[103,"水泥砂浆抹灰","1.墙面水泥砂浆抹灰找平","m2",23.2,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[104,"水泥砂浆找平层","1.20mm水泥砂浆找平","m2",{"$f":"355+3794","v":4149},null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[105,"镀锌方钢龙骨","1.预埋铁件，镀锌方钢龙骨\n2.焊点防锈处理","t",{"v":15.32,"d":"15.320"},"钢材",{"v":0,"d":"0.00"},null,"镀锌方钢","t",null,null,{"$f":"L111*K111","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[106,"镀锌方钢龙骨（龙骨弧形折弯处理）","1.预埋铁件，镀锌方钢龙骨\n2.龙骨弧形折弯处理\n3.焊点防锈处理","t",{"v":3.44,"d":"3.440"},"钢材",{"v":0,"d":"0.00"},null,"镀锌方钢","t",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[107,"镀锌型钢转换层","1.预埋铁件，镀锌型钢转换层\n2.焊点防锈处理","t",{"v":4,"d":"4.000"},"钢材",{"v":0,"d":"0.00"},null,"镀锌方钢","t",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[108,"防火板封板","1.防火板18mm厚\n2.综合墙面、顶面","m2",431,"防火板",{"v":0,"d":"0.00"},null,"防火板\n18mm厚","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[109,"纸面石膏板封板","1.纸面石膏板9.5mm\n2.综合墙面、顶面","m2",120,"纸面石膏板",{"v":0,"d":"0.00"},null,"纸面石膏板9.5mm厚","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[110,"木饰面","1.成品木饰面安装","m2",45,"木饰面",{"v":0,"d":"0.00"},null,"木饰面","m2",null,320,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},"木饰面甲控乙供，主材价暂定，按质定价"]
[111,"自粘胶带密封","1.石膏板面自粘胶带密封，自攻钉防锈处理。","m2",220,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[112,"基层批腻子腻子","1.腻子两遍\n2.综合墙、顶面及抹灰面、石膏板面","m2",{"$f":"294.57+120","v":414.57},"腻子",{"v":0,"d":"0.00"},null,"腻子","m2",null,null,{"$f":"L118*K118","v":{"v":0,"d":"0.00"}},null,null,{"v":0,"d":"0.00"}]
[113,"乳胶漆","1.两遍PT-01白色乳胶漆\n2.综合墙面、顶面","m2",294.57,"乳胶漆",{"v":0,"d":"0.00"},null,"PT-01白色乳胶漆","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[114,"防潮乳胶漆","1.两遍PT-02白色防水防潮乳胶漆\n2.综合墙面、顶面","m2",120,"乳胶漆",{"v":0,"d":"0.00"},null,"PT-02白色防水防潮乳胶漆","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[115,"门铰链","1.平开门铰链安装","套",{"$f":"16*3","v":48},"五金",{"v":0,"d":"0.00"},null,"平开门铰链","套",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[116,"门执手锁","1.平开门执手锁安装","套",22,"五金",{"v":0,"d":"0.00"},null,"平开门执手锁","套",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[117,"门吸","1.平开门门吸安装","套",30,"五金",{"v":0,"d":"0.00"},null,"平开门门吸","套",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[118,"门插销","1.平开门插销安装","套",8,"五金",{"v":0,"d":"0.00"},null,"平开门插销","套",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[119,"轻钢龙骨双面石膏板隔墙","1.75型轻钢龙骨\n2.隔音棉\n3.双面单层纸面石膏板9.5mm","m2",120,"纸面石膏板",{"v":0,"d":"0.00"},null,"纸面石膏板9.5mm厚","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[120,"石膏板封堵洞口","1.木基层\n2.单层纸面石膏板9.5mm","m2",100,"纸面石膏板",{"v":0,"d":"0.00"},null,"单层纸面石膏板9.5mm","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[121,"砌体封堵洞口","1.水泥砖水泥砂浆封堵","m2",25,"水泥砖",{"v":0,"d":"0.00"},null,"水泥砖","m2",null,null,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[122,"石材地面抛光","1.石材面做缝、修补、抛光","m2",450,null,{"v":0,"d":"0.00"},null,"/",null,null,"/",{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
[123,"小计",{"$nulls":13},{"$f":"SUM(P3:P128)","v":{"v":54000,"d":"54000.00"}}]
[124,"计费明细","管理费","项",{"v":0.04,"d":"4%"},{"$nulls":10},{"$f":"P129*E130","v":{"v":2160,"d":"2160.00"}}]
[125,null,"利润","项",{"v":0.1,"d":"10%"},{"$nulls":10},{"$f":"P129*E131","v":{"v":5400,"d":"5400.00"}}]
[126,null,"税金","项",{"v":0.09,"d":"9%"},{"$nulls":10},{"$f":"(P131+P130+P129)*E132","v":{"v":5540.4,"d":"5540.40"}}]
[127,"工程总造价",{"$nulls":13},{"$f":"P132+P131+P130+P129","v":{"v":67100.4,"d":"67100.40"}}]
["1、综合单价为包含人工费（包括人员加班工资、差旅及窝工费）、材料费、机械费、风险的包工包料价格，包含深化设计、监理资料及竣工图绘制费用，包括水电、卸货、材料保管、二次搬运、上楼、各种保险、加班、临时设施、赶工措施、已完工项目成品保护措施、夜间照明、安全文明施工等费用，施工人员的食宿费、劳保费用、办公费、生活生产水电费、保险费也包含在报价里。其中：主材费单价包含主要材料费、运输费、运输损耗费、施工损耗费。施工单价包含人工费、机械费及除主要材料费以外辅材及其他所有费用。"]
["2、报价税率按9%考虑，提供9%税率的增值税专用发票。"]
["3、甲控乙供材料按提供的单价暂定，投标时价格不可调整，施工过程中投标人送样，招标人按质定价。"]
[null,"投标单位（公章）："]
[null,"授权委托人："]
[null,"日    期：     2020   年    月     日"]

{"sheet":"花园餐厅安装","index":5,"n_rows":97,"n_cols":17,"rows_kept":97,"merged":[[0,0,0,16],[1,0,1,16],[2,0,5,0],[2,1,5,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6],[2,7,2,14],[2,15,5,15],[2,16,5,16],[3,7,5,7],[3,8,3,13],[4,8,4,12],[4,14,5,14],[91,0,91,16],[92,0,92,17],[93,0,93,17]]}
["安装工程量报价清单"]
["工程名称：第四届中国绿博会花园餐厅装饰装修专业分包工程"]
["序号","分项工程名称","项目特征","单位","数量","主材名称","综合单价","其        中：",{"$nulls":7},"合价","备注"]
[{"$nulls":7},"人工费","材    料    费"]
[{"$nulls":8},"主材费",{"$nulls":5},"机械费"]
[{"$nulls":8},"名称及规格","单位","单位耗量","单价","单位主材费合价","辅材"]
[1,"电气工程"]
[2,"配电箱","1.名称：配电柜AP\n2.规格：详见图纸\n3.安装方式：落地安装","台",8,"配电箱",230,null,"配电箱","套",null,"/",0,null,null,{"v":1840,"d":"1840.00"},"配电箱甲供"]
[3,"配电箱","1.名称：应急照明箱ALE1\n2.规格：详见图纸\n3.安装方式：落地安装","台",4,"配电箱",230,null,"配电箱","套",null,"/",0,null,null,{"v":920,"d":"920.00"},"配电箱甲供"]
[4,"配电箱","1.名称：空调VRV1配电箱\n2.规格：详见图纸\n3.安装方式：落地安装","台",4,"配电箱",230,null,"配电箱","套",null,"/",0,null,null,{"v":920,"d":"920.00"},"配电箱甲供"]
[5,"配电箱","1.名称：消控中心电柜AT-XF\n2.规格：详见图纸\n3.安装方式：落地安装","台",1,"配电箱",230,null,"配电箱","套",null,"/",0,null,null,{"v":230,"d":"230.00"},"配电箱甲供"]
[6,"配电箱","1.名称：给水泵动力配电柜AT-SHSB\n2.规格：详见图纸\n3.安装方式：挂墙明装","台",1,"配电箱",230,null,"配电箱","套",null,"/",0,null,null,{"v":230,"d":"230.00"},"配电箱甲供"]
[7,"配电柜","1.名称：消防电源柜AT-XFBF\n2.规格：详见图纸\n3.安装方式：落地安装","组",1,"配电柜",1200,null,"配电柜","套",null,"/",0,null,null,{"v":1200,"d":"1200.00"},"配电柜甲供"]
[8,"凿（压)槽","1.名称:砖墙开槽\n2.填充(恢复)方式:水泥砂浆恢复","m",272.4,"/",{"$f":"H14+M14+N14+O14","v":0},null,"/","/",null,null,{"$f":"L14*K14","v":0},null,null,{"$f":"G14*E14","v":{"v":0,"d":"0.00"}}]
[9,"配管","1.名称:硬塑料管（PVC）\n2.规格:PC20\n3.配置形式:砖、混凝土结构暗配","m",250,"PVC电线管",0,null,"PVC电线管20","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[10,"配管","1.名称:硬塑料管（PVC）\n2.规格:PC20\n3.配置形式:砖、混凝土结构明配","m",450,"PVC电线管",0,null,"PVC电线管20","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[11,"配管","1.名称:硬塑料管（PVC）\n2.规格:PC25\n3.配置形式:砖、混凝土结构暗配","m",360,"PVC电线管",0,null,"PVC电线管25","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[12,"配管","1.名称:硬塑料管（PVC）\n2.规格:PC25\n3.配置形式:砖、混凝土结构明配","m",1650,"PVC电线管",0,null,"PVC电线管25","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[13,"配管","1.名称:硬塑料管（PVC）\n2.规格:PC32\n3.配置形式:砖、混凝土结构暗配","m",220,"PVC电线管",0,null,"PVC电线管32","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[14,"配管","1.名称:硬塑料管（PVC）\n2.规格:PC32\n3.配置形式:砖、混凝土结构明配","m",450,"PVC电线管",0,null,"PVC电线管32","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[15,"配管","1.名称:紧定式镀锌钢导管\n2.规格:JDG20\n3.配置形式:砖、混凝土结构暗配","m",85,"紧定式镀锌钢导管",0,null,"紧定式镀锌钢导管20","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[16,"配管","1.名称:紧定式镀锌钢导管\n2.规格:JDG20\n3.配置形式:砖、混凝土结构明配","m",75,"紧定式镀锌钢导管",0,null,"紧定式镀锌钢导管20","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[17,"配管","1.名称:紧定式镀锌钢导管\n2.规格:JDG40\n3.配置形式:砖、混凝土结构暗配","m",65,"紧定式镀锌钢导管",0,null,"紧定式镀锌钢导管40","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[18,"配管","1.名称:紧定式镀锌钢导管\n2.规格:JDG40\n3.配置形式:砖、混凝土结构明配","m",85,"紧定式镀锌钢导管",0,null,"紧定式镀锌钢导管40","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[19,"配管","1.名称:紧定式镀锌钢导管\n2.规格:JDG50\n3.配置形式:砖、混凝土结构暗配","m",95,"紧定式镀锌钢导管",0,null,"紧定式镀锌钢导管50","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[20,"配管","1.名称:紧定式镀锌钢导管\n2.规格:JDG50\n3.配置形式:砖、混凝土结构明配","m",65,"紧定式镀锌钢导管",0,null,"紧定式镀锌钢导管50","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[21,"桥架","1.名称:钢制桥架\n2.规格:300*150","m",96,"桥架",0,null,"成品镀锌钢桥架300*150","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[22,"桥架","1.名称:钢制桥架\n2.规格:200*100","m",45,"桥架",0,null,"成品镀锌钢桥架200*100","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[23,"电力电缆","1.名称:铜芯电缆\n2.型号:WDZ-YJV-4*35+1*16\n3.敷设方式、部位:穿管","m",65,"铜芯电缆",0,null,"DZ-YJV-4*35+1*16\n3.敷设方式、","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[24,"电力电缆","1.名称:铜芯电缆\n2.型号:WDZ-BYJ-4*25+1*16\n3.敷设方式、部位:穿管","m",78,"铜芯电缆",0,null,"WDZ-BYJ-4*25+1*16","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[25,"电力电缆","1.名称:铜芯电缆\n2.型号:WDZN-YJV-4*25\n3.敷设方式、部位:穿管","m",68,"铜芯电缆",0,null,"WDZN-YJV-4*25","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[26,"电力电缆","1.名称:铜芯电缆\n2.型号:WDZ-YJV-5*16\n3.敷设方式、部位:穿管","m",77,"铜芯电缆",0,null,"WDZ-YJV-5*16","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[27,"电力电缆","1.名称:铜芯电缆\n2.型号:WDZ-YJV-5*10\n3.敷设方式、部位:穿管","m",65,"铜芯电缆",0,null,"WDZ-YJV-5*10","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[28,"电力电缆","1.名称:铜芯电缆\n2.型号:NG-A-5*6\n3.敷设方式、部位:穿管","m",120,"铜芯电缆",0,null,"NG-A-5*6","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[29,"配线","1.名称:铜芯电线\n2.型号:WDZ-BYJ-10","m",150,"铜芯电线",0,null,"WDZ-BYJ-10","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[30,"配线","1.名称:铜芯电线\n2.型号:WDZ-BYJ-10","m",890,"铜芯电线",0,null,"WDZ-BYJ-10","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[31,"配线","1.名称:铜芯电线\n2.型号:WDZN-BYJ-6","m",650,"铜芯电线",0,null,"WDZN-BYJ-6","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[32,"配线","1.名称:铜芯电线\n2.型号:WDZN-BYJ-6","m",750,"铜芯电线",0,null,"WDZN-BYJ-6","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[33,"配线","1.名称:铜芯电线\n2.型号:WDZ-BYJ-4","m",3260,"铜芯电线",0,null,"WDZ-BYJ-4","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[34,"配线","1.名称:铜芯电线\n2.型号:WDZN-BYJ-4","m",460,"铜芯电线",0,null,"DZN-BYJ-4","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[35,"配线","1.名称:铜芯电线\n2.型号:WDZ-BYJ-2.5","m",1450,"铜芯电线",0,null,"WDZ-BYJ-2.5","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[36,"配线","1.名称:铜芯电线\n2.型号:WDZN-BYJ-2.5","m",1650,"铜芯电线",0,null,"WDZN-BYJ-2.5","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[37,"电力电缆头","1.名称:成套型电缆头\n2.规格:电缆截面35mm2以下","个",75,"电缆头",0,null,"电缆头截面35mm2以下","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[38,"接线盒","1.名称:接线盒\n2.材质:镀锌","个",320,"镀锌接线盒",0,null,"镀锌接线盒","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[39,"装饰灯具安装","1.名称:成品装饰吊灯\n2.类型:LED","套",36,"灯具",0,null,"成品装饰吊灯","套",null,450,0,null,null,{"v":0,"d":"0.00"},"成品装饰吊灯甲控乙供，主材价暂定，按质定价"]
[40,"装饰灯具安装","1.名称:成品装饰吸顶灯\n2.类型:LED","套",15,"灯具",0,null,"成品装饰吸顶灯","套",null,250,0,null,null,{"v":0,"d":"0.00"},"成品装饰吸顶灯甲控乙供，主材价暂定，按质定价"]
[41,"普通灯具","1.名称:双头斗胆灯\n2.类型:LED","套",464,"灯具",0,null,"双头斗胆灯","套",null,null,0,null,null,{"v":0,"d":"0.00"}]
[42,"普通灯具","1.名称:单头斗胆灯\n2.类型:LED","套",84,"灯具",0,null,"双头斗胆灯","套",null,null,0,null,null,{"v":0,"d":"0.00"}]
[43,"普通灯具","1.名称:嵌入式筒灯\n2.类型:LED","套",45,"灯具",0,null,"嵌入式筒灯","套",null,null,0,null,null,{"v":0,"d":"0.00"}]
[44,"普通灯具","1.名称:嵌入式防潮筒灯\n2.类型:LED","套",25,"灯具",0,null,"嵌入式防潮筒灯","套",null,null,0,null,null,{"v":0,"d":"0.00"}]
[45,"普通灯具","1.名称:600*600面板灯\n2.类型:LED","套",51,"灯具",0,null,"600*600面板灯","套",null,null,0,null,null,{"v":0,"d":"0.00"}]
[46,"普通灯具","1.名称:灯带\n2.类型:LED","m",360,"灯具",0,null,"LED灯带","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[47,"普通灯具","1.名称:应急照明筒灯\n2.类型:LED","套",38,"灯具",{"$f":"H53+M53+N53+O53","v":0},null,"应急照明筒灯","套",null,null,0,null,null,{"$f":"G53*E53","v":{"v":0,"d":"0.00"}}]
[48,"普通灯具","1.名称:应急照明格栅灯\n2.类型:LED","套",6,"灯具",0,null,"应急照明格栅灯","套",null,null,0,null,null,{"v":0,"d":"0.00"}]
[49,"普通灯具","1.名称:应急照明挂壁式\n2.类型:LED","套",45,"灯具",0,null,"应急照明挂壁式","套",null,null,0,null,null,{"v":0,"d":"0.00"}]
[50,"普通灯具","1.名称:应急出口指示灯\n2.类型:LED","套",88,"灯具",0,null,"应急出口指示灯","套",null,null,0,null,null,{"v":0,"d":"0.00"}]
[51,"小电器","1.名称:单联单控开关","个",45,"开关",0,null,"单联单控开关","个",null,null,{"$f":"H57*K57","v":0},null,null,{"v":0,"d":"0.00"}]
[52,"小电器","1.名称:双联单控开关","个",22,"开关",0,null,"双联单控开关","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[53,"小电器","1.名称:三联单控开关","个",32,"开关",0,null,"三联单控开关","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[54,"小电器","1.名称:单联双控开关","个",31,"开关",0,null,"单联双控开关","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[55,"小电器","1.名称:地面铜插座\n2.型号:15A","个",20,"插座",0,null,"地面铜插座","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[56,"小电器","1.名称:五孔普通插座\n2.型号:15A","个",56,"插座",0,null,"五孔普通插座","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[57,"小电器","1.名称:轴流排风扇","个",12,"轴流排风扇",0,null,"轴流排风扇","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[58,"网络、电视、电话",{"$nulls":4},0,{"$nulls":5},{"$f":"L64*K64","v":0},null,null,{"v":0,"d":"0.00"}]
[59,"光缆终端盒","1.弱电箱","个",3,"弱电箱",0,null,"弱电箱","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[60,"配线","1.名称:视频同轴电缆\n2.配线形式:穿管","m",425,"同轴电缆",0,null,"视频同轴电缆","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[61,"配线","1.名称:双绞线（6芯）\n2.配线形式:穿管","m",320,"双绞线",0,null,"双绞线（6芯）","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[62,"小电器","1.名称:有线电视插座\n2.安装方式:墙面安装","个",20,"插座",0,null,"有线电视插座","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[63,"小电器","1.名称:网络插座单口\n2.安装方式:墙面安装","个",12,"插座",0,null,"网络插座单口","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[64,"小电器","1.名称:网络插座单口\n2.安装方式:地面安装","个",12,"插座",0,null,"网络插座单口","个",null,null,0,null,null,{"v":0,"d":"0.00"}]
[65,"给排水、洁具安装工程",{"$nulls":10},0,null,null,{"v":0,"d":"0.00"}]
[66,"塑料管","1.材质、规格:PPR管DN20\n2.连接形式:热熔\n3.压力试验及吹、洗设计要求:符合规范及设计要求","m",120,"PPR管",{"$f":"H72+M72+N72+O72","v":0},null,"PPR管DN20","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[67,"塑料管","1.材质、规格:PPR管DN25\n2.连接形式:热熔\n3.压力试验及吹、洗设计要求:符合规范及设计要求","m",80,"PPR管",0,null,"PPR管DN25","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[68,"塑料管","1.材质、规格:PPR管DN32\n2.连接形式:热熔\n3.压力试验及吹、洗设计要求:符合规范及设计要求","m",60,"PPR管",0,null,"PPR管DN32","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[69,"塑料管","1.材质、规格:U-PVCP排水管Φ50\n2.连接形式:胶粘\n3.压力试验及吹、洗设计要求:符合规范及设计要求","m",110,"排水管",0,null,"U-PVCP排水管Φ50","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[70,"塑料管","1.材质、规格:U-PVCP排水管Φ75\n2.连接形式:胶粘\n3.压力试验及吹、洗设计要求:符合规范及设计要求","m",120,"排水管",0,null,"U-PVCP排水管Φ75","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[71,"塑料管","1.材质、规格:U-PVCP排水管Φ110\n2.连接形式:胶粘\n3.压力试验及吹、洗设计要求:符合规范及设计要求","m",220,"排水管",0,null,"U-PVCP排水管Φ110","m",null,null,0,null,null,{"v":0,"d":"0.00"}]
[72,"洗脸盆","1.材质:陶瓷\n2.规格、类型:嵌入式台上式洗脸盆\n3.附件名称、数量:含下水","组",22,"洗脸盆",{"$f":"H78+M78+N78+O78","v":0},null,"嵌入式台上式洗脸盆","组",null,550,0,null,null,{"v":0,"d":"0.00"},"嵌入式台上式洗脸盆甲控乙供，主材价暂定，按质定价"]
[73,"洗脸盆龙头","1.台上盆冷热水龙头","套",22,"台上盆冷热水龙头",0,null,"台上盆冷热水龙头","套",null,350,0,null,null,{"v":0,"d":"0.00"},"台上盆冷热水龙头甲控乙供，主材价暂定，按质定价"]
[74,"大便器","1.材质:陶瓷\n2.规格、类型:蹲便器","组",28,"蹲便器",0,null,"蹲便器","组",null,350,0,null,null,{"v":0,"d":"0.00"},"蹲便器甲控乙供，主材价暂定，按质定价"]
[75,"大便器脚踏阀","1.大便器脚踏阀","套",28,"大便器脚踏阀",0,null,"大便器脚踏阀","套",null,90,0,null,null,{"v":0,"d":"0.00"},"大便器脚踏阀甲控乙供，主材价暂定，按质定价"]
[76,"大便器","1.材质:陶瓷\n2.规格、类型:坐便器","组",4,"坐便器",0,null,"坐便器","组",null,2800,0,null,null,{"v":0,"d":"0.00"},"坐便器甲控乙供，主材价暂定，按质定价"]
[77,"小便器","1.材质:陶瓷\n2.规格、类型:成品小便斗","组",12,"成品小便斗",0,null,"感应阀","组",null,680,0,null,null,{"v":0,"d":"0.00"},"感应阀甲控乙供，主材价暂定，按质定价"]
[78,"小便器感应阀","1.小便器感应阀","组",12,"小便器感应阀",0,null,"小便器感应阀","组",null,320,0,null,null,{"v":0,"d":"0.00"},"小便器感应阀甲控乙供，主材价暂定，按质定价"]
[79,"烘手器","1.型号、规格:成品烘手器","个",6,"成品烘手器",0,null,"成品烘手器","个",null,220,0,null,null,{"v":0,"d":"0.00"},"成品烘手器甲控乙供，主材价暂定，按质定价"]
[80,"洗涤盆","1.材质:陶瓷\n2.规格、类型:拖把池","组",6,"拖把池",0,null,"拖把池","组",null,450,0,null,null,{"v":0,"d":"0.00"},"拖把池甲控乙供，主材价暂定，按质定价"]
[81,"小计",{"$nulls":13},{"$f":"SUM(P3:P86)","v":{"v":5340,"d":"5340.00"}}]
[82,"计费明细","管理费","项",{"v":0.04,"d":"4%"},{"$nulls":10},{"$f":"P87*E88","v":{"v":213.6,"d":"213.60"}}]
[83,null,"利润","项",{"v":0.1,"d":"10%"},{"$nulls":10},{"$f":"P87*E89","v":{"v":534,"d":"534.00"}}]
[84,null,"税金","项",{"v":0.09,"d":"9%"},{"$nulls":10},{"$f":"(P89+P88+P87)*E90","v":{"v":547.884,"d":"547.88"}}]
[85,"工程总造价",{"$nulls":13},{"$f":"P90+P89+P88+P87","v":{"v":6635.484,"d":"6635.48"}}]
["1、综合单价为包含人工费（包括人员加班工资、差旅及窝工费）、材料费、机械费、风险的包工包料价格，包含深化设计、监理资料及竣工图绘制费用，包括水电、卸货、材料保管、二次搬运、上楼、各种保险、加班、临时设施、赶工措施、已完工项目成品保护措施、夜间照明、安全文明施工等费用，施工人员的食宿费、劳保费用、办公费、生活生产水电费、保险费也包含在报价里。其中：主材费单价包含主要材料费、运输费、运输损耗费、施工损耗费。施工单价包含人工费、机械费及除主要材料费以外辅材及其他所有费用。"]
["2、报价税率按9%考虑，提供9%税率的增值税专用发票。"]
["3、甲控乙供材料按提供的单价暂定，投标时价格不可调整，施工过程中投标人送样，招标人按质定价。"]
[null,"投标单位（公章）："]
[null,"授权委托人："]
[null,"日    期：     2020   年    月     日"]

{"sheet":"花园餐厅措施费","index":6,"n_rows":20,"n_cols":6,"rows_kept":20,"merged":[[0,0,0,5],[1,0,1,5],[14,1,14,5]]}
["措施费项目计价表"]
["工程名称：第四届中国绿博会花园餐厅装饰装修专业分包工程"]
["序号","项目名称","单位","数量"," 金额（元）","备注"]
[1,"安全文明施工费","项",1,null,"专项包干费"]
[2,"成品保护费","项",1,null,"专项包干费"]
[3,"开荒清洁、垃圾清运费","项",1,null,"专项包干费"]
[4,"临时设施费","项",1,null,"专项包干费"]
[5,"专业交叉施工增加费","项",1,null,"专项包干费"]
[6,"脚手架","项",1,null,"专项包干费"]
[7,"运杂费（二次搬运费等）","项",1,null,"专项包干费"]
[8,"其它配合费","项",1,null,"专项包干费"]
[10,"工地开放日保洁","项",1,null,"专项包干费"]
[null,"合价",null,null,{"$f":"(SUM(E4:E12))*0.7","v":{"v":0,"d":"0.00"}}]
[]
["说明：","措施费用各项应为含税包干报价，不因任何情况调整，措施费按实际发生计取，不发生不计取。。"]
[]
[]
[null,"投标单位（公章）："]
[null,"授权委托人："]
[null,"日    期：     2020   年    月     日"]